(footprint "XIAO-nRF52840-Plus-SMD"(version 20241229) (generator "pcbnew") (generator_version "9.0")(layer "F.Cu" )(property "Reference" "REF**"(at 11.225 -0.075 270)(unlocked yes)(layer "F.SilkS" ))(property "Value" "XIAO-nRF52840-Plus-SMD"(at 0 0 0)(unlocked yes)(layer "F.Fab" ))(property "Datasheet" ""(at 0 0 0)(unlocked yes)(layer "F.Fab" )(hide yes))(property "Description" ""(at 0 0 0)(unlocked yes)(layer "F.Fab" )(hide yes))(attr smd)(pad "1" smd roundrect(at 7.62 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "2" smd roundrect(at 5.08 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "3" smd roundrect(at 2.54 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "4" smd roundrect(at 0 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "5" smd roundrect(at -2.54 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "6" smd roundrect(at -5.08 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "7" smd roundrect(at -7.62 -8.255 90)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "8" smd roundrect(at -7.62 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "9" smd roundrect(at -5.08 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "10" smd roundrect(at -2.54 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "11" smd roundrect(at 0 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "12" smd roundrect(at 2.54 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "13" smd roundrect(at 5.08 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "14" smd roundrect(at 7.62 8.255 270)(size 2.032 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "15" smd roundrect(at 6.35 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "16" smd roundrect(at 3.81 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "17" smd roundrect(at 1.27 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "18" smd roundrect(at -1.27 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "19" smd roundrect(at -3.81 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "20" smd roundrect(at -6.35 -8.655 90)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "21" smd roundrect(at -6.35 8.655 270)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "22" smd roundrect(at -3.81 8.655 270)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "23" smd roundrect(at -1.27 8.655 270)(size 1.232 0.95)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(chamfer_ratio 0.35)(chamfer top_left bottom_left)(thermal_bridge_angle 45))(pad "24" smd circle(at 8.5725 -1.27 270)(size 1.7 1.7)(layers  "F.Cu" "F.Mask" "F.Paste"))(pad "25" smd circle(at 8.5725 1.27 270)(size 1.7 1.7)(layers  "F.Cu" "F.Mask" "F.Paste"))(pad "26" smd circle(at 6.0325 -1.27 270)(size 1.7 1.7)(layers  "F.Cu" "F.Mask" "F.Paste"))(pad "27" smd circle(at 6.0325 1.27 270)(size 1.7 1.7)(layers  "F.Cu" "F.Mask" "F.Paste"))(pad "32" smd roundrect(at -5.517823 -0.993988 180)(size 2.5 1.1)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(pad "33" smd roundrect(at -5.517823 1.006012 180)(size 2.5 1.1)(layers  "F.Cu" "F.Mask" "F.Paste")(roundrect_rratio 0.1)(thermal_bridge_angle 45))(embedded_fonts no)(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-nRF52840 v15.step"(hide yes)(offset (xyz -1.778 -6.096 0.381))(scale (xyz 1 1 1))(rotate (xyz -90 0 0)))(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeeduino XIAO SAMD21 v4.step"(offset (xyz 0 0 0))(scale (xyz 1 1 1))(rotate (xyz 0 0 0)))(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO RP2040 v26.step"(hide yes)(offset (xyz 0 0 0))(scale (xyz 1 1 1))(rotate (xyz 0 0 90)))(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO-ESP32-C3.step"(hide yes)(offset (xyz -1.7018 -6.096 0))(scale (xyz 1 1 1))(rotate (xyz -90 0 0)))(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-ESP32S3 v2.step"(hide yes)(offset (xyz -1.778 -6.1722 0))(scale (xyz 1 1 1))(rotate (xyz -90 0 0))))