(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top")
		(1 "In1.Cu" signal "gnd")
		(2 "In2.Cu" signal "power")
		(31 "B.Cu" signal "Bottom")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Paste Mask Bottom")
		(35 "F.Paste" user "Paste Mask Top")
		(36 "B.SilkS" user "Silkscreen Bottom")
		(37 "F.SilkS" user "Silkscreen Top")
		(38 "B.Mask" user "Solder Mask Bottom")
		(39 "F.Mask" user "Solder Mask Top")
		(40 "Dwgs.User" user "Layer_12")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Layer_13")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Layer_15")
		(49 "F.Fab" user "Layer_14")
		(50 "User.1" user "Assembly Drawing Top")
		(51 "User.2" user "Assembly Drawing Bottom")
		(52 "User.3" user "Layer_5")
		(53 "User.4" user "Layer_6")
		(54 "User.5" user "Layer_7")
		(55 "User.6" user "Layer_8")
		(56 "User.7" user "Layer_9")
		(57 "User.8" user "Layer_10")
		(58 "User.9" user "Layer_11")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin -604.17195 766.479835)
		(grid_origin -604.17195 766.479835)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "VDD_5V")
	(net 2 "VBAT_1V5")
	(net 3 "VBAT-")
	(net 4 "VBAT")
	(net 5 "N34428841")
	(net 6 "N34424789")
	(net 7 "N34422366")
	(net 8 "N34422338")
	(net 9 "N34422069")
	(net 10 "N34422041")
	(net 11 "N34421831")
	(net 12 "N34420928")
	(net 13 "N34420537")
	(net 14 "N34420131")
	(net 15 "N34419863")
	(net 16 "N34418617")
	(net 17 "LED_YELLO")
	(net 18 "LED_RED")
	(net 19 "LED_GREEN")
	(net 20 "GND")
	(net 21 "CAP_SEN")
	(net 22 "A9_D9")
	(net 23 "A8_D8")
	(net 24 "A7_D7_RX")
	(net 25 "A6_D6_TX")
	(net 26 "A5_D5")
	(net 27 "A4_D4")
	(net 28 "A3_D3")
	(net 29 "A2_D2")
	(net 30 "A10_D10")
	(net 31 "A1_D1")
	(net 32 "A0_D0")
	(net 33 "3V3")
	(footprint "PL_SWPA4020"
		(layer "F.Cu")
		(at 82.45145 106.653635 180)
		(property "Reference" "L1"
			(at -2.8634 -0.496405 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PL_SWPA4020"
			(at -1.55 1.770575 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.55 0 270)
			(size 3.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "N34418617")
		)
		(pad "2" smd rect
			(at 1.55 0 270)
			(size 3.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 83.09145 108.653635) (xy 81.81145 108.653635) (xy 81.81145 104.673635) (xy 83.09145 104.673635)
				)
			)
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 84.17185 114.735035 -90)
		(property "Reference" "C3"
			(at 2.499608 0.4826 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 78.12665 100.511035 90)
		(property "Reference" "R1"
			(at -2.121694 -0.762 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "LED_RED")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "N34421831")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 79.19345 114.404835)
		(property "Reference" "R12"
			(at -0.7874 1.639094 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "N34424789")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 82.06365 103.228835)
		(property "Reference" "C2"
			(at 1.7018 0.493008 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "TPS61021_WSON8-EP"
		(layer "F.Cu")
		(at 82.36845 111.026635 90)
		(property "Reference" "U1"
			(at -1.359694 1.4732 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS61021_WSON8-EP"
			(at -1 1.725634 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -0.45 0.15)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.36) (xy 0.65 -0.36) (xy 0.65 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 0.09 -0.8)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.36) (xy 0.65 -0.36) (xy 0.65 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 0.09 0.15)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -0.36) (xy 0.65 -0.36) (xy 0.65 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd rect
			(at -1 -0.75 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "2" smd rect
			(at -1 -0.25 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "N34424789")
		)
		(pad "3" smd rect
			(at -1 0.25 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "4" smd rect
			(at -1 0.75 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "5" smd rect
			(at 1 0.75 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "N34419863")
		)
		(pad "6" smd rect
			(at 1 0.25 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "N34418617")
		)
		(pad "7" smd rect
			(at 1 -0.25 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "N34418617")
		)
		(pad "8" smd rect
			(at 1 -0.75 90)
			(size 0.6 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "9" smd rect
			(at -0.27 -0.475 180)
			(size 0.65 0.36)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 81.36845 112.026635) (xy 81.36845 110.026635) (xy 83.36845 110.026635) (xy 83.36845 112.026635)
				)
			)
		)
	)
	(footprint "HEADER_PIN_SIP7_2MM54"
		(layer "F.Cu")
		(at 118.18025 112.843635 180)
		(property "Reference" "CN2"
			(at 3.2236 -3.124094 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HEADER_PIN_SIP7_2MM54"
			(at 0.508 -2.070894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A7_D7_RX")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A8_D8")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A9_D9")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A10_D10")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "3V3")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24 180)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD_5V")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 79.21885 112.449035 180)
		(property "Reference" "R15"
			(at 0.7366 0.672306 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "N34424789")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 74.87545 100.155435 180)
		(property "Reference" "R5"
			(at 0.5334 -1.537494 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "A8_D8")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "N34422069")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 71.70045 99.164835 90)
		(property "Reference" "Q2"
			(at -0.419894 -3.3274 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.939824 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "N34422069")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414 180)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N34422041")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 75.23105 112.220435 90)
		(property "Reference" "Q3"
			(at -0.71392 2.717354 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.939824 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "N34422366")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414 180)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "N34422338")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 81.98745 100.130035)
		(property "Reference" "R16"
			(at 1.1684 0.470694 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "A0_D0")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 75.56125 109.223235 -90)
		(property "Reference" "R8"
			(at 0.54612 -1.578154 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "LED_YELLO")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "N34422338")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 79.21885 113.439635)
		(property "Reference" "C9"
			(at 1.60434 0.102354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "N34424789")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 86.05145 110.747235 90)
		(property "Reference" "Q4"
			(at 1.866106 -0.4572 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.939824 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "N34420131")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414 180)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "N34419863")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 79.34585 100.536435 90)
		(property "Reference" "R4"
			(at -2.070894 -0.2032 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "LED_GREEN")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N34422041")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 128.41865 109.020035 90)
		(property "Reference" "ED2"
			(at -3.0988 0.445294 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "CAP_SEN")
		)
	)
	(footprint "R0603"
		(layer "F.Cu")
		(at 125.77705 101.704835)
		(property "Reference" "R21"
			(at -0.67554 1.872525 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0603"
			(at -1.3 1.735005 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.8 0)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VBAT-")
		)
		(pad "2" smd rect
			(at 0.8 0)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 123.99905 97.158235 90)
		(property "Reference" "C7"
			(at 1.834672 -0.64154 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "A1_D1")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 85.67045 114.684235 -90)
		(property "Reference" "C5"
			(at 0.267454 -0.97448 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 122.22105 98.225035)
		(property "Reference" "R20"
			(at -1.09654 -0.760786 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VBAT_1V5")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "N34428841")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 122.90685 100.587235 180)
		(property "Reference" "Q5"
			(at 2.14934 -2.078014 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.100176 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 180)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "N34428841")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 180)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414 270)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VBAT-")
		)
	)
	(footprint "LED_SP1943_1615"
		(layer "F.Cu")
		(at 76.00145 105.003635 -90)
		(property "Reference" "D1"
			(at 0.575494 -1.6934 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED_SP1943_1615"
			(at -1.05 2.011106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.7 0.6 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 18 "LED_RED")
		)
		(pad "2" smd roundrect
			(at -0.7 -0.6 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 19 "LED_GREEN")
		)
		(pad "3" smd roundrect
			(at 0.7 -0.6 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 33 "3V3")
		)
		(pad "4" smd roundrect
			(at 0.7 0.6 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 17 "LED_YELLO")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 89.78525 104.778235 -90)
		(property "Reference" "R6"
			(at -1.27 -0.521494 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "A2_D2")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 88.56605 110.163035 90)
		(property "Reference" "R14"
			(at -0.521494 0.7366 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "N34420131")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 74.90085 96.523235 180)
		(property "Reference" "R2"
			(at 0.508 -1.410494 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "A9_D9")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "N34420537")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 85.87365 100.130035)
		(property "Reference" "C6"
			(at 1.57894 0.127754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 32 "A0_D0")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 71.67505 95.481835 90)
		(property "Reference" "Q1"
			(at -0.470694 -3.1496 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.939824 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "N34420537")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 90)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414 180)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "N34421831")
		)
	)
	(footprint "CN_ESP32C6_XIAO_DIP14"
		(layer "F.Cu")
		(at 106.00145 97.603635)
		(property "Reference" "CN3"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CN_ESP32C6_XIAO_DIP14"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -7.61887 -0.75)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 1.79)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 4.33)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 6.87)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 9.41)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 11.95)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61887 14.49)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -1.88113 0) (xy -1.88113 1.5) (xy 0 1.50647) (xy 0.19579 1.4807) (xy 0.37823 1.40512)
						(xy 0.5349 1.2849) (xy 0.65512 1.12823) (xy 0.73069 0.94579) (xy 0.75647 0.75) (xy 0.73069 0.55421)
						(xy 0.65512 0.37176) (xy 0.5349 0.21509) (xy 0.37823 0.09487) (xy 0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 -0.75)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 1.79)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 4.33)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 6.87)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 9.41)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 11.95)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61888 14.49)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 1.88112 0) (xy 1.88112 1.5) (xy 0 1.50647) (xy -0.19579 1.4807) (xy -0.37824 1.40512)
						(xy -0.53491 1.2849) (xy -0.65513 1.12823) (xy -0.7307 0.94579) (xy -0.75648 0.75) (xy -0.7307 0.55421)
						(xy -0.65513 0.37176) (xy -0.53491 0.21509) (xy -0.37824 0.09487) (xy -0.19579 0.0193) (xy 0 -0.00647)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" thru_hole oval
			(at -7.874 0)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A0_D0")
		)
		(pad "2" thru_hole oval
			(at -7.874 2.54)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A1_D1")
		)
		(pad "3" thru_hole oval
			(at -7.874 5.08)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A2_D2")
		)
		(pad "4" thru_hole oval
			(at -7.874 7.62)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A3_D3")
		)
		(pad "5" thru_hole oval
			(at -7.874 10.16)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A4_D4")
		)
		(pad "6" thru_hole oval
			(at -7.874 12.7)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A5_D5")
		)
		(pad "7" thru_hole oval
			(at -7.874 15.24)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A6_D6_TX")
		)
		(pad "8" thru_hole oval
			(at 7.874 15.24)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A7_D7_RX")
		)
		(pad "9" thru_hole oval
			(at 7.874 12.7)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A8_D8")
		)
		(pad "10" thru_hole oval
			(at 7.874 10.16)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A9_D9")
		)
		(pad "11" thru_hole oval
			(at 7.874 7.62)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A10_D10")
		)
		(pad "12" thru_hole oval
			(at 7.874 5.08)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "3V3")
		)
		(pad "13" thru_hole oval
			(at 7.874 2.54)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "GND")
		)
		(pad "14" thru_hole oval
			(at 7.874 0)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "VDD_5V")
		)
	)
	(footprint "SWITCH_TS24CA"
		(layer "F.Cu")
		(at 67.60145 105.003635 90)
		(property "Reference" "CN4"
			(at -4.304504 -0.12194 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_TS24CA"
			(at -1.98 4.052784 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -1.85 0.4)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1) (xy 0.6 1) (xy 0.6 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -0.85 0.9 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 0.85 0.9 90)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" smd custom
			(at 1.85 0.4)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1) (xy 0.6 -1) (xy 0.6 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd rect
			(at 1.7 2.2 180)
			(size 1.25 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "A2_D2")
		)
		(pad "2" smd rect
			(at -1.7 2.2 180)
			(size 1.25 0.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "3" smd rect
			(at -2.2 0 90)
			(size 1.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "4" smd rect
			(at 2.2 0 90)
			(size 1.3 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 75.05325 114.836635 180)
		(property "Reference" "R11"
			(at 2.5908 -0.445294 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "N34422366")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 71.62425 108.715235)
		(property "Reference" "Q6"
			(at -2.86774 2.567014 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23"
			(at -1.39 1.939824 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.9525 0.9906)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "3" smd rect
			(at 0 -1.0414 90)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VBAT_1V5")
		)
	)
	(footprint "HEADER_PIN_SIP7_2MM54"
		(layer "F.Cu")
		(at 93.83145 97.603635)
		(property "Reference" "CN1"
			(at 1.4402 18.287894 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HEADER_PIN_SIP7_2MM54"
			(at 0.508 -1.993106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A0_D0")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A1_D1")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A2_D2")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A3_D3")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A4_D4")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A5_D5")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.8 1.8)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A6_D6_TX")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 126.05645 99.241035 180)
		(property "Reference" "R18"
			(at -1.25406 -0.316214 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "N34420928")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "A1_D1")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 127.09785 109.020035 90)
		(property "Reference" "R17"
			(at -2.8956 0.521494 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "A3_D3")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "CAP_SEN")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 78.80145 109.353635 -90)
		(property "Reference" "R10"
			(at -1.18428 -0.333954 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "N34419863")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 74.90085 95.151635)
		(property "Reference" "R3"
			(at -0.5588 -0.570706 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "N34420537")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "SOD123"
		(layer "F.Cu")
		(at 128.44405 103.178035 90)
		(property "Reference" "D2"
			(at -3.729673 -0.6096 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOD123"
			(at -1.397 2.020094 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "CAP_SEN")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "N34420928")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 74.87545 98.377435)
		(property "Reference" "R7"
			(at -0.4826 1.435894 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "N34422069")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 88.61685 104.778235 -90)
		(property "Reference" "ED1"
			(at -1.27 -0.369094 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "A2_D2")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 126.08185 98.098035)
		(property "Reference" "C8"
			(at -0.35902 -1.015246 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 31 "A1_D1")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 126.05645 100.384035 180)
		(property "Reference" "R19"
			(at -1.25406 -0.289214 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "N34420928")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 82.06365 101.527035)
		(property "Reference" "C1"
			(at 1.7272 0.391408 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 82.57165 114.709635 -90)
		(property "Reference" "C4"
			(at 2.499608 1.4986 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "3V3")
		)
		(pad "2" smd rect
			(at 0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 88.99785 111.763235 180)
		(property "Reference" "R13"
			(at 0.635 -1.537494 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "VDD_5V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "N34420131")
		)
	)
	(footprint "R0603"
		(layer "F.Cu")
		(at 74.13885 107.953235 -90)
		(property "Reference" "R22"
			(at -0.054875 -1.05566 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0603"
			(at -1.3 1.664995 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.8 0 270)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VBAT_1V5")
		)
		(pad "2" smd rect
			(at 0.8 0 270)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VBAT")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 75.05325 116.030435 180)
		(property "Reference" "R9"
			(at 2.4892 -0.470694 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "A10_D10")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "N34422366")
		)
	)
	(footprint "CON_BAT5_2_14500"
		(layer "B.Cu")
		(at 98.60145 105.003635)
		(property "Reference" "CN5"
			(at -12.4484 -8.873306 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CON_BAT5_2_14500"
			(at -0.75 -0.524366 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at -27.2 7.1)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "1" thru_hole circle
			(at -27.2 0)
			(size 2.3 2.3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VBAT_1V5")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 27.2 0)
			(size 2.3 2.3)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VBAT-")
			(thermal_bridge_angle 90)
		)
	)
)
