(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(title_block
		(title "Seeed Studio XIAO-RS485-Expansion-Board")
		(date "2024-09-27")
		(rev "V1.1")
	)
	(lib_symbols
		(symbol "Power:+12V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+12V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+12V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+12V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+12V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "Power:+3.3V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+3.3V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3.3V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+3.3V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+3.3V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "Power_Gnd:+12V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+12V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+12V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+12V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+12V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "Power_Gnd:+5V"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "Power_Gnd:GND"
			(power)
			(pin_numbers hide)
			(pin_names
				(offset 0) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
		)
		(symbol "Seeed_libdb:Capacitors/302010006"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.175 0 0)
			)
			(property "Value" "10nF"
				(at 5.715 -1.905 0)
			)
			(property "Footprint" "Capacitor:C0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD CAP Ceramic 10nF-50V-10%-X7R;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "CC0402KRX7R9BB103"
				(at 0 0 0)
			)
			(property "SKU" "302010006"
				(at 0 0 0)
			)
			(property "Dielectric" ""
				(at 0 0 0)
			)
			(property "Part Type" "Ceramic"
				(at 0 0 0)
			)
			(property "Voltage Rating" "50V,X7R"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Capacitor:C0402"
				(at 0 0 0)
			)
			(symbol "Capacitors/302010006_0_1"
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Capacitors/302010006_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Capacitors/302010043"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.175 0 0)
			)
			(property "Value" "100nF"
				(at 5.715 -1.905 0)
			)
			(property "Footprint" "Capacitor:C0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "TDK"
				(at 0 0 0)
			)
			(property "MPN" "C1005X7R1H104K"
				(at 0 0 0)
			)
			(property "SKU" "302010043"
				(at 0 0 0)
			)
			(property "Dielectric" ""
				(at 0 0 0)
			)
			(property "Part Type" "Ceramic"
				(at 0 0 0)
			)
			(property "Voltage Rating" "50V,X7R"
				(at 0 0 0)
			)
			(property "Status" "Testo PoE"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Capacitor:C0402"
				(at 0 0 0)
			)
			(symbol "Capacitors/302010043_0_1"
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Capacitors/302010043_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Capacitors/302010519"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.175 0 0)
			)
			(property "Value" "10uF"
				(at 5.715 -1.905 0)
			)
			(property "Footprint" "Capacitor:C0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD CAP Ceramic 10uF-10V-20%-X5R;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "CC0402MRX5R6BB106"
				(at 0 0 0)
			)
			(property "SKU" "302010519"
				(at 0 0 0)
			)
			(property "Dielectric" ""
				(at 0 0 0)
			)
			(property "Part Type" "10uF"
				(at 0 0 0)
			)
			(property "Voltage Rating" "10V,X5R"
				(at 0 0 0)
			)
			(property "Status" "XIAO"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 85°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Capacitor:C0402"
				(at 0 0 0)
			)
			(symbol "Capacitors/302010519_0_1"
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Capacitors/302010519_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Capacitors/302011019"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.175 0 0)
			)
			(property "Value" "75pF"
				(at 5.715 -1.905 0)
			)
			(property "Footprint" "Capacitor:C0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD CAP Ceramic 75pF-50V-5%-NPO;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "CC0402JRNPO9BN750"
				(at 0 0 0)
			)
			(property "SKU" "302011019"
				(at 0 0 0)
			)
			(property "Dielectric" ""
				(at 0 0 0)
			)
			(property "Part Type" "Ceramic"
				(at 0 0 0)
			)
			(property "Voltage Rating" "50V,NP0"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Capacitor:C0402"
				(at 0 0 0)
			)
			(symbol "Capacitors/302011019_0_1"
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Capacitors/302011019_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Capacitors/302013260"
			(pin_numbers hide)
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "C"
				(at 3.175 0 0)
			)
			(property "Value" "22uF"
				(at 5.715 -1.905 0)
			)
			(property "Footprint" "Capacitor:C0805"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD CAP Ceramic 22uF-25V-20%-X5R;0805"
				(at 0 0 0)
			)
			(property "Manufacturer" "Samsung"
				(at 0 0 0)
			)
			(property "MPN" "CL21A226MAYNNNE"
				(at 0 0 0)
			)
			(property "SKU" "302013260"
				(at 0 0 0)
			)
			(property "Dielectric" ""
				(at 0 0 0)
			)
			(property "Part Type" "Ceramic"
				(at 0 0 0)
			)
			(property "Voltage Rating" "25V,X5R"
				(at 0 0 0)
			)
			(property "Status" ""
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 85°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Capacitor:C0805"
				(at 0 0 0)
			)
			(symbol "Capacitors/302013260_0_1"
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0.635)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Capacitors/302013260_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Connector/320020216"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -2.54 10.16 0)
			)
			(property "Value" "Header 1x7 2.54mm"
				(at -2.54 8.89 0)
			)
			(property "Footprint" "Connector:H7-2.54"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "DIP Black Male Header VERT;1*7P-2.54-2.54-11.6/3.0mm"
				(at 0 0 0)
			)
			(property "Manufacturer" ""
				(at 0 0 0)
			)
			(property "MPN" ""
				(at 0 0 0)
			)
			(property "SKU" "320020216"
				(at 0 0 0)
			)
			(property "Part Type" "Header"
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" "Grove AI HAT for Edge Computing"
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector:H7-2.54"
				(at 0 0 0)
			)
			(symbol "Connector/320020216_1_0"
				(polyline
					(pts
						(xy -2.54 -8.89) (xy -2.54 8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 8.89) (xy 2.54 8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -8.89) (xy -2.54 -8.89)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 8.89) (xy 2.54 -8.89)
					)
					(fill
						(type none)
					)
				)
				(pin passive inverted_clock
					(at -7.62 7.62 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -7.62 5.08 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at -7.62 2.54 0)
					(length 5.08)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 5.08)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 5.08)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at -7.62 -5.08 0)
					(length 5.08)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at -7.62 -7.62 0)
					(length 5.08)
					(name "7")
					(number "7")
				)
			)
		)
		(symbol "Seeed_libdb:Connector/320110007"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -2.54 6.35 0)
			)
			(property "Value" "3P-3.5"
				(at -2.54 5.08 0)
			)
			(property "Footprint" "Connector:H3_3d5_11_5x7mm"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "DIP Female Screw Terminal-Green;3P-3.5"
				(at 0 0 0)
			)
			(property "Manufacturer" "SENGER"
				(at 0 0 0)
			)
			(property "MPN" "GS012S-3.5mm-3P"
				(at 0 0 0)
			)
			(property "SKU" "320110007"
				(at 0 0 0)
			)
			(property "Part Type" "Connector"
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" "-40°C to 105°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector:H3_3d5_11_5x7mm"
				(at 0 0 0)
			)
			(symbol "Connector/320110007_1_0"
				(polyline
					(pts
						(xy -2.54 -5.08) (xy -2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 5.08) (xy 2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -5.08) (xy -2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 5.08) (xy 2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(pin passive inverted_clock
					(at -7.62 3.81 0)
					(length 5.08)
					(name "P$1")
					(number "1")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 5.08)
					(name "P$2")
					(number "2")
				)
				(pin passive line
					(at -7.62 -3.81 0)
					(length 5.08)
					(name "P$3")
					(number "3")
				)
			)
		)
		(symbol "Seeed_libdb:Diode/304011053"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at -2.54 1.27 0)
			)
			(property "Value" "B5819WS SL"
				(at 0 1.27 0)
			)
			(property "Footprint" "Diode:SOD-323"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD Diode Schottky 40V-1A;SOD-323"
				(at 0 0 0)
			)
			(property "Manufacturer" "CJ"
				(at 0 0 0)
			)
			(property "MPN" "B5819WS SL"
				(at 0 0 0)
			)
			(property "SKU" "304011053"
				(at 0 0 0)
			)
			(property "Part Type" "Schottky Diode"
				(at 0 0 0)
			)
			(property "Rating" "40V"
				(at 0 0 0)
			)
			(property "Status" "reTerminal DM"
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Diode:SOD-323"
				(at 0 0 0)
			)
			(symbol "Diode/304011053_0_0"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Diode/304011053_1_0"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 2.54 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Diode/304040144"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at -3.175 0.635 0)
			)
			(property "Value" "SMBJ15CATR7"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Diode:DO-214AA_SMB"
				(at -0.635 -3.81 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD Diode TVS 15V-600W"
				(at 0 0 0)
			)
			(property "Manufacturer" "Brightking"
				(at 0 0 0)
			)
			(property "MPN" "SMBJ15CATR7"
				(at 0 0 0)
			)
			(property "SKU" "304040144"
				(at 0 0 0)
			)
			(property "Part Type" "Diode"
				(at 0 0 0)
			)
			(property "Rating" "15V-600W"
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" "-55℃ to 150℃"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Diode:DO-214AA_SMB"
				(at 0 0 0)
			)
			(symbol "Diode/304040144_1_0"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy -0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0.635 1.905)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "+")
					(number "1")
				)
				(pin passive line
					(at 2.54 0 180)
					(length 2.54)
					(name "-")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Diode/304050312"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at -1.905 1.27 0)
			)
			(property "Value" "TPD1E10B06DPYR"
				(at 1.27 1.27 0)
			)
			(property "Footprint" "Diode:ESD-0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD Diode ESD 5.5V-6V-12pF-30KV-30KV;X1SON(2)"
				(at 0 0 0)
			)
			(property "Manufacturer" "TI"
				(at 0 0 0)
			)
			(property "MPN" "TPD1E10B06DPYR"
				(at 0 0 0)
			)
			(property "SKU" "304050312"
				(at 0 0 0)
			)
			(property "Part Type" "ESD"
				(at 0 0 0)
			)
			(property "Rating" "5.5V"
				(at 0 0 0)
			)
			(property "Status" ""
				(at 0 0 0)
			)
			(property "Temperature" "-40°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Diode:ESD-0402"
				(at 0 0 0)
			)
			(symbol "Diode/304050312_1_0"
				(polyline
					(pts
						(xy -1.27 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy -0.635 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0.635 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy 0 0) (xy -1.27 -1.27)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 0 0) (xy 1.27 1.27)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Diode/304050558"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at -3.81 5.08 0)
			)
			(property "Value" "SM712-02HTG"
				(at -1.905 5.08 0)
			)
			(property "Footprint" "Diode:SOT-23"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD Diode TVS 12VWM 31VC"
				(at 0 0 0)
			)
			(property "Manufacturer" "Littelfuse"
				(at 0 0 0)
			)
			(property "MPN" "SM712-02HTG"
				(at 0 0 0)
			)
			(property "SKU" "304050558"
				(at 0 0 0)
			)
			(property "Part Type" "Diode"
				(at 0 0 0)
			)
			(property "Rating" "12V"
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" "-40°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Diode:SOT-23"
				(at 0 0 0)
			)
			(symbol "Diode/304050558_1_0"
				(polyline
					(pts
						(xy -3.81 -5.08) (xy -3.81 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -2.54) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 2.54) (xy -2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 5.08) (xy 3.81 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.667 -3.937) (xy -2.286 -3.937)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.667 -1.27) (xy -2.667 -3.937)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.667 1.143) (xy -2.286 1.143)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.667 3.81) (xy -2.667 1.143)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -3.81) (xy -2.286 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -2.54) (xy -2.54 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -2.54) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -1.27) (xy -2.667 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -1.27) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 1.27) (xy -2.286 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 3.81) (xy -2.667 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 3.81) (xy -2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.286 -3.937) (xy -2.286 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.286 1.143) (xy -2.286 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -3.81) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -2.54) (xy -1.27 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -2.54 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.54) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.54) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 3.81) (xy -1.27 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 3.81) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 -1.143) (xy 1.016 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.016 3.937) (xy 1.016 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.81) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.81) (xy 1.397 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.016 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.397 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 3.81) (xy 1.016 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.397 -3.81) (xy 1.397 -1.143)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.397 -1.143) (xy 1.016 -1.143)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.397 1.27) (xy 1.397 3.937)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.397 3.937) (xy 1.016 3.937)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 3.81 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 -5.08) (xy -3.81 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 0) (xy 3.81 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 5.08) (xy 3.81 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -6.35 2.54 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -6.35 -2.54 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 6.35 0 180)
					(length 2.54)
					(name "3")
					(number "3")
				)
			)
		)
		(symbol "Seeed_libdb:Ic/310031254"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 8.89 0)
			)
			(property "Value" "TPS54302"
				(at 2.54 8.89 0)
			)
			(property "Footprint" "Ic:SOT23-6"
				(at 5.08 5.08 0)
			)
			(property "Datasheet" ""
				(at 5.08 5.08 0)
			)
			(property "Description" "SMD IC PMIC;SOT23-6"
				(at 0 0 0)
			)
			(property "Manufacturer" "TI"
				(at 0 0 0)
			)
			(property "MPN" "TPS54302"
				(at 0 0 0)
			)
			(property "SKU" "310031254"
				(at 0 0 0)
			)
			(property "Part Type" ""
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" ""
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Ic:SOT23-6"
				(at 0 0 0)
			)
			(symbol "Ic/310031254_0_1"
				(rectangle
					(start -5.08 7.62)
					(end 5.08 -7.62)
					(fill
						(type none)
					)
				)
			)
			(symbol "Ic/310031254_1_1"
				(pin passive line
					(at -7.62 0 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "SW")
					(number "2")
				)
				(pin passive line
					(at -7.62 5.08 0)
					(length 2.54)
					(name "VIN")
					(number "3")
				)
				(pin passive line
					(at 7.62 -5.08 180)
					(length 2.54)
					(name "FB")
					(number "4")
				)
				(pin passive line
					(at -7.62 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "5")
				)
				(pin passive line
					(at 7.62 5.08 180)
					(length 2.54)
					(name "BOOT")
					(number "6")
				)
			)
		)
		(symbol "Seeed_libdb:Ic/310071191"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.842 7.874 0)
			)
			(property "Value" "TP8485E-SR"
				(at -3.81 6.096 0)
			)
			(property "Footprint" "Ic:SOIC8-1.27-5X4MM"
				(at -6.35 -5.08 0)
			)
			(property "Datasheet" ""
				(at -6.35 -5.08 0)
			)
			(property "Description" "SMD IC Interface RS485/422"
				(at -6.35 -5.08 0)
			)
			(property "Manufacturer" "3PEAK"
				(at 0 0 0)
			)
			(property "MPN" "TP8485E-SR"
				(at 0 0 0)
			)
			(property "SKU" "310071191"
				(at 0 0 0)
			)
			(property "Part Type" "IC"
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" "-40°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Ic:SOIC8-1.27-5X4MM"
				(at 0 0 0)
			)
			(symbol "Ic/310071191_0_1"
				(rectangle
					(start -6.35 5.08)
					(end 6.35 -7.62)
					(fill
						(type none)
					)
				)
			)
			(symbol "Ic/310071191_1_1"
				(pin passive line
					(at -8.89 2.54 0)
					(length 2.54)
					(name "R")
					(number "1")
				)
				(pin passive line
					(at -8.89 0 0)
					(length 2.54)
					(name "/RE")
					(number "2")
				)
				(pin passive line
					(at -8.89 -2.54 0)
					(length 2.54)
					(name "DE")
					(number "3")
				)
				(pin passive line
					(at -8.89 -5.08 0)
					(length 2.54)
					(name "D")
					(number "4")
				)
				(pin passive line
					(at 8.89 -5.08 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 8.89 -2.54 180)
					(length 2.54)
					(name "A/Y")
					(number "6")
				)
				(pin passive line
					(at 8.89 0 180)
					(length 2.54)
					(name "B/Z")
					(number "7")
				)
				(pin passive line
					(at 8.89 2.54 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
		)
		(symbol "Seeed_libdb:Inductor/303010147"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "L"
				(at -3.175 1.27 0)
			)
			(property "Value" "10uH"
				(at 0 1.27 0)
			)
			(property "Footprint" "Inductor:L5040S"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD Inductor 10uH-20％-2.35A;5*5*4mm"
				(at 0 0 0)
			)
			(property "Manufacturer" "Sunlord"
				(at 0 0 0)
			)
			(property "MPN" "SWPA5040S100MT"
				(at 0 0 0)
			)
			(property "SKU" "303010147"
				(at 0 0 0)
			)
			(property "Part Type" "Inductor"
				(at 0 0 0)
			)
			(property "Rating" "2.35A"
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" "-40℃~+125℃"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Inductor:L5040S"
				(at 0 0 0)
			)
			(symbol "Inductor/303010147_0_0"
				(arc
					(start -1.27 0)
					(mid -1.905 0.6323)
					(end -2.54 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 0 0)
					(mid -0.635 0.6323)
					(end -1.27 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 1.27 0)
					(mid 0.635 0.6323)
					(end 0 0)
					(fill
						(type none)
					)
				)
				(arc
					(start 2.54 0)
					(mid 1.905 0.6323)
					(end 1.27 0)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Misc/TP35C_SMD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TP"
				(at -2.54 0 0)
			)
			(property "Value" "Test Point"
				(at 5.08 0 0)
			)
			(property "Footprint" "Misc:TP-D35MIL"
				(at -2.54 -5.08 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Test Point;TP35C_SMD"
				(at 0 0 0)
			)
			(property "Manufacturer" ""
				(at 0 0 0)
			)
			(property "MPN" ""
				(at 0 0 0)
			)
			(property "SKU" "TP35C_SMD"
				(at 0 0 0)
			)
			(property "Part Type" "Test Point"
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" ""
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Misc:TP-D35MIL"
				(at 0 0 0)
			)
			(symbol "Misc/TP35C_SMD_1_0"
				(polyline
					(pts
						(xy -2.54 0) (xy -1.27 0)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 0)
					(radius 1.27)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -2.54 0 0)
					(length 0)
					(name "T")
					(number "1")
				)
			)
		)
		(symbol "Seeed_libdb:Module/XIAO-DIP-SMD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -21.59 13.97 0)
			)
			(property "Value" ""
				(at -1.27 13.97 0)
			)
			(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "Manufacturer" ""
				(at 0 0 0)
			)
			(property "MPN" ""
				(at 0 0 0)
			)
			(property "SKU" "XIAO-DIP-SMD"
				(at 0 0 0)
			)
			(property "Part Type" ""
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" ""
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Module:MOUDLE14P-XIAO-DIP-SMD"
				(at 0 0 0)
			)
			(symbol "Module/XIAO-DIP-SMD_1_0"
				(polyline
					(pts
						(xy -21.59 -13.97) (xy -21.59 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -11.43) (xy -22.86 -11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -7.62) (xy -22.86 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 -3.81) (xy -22.86 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 0) (xy -22.86 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 0) (xy -21.59 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 3.81) (xy -22.86 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 3.81) (xy -21.59 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 7.62) (xy -22.86 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 7.62) (xy -21.59 11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 11.43) (xy -22.86 11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 11.43) (xy -21.59 13.97)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -21.59 13.97) (xy 20.32 13.97)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 20.32 -13.97) (xy -21.59 -13.97)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 20.32 3.81) (xy 20.32 -13.97)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 20.32 7.62) (xy 20.32 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 20.32 11.43) (xy 20.32 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 20.32 13.97) (xy 20.32 11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 -11.43) (xy 20.32 -11.43)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 -7.62) (xy 20.32 -7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 -3.81) (xy 20.32 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 0) (xy 20.32 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 3.81) (xy 20.32 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 7.62) (xy 20.32 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 21.59 11.43) (xy 20.32 11.43)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -24.13 11.43 0)
					(length 2.54)
					(name "PA02_A0_D0")
					(number "1")
				)
				(pin passive line
					(at 22.86 -3.81 180)
					(length 2.54)
					(name "PA5_A9_D9_MISO")
					(number "10")
				)
				(pin passive line
					(at 22.86 0 180)
					(length 2.54)
					(name "PA6_A10_D10_MOSI")
					(number "11")
				)
				(pin passive line
					(at 22.86 3.81 180)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin passive line
					(at 22.86 7.62 180)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin passive line
					(at 22.86 11.43 180)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin passive line
					(at -24.13 7.62 0)
					(length 2.54)
					(name "PA4_A1_D1")
					(number "2")
				)
				(pin passive line
					(at -24.13 3.81 0)
					(length 2.54)
					(name "PA10_A2_D2")
					(number "3")
				)
				(pin passive line
					(at -24.13 0 0)
					(length 2.54)
					(name "PA11_A3_D3")
					(number "4")
				)
				(pin passive line
					(at -24.13 -3.81 0)
					(length 2.54)
					(name "PA8_A4_D4_SDA")
					(number "5")
				)
				(pin passive line
					(at -24.13 -7.62 0)
					(length 2.54)
					(name "PA9_A5_D5_SCL")
					(number "6")
				)
				(pin passive line
					(at -24.13 -11.43 0)
					(length 2.54)
					(name "PB08_A6_D6_TX")
					(number "7")
				)
				(pin passive line
					(at 22.86 -11.43 180)
					(length 2.54)
					(name "PB09_A7_D7_RX")
					(number "8")
				)
				(pin passive line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "PA7_A8_D8_SCK")
					(number "9")
				)
			)
		)
		(symbol "Seeed_libdb:Mosfet/305030010"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at -2.54 2.54 0)
			)
			(property "Value" "CJ3407"
				(at 0 2.54 0)
			)
			(property "Footprint" "Mosfet:SOT23"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD MOSFET P-CH 30V-4.3A;SOT-23"
				(at 0 0 0)
			)
			(property "Manufacturer" "长电"
				(at 0 0 0)
			)
			(property "MPN" "CJ3407"
				(at 0 0 0)
			)
			(property "SKU" "305030010"
				(at 0 0 0)
			)
			(property "Part Type" "PMOS"
				(at 0 0 0)
			)
			(property "Rating" "30V;4.3A"
				(at 0 0 0)
			)
			(property "Status" "Sensor Hub"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 150°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Mosfet:SOT23"
				(at 0 0 0)
			)
			(symbol "Mosfet/305030010_1_0"
				(circle
					(center 0 -1.905)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.54) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 -2.54) (xy -1.905 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 -1.905) (xy -1.905 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 -1.905) (xy 0 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0) (xy -1.905 -0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0) (xy -0.3175 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0.635) (xy -1.905 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 1.905) (xy -1.905 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 1.905) (xy 0 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 2.54) (xy -1.905 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.9525 -0.3175) (xy -0.3175 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.9525 0.3175) (xy -0.9525 -0.3175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.9525 0.3175) (xy -0.508 -0.127)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.3175 0) (xy -0.9525 0.3175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.3175 0) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.905) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -0.9525 -0.3175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -0.9525 0.3175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.905) (xy 1.5875 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0 1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.9525 -0.4445) (xy 1.5875 -0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.9525 0.4445) (xy 1.27 0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0.3175) (xy 1.5875 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0.4445) (xy 1.5875 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0.4445) (xy 1.905 0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 -1.905) (xy 0 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 -0.4445) (xy 0.9525 0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 -0.4445) (xy 1.5875 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 -0.4445) (xy 2.2225 -0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 0) (xy 1.5875 -0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 0) (xy 1.905 0.3175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 0) (xy 1.905 0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.5875 1.905) (xy 1.5875 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.905 0.4445) (xy 2.2225 0.4445)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.2225 0.4445) (xy 1.5875 -0.4445)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 0 1.905)
					(radius 0.254)
					(fill
						(type none)
					)
				)
				(text "D"
					(at -0.635 2.2225 0)
				)
				(text "G"
					(at -3.4925 0 0)
				)
				(text "S"
					(at -0.635 -3.175 0)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010004"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "10K"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 10K-5%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402JR-0710KL"
				(at 0 0 0)
			)
			(property "SKU" "301010004"
				(at 0 0 0)
			)
			(property "Resistance" "10K"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "5%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010004_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010005"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "47K"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 47K-5%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402JR-0747KL"
				(at 0 0 0)
			)
			(property "SKU" "301010005"
				(at 0 0 0)
			)
			(property "Resistance" "47K"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "5%"
				(at 0 0 0)
			)
			(property "Status" "reSpeaker"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010005_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010010"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "4.7K"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 4.7K-5%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402JR-074K7L"
				(at 0 0 0)
			)
			(property "SKU" "301010010"
				(at 0 0 0)
			)
			(property "Resistance" "4.7K"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "5%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010010_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010028"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "100R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 100R-5%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402JR-07100RL"
				(at 0 0 0)
			)
			(property "SKU" "301010028"
				(at 0 0 0)
			)
			(property "Resistance" "100R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "5%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010028_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010034"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "33R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 33R-5%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402JR-0733RL"
				(at 0 0 0)
			)
			(property "SKU" "301010034"
				(at 0 0 0)
			)
			(property "Resistance" "33R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "5%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010034_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010041"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "49.9R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 49.9R-1%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-0749R9L"
				(at 0 0 0)
			)
			(property "SKU" "301010041"
				(at 0 0 0)
			)
			(property "Resistance" "49.9R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010041_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010058"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "75R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 75R-1%-1/10W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-0775RL"
				(at 0 0 0)
			)
			(property "SKU" "301010058"
				(at 0 0 0)
			)
			(property "Resistance" "75R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "JetsonNano Cluster"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 125°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010058_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010444"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "10R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 10R-1%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-0710RL"
				(at 0 0 0)
			)
			(property "SKU" "301010444"
				(at 0 0 0)
			)
			(property "Resistance" "10R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "IOT Enabling Dongle Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010444_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010456"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "100K"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 100K-1%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-07100KL"
				(at 0 0 0)
			)
			(property "SKU" "301010456"
				(at 0 0 0)
			)
			(property "Resistance" "100K"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010456_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301010626"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "120R"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES;120R-1%-1/16W-0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-07120RL"
				(at 0 0 0)
			)
			(property "SKU" "301010626"
				(at 0 0 0)
			)
			(property "Resistance" "120R"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "reTerminal DM"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301010626_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Resistors/301011829"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at -1.905 0.635 0)
			)
			(property "Value" "13.3K"
				(at 0.635 0.635 0)
			)
			(property "Footprint" "Resistor:R0402"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD RES 13.3K-1%-1/16W;0402"
				(at 0 0 0)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
			)
			(property "MPN" "RC0402FR-0713K3L"
				(at 0 0 0)
			)
			(property "SKU" "301011829"
				(at 0 0 0)
			)
			(property "Resistance" "13.3K"
				(at 0 0 0)
			)
			(property "Tolerance" ""
				(at 0 0 0)
			)
			(property "Part Type" "RES"
				(at 0 0 0)
			)
			(property "Power Rating" "1%"
				(at 0 0 0)
			)
			(property "Status" "BeagleBone Carrier Board"
				(at 0 0 0)
			)
			(property "Temperature" "-55°C to 155°C"
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor:R0402"
				(at 0 0 0)
			)
			(symbol "Resistors/301011829_0_0"
				(rectangle
					(start -1.27 -0.508)
					(end 1.27 0.508)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "Seeed_libdb:Switch/311030001"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at -3.81 3.81 0)
			)
			(property "Value" "MK-12C02 G1.5"
				(at -1.27 2.54 0)
			)
			(property "Footprint" "Switch:SW7-SMD-L6.7X2.7X3.2MM"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "SMD TopToggle Switch SPDT;7P-L6.7*W2.7*H3.2mm"
				(at 0 0 0)
			)
			(property "Manufacturer" "DeYiLong"
				(at 0 0 0)
			)
			(property "MPN" "MK-12C02 G1.5"
				(at 0 0 0)
			)
			(property "SKU" "311030001"
				(at 0 0 0)
			)
			(property "Part Type" "Switch"
				(at 0 0 0)
			)
			(property "Rating" ""
				(at 0 0 0)
			)
			(property "Status" "HA Voice KIT"
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Switch:SW7-SMD-L6.7X2.7X3.2MM"
				(at 0 0 0)
			)
			(symbol "Switch/311030001_1_0"
				(polyline
					(pts
						(xy -3.81 -3.175) (xy -4.445 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -2.54) (xy -4.445 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -2.54) (xy -3.81 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -1.27) (xy -2.54 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -2.54) (xy -3.81 -3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.175 -2.54) (xy -3.81 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -1.27) (xy -2.54 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 0) (xy -3.81 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 0) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 1.27 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 2.54 2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "COM")
					(number "2")
				)
				(pin passive line
					(at 2.54 -2.54 180)
					(length 2.54)
					(name "B")
					(number "3")
				)
				(pin passive line
					(at -2.54 -3.81 90)
					(length 2.54)
					(name "SS2")
					(number "P1")
				)
				(pin passive line
					(at -2.54 -3.81 90)
					(length 2.54)
					(name "SS2")
					(number "P2")
				)
				(pin passive line
					(at -2.54 -3.81 90)
					(length 2.54)
					(name "SS2")
					(number "P3")
				)
				(pin passive line
					(at -2.54 -3.81 90)
					(length 2.54)
					(name "SS2")
					(number "P4")
				)
			)
		)
		(symbol "Seeed_libdb:Transistor/305050111"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 1.27 1.27 0)
			)
			(property "Value" "BC856S"
				(at 3.81 1.27 0)
			)
			(property "Footprint" "Transistor:SOT-363"
				(at 5.08 0 0)
			)
			(property "Datasheet" ""
				(at 5.08 0 0)
			)
			(property "Description" "SMD Transistor Array 2 PNP -65V-100mA"
				(at 5.08 0 0)
			)
			(property "Manufacturer" "CJ"
				(at 0 0 0)
			)
			(property "MPN" "BC856S"
				(at 0 0 0)
			)
			(property "SKU" "305050111"
				(at 0 0 0)
			)
			(property "Part Type" "PNP"
				(at 0 0 0)
			)
			(property "Rating" "65V-100mA"
				(at 0 0 0)
			)
			(property "Status" "SenseCAP A1102"
				(at 0 0 0)
			)
			(property "Temperature" ""
				(at 0 0 0)
			)
			(property "Priority" ""
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Transistor:SOT-363"
				(at 0 0 0)
			)
			(symbol "Transistor/305050111_0_1"
				(polyline
					(pts
						(xy -1.27 -2.54) (xy -1.27 0) (xy -5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 1.27 0) (xy 1.27 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Transistor/305050111_1_0"
				(polyline
					(pts
						(xy -5.08 -2.54) (xy -5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -7.62 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -7.62 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -6.35 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -5.715 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -5.08 0) (xy -5.08 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 -2.54) (xy 5.08 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.08 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 5.715 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 6.35 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 7.62 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 7.62 2.54)
					)
					(fill
						(type none)
					)
				)
				(text "B"
					(at -4.445 0 0)
				)
				(text "B"
					(at 4.445 0 0)
				)
				(text "C"
					(at -6.985 -3.175 0)
				)
				(text "C"
					(at 6.985 -3.175 0)
				)
				(text "E"
					(at -6.985 2.54 0)
				)
				(text "E"
					(at 6.985 2.54 0)
				)
				(pin passive line
					(at -7.62 5.08 270)
					(length 2.54)
					(name "E")
					(number "1")
				)
				(pin passive line
					(at -1.27 -5.08 90)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 7.62 -5.08 90)
					(length 2.54)
					(name "C")
					(number "3")
				)
				(pin passive line
					(at 7.62 5.08 270)
					(length 2.54)
					(name "E")
					(number "4")
				)
				(pin passive line
					(at 1.27 5.08 270)
					(length 2.54)
					(name "B")
					(number "5")
				)
				(pin passive line
					(at -7.62 -5.08 90)
					(length 2.54)
					(name "C")
					(number "6")
				)
			)
		)
	)
	(junction
		(at 171.45 30.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 87.63 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 83.82 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 120.65 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 127 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 266.7 138.43)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 226.06 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 99.06 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 156.21)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 226.06 30.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 116.84 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 212.09 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 124.46 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 40.64 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 232.41 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 135.89 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 110.49)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 100.33)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 153.67)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 200.66 40.64)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 254 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 121.92)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 241.3 30.48)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 262.89 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 30.48 158.75)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 30.48 151.13)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 257.81 130.81)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 22.86 38.1)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 161.29 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 198.12 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 137.16 88.9)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 100.33 176.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 95.25 173.99)
	)
	(no_connect
		(at 176.53 43.18)
	)
	(no_connect
		(at 59.69 93.98)
	)
	(wire
		(pts
			(xy 22.86 34.29) (xy 22.86 38.1)
		)
	)
	(wire
		(pts
			(xy 233.68 49.53) (xy 233.68 38.1)
		)
	)
	(wire
		(pts
			(xy 254 60.96) (xy 254 59.69)
		)
	)
	(wire
		(pts
			(xy 53.34 88.9) (xy 59.69 88.9)
		)
	)
	(wire
		(pts
			(xy 201.93 76.2) (xy 201.93 73.66)
		)
	)
	(wire
		(pts
			(xy 233.68 73.66) (xy 255.27 73.66)
		)
	)
	(wire
		(pts
			(xy 100.33 176.53) (xy 116.84 176.53)
		)
	)
	(wire
		(pts
			(xy 217.17 30.48) (xy 226.06 30.48)
		)
	)
	(wire
		(pts
			(xy 176.53 38.1) (xy 171.45 38.1)
		)
	)
	(wire
		(pts
			(xy 250.19 142.24) (xy 278.13 142.24)
		)
	)
	(wire
		(pts
			(xy 233.68 35.56) (xy 233.68 36.83)
		)
	)
	(wire
		(pts
			(xy 161.29 83.82) (xy 161.29 88.9)
		)
	)
	(wire
		(pts
			(xy 36.83 38.1) (xy 45.72 38.1)
		)
	)
	(wire
		(pts
			(xy 171.45 24.13) (xy 171.45 30.48)
		)
	)
	(wire
		(pts
			(xy 80.01 153.67) (xy 97.79 153.67)
		)
	)
	(wire
		(pts
			(xy 137.16 100.33) (xy 147.32 100.33)
		)
	)
	(wire
		(pts
			(xy 50.8 151.13) (xy 62.23 151.13)
		)
	)
	(wire
		(pts
			(xy 135.89 167.64) (xy 146.05 167.64)
		)
	)
	(wire
		(pts
			(xy 262.89 49.53) (xy 262.89 52.07)
		)
	)
	(wire
		(pts
			(xy 198.12 83.82) (xy 198.12 85.09)
		)
	)
	(wire
		(pts
			(xy 137.16 100.33) (xy 137.16 101.6)
		)
	)
	(wire
		(pts
			(xy 40.64 93.98) (xy 40.64 96.52)
		)
	)
	(wire
		(pts
			(xy 196.85 76.2) (xy 201.93 76.2)
		)
	)
	(wire
		(pts
			(xy 226.06 30.48) (xy 226.06 38.1)
		)
	)
	(wire
		(pts
			(xy 50.8 158.75) (xy 62.23 158.75)
		)
	)
	(wire
		(pts
			(xy 181.61 44.45) (xy 181.61 46.99)
		)
	)
	(wire
		(pts
			(xy 233.68 36.83) (xy 240.03 36.83)
		)
	)
	(wire
		(pts
			(xy 80.01 151.13) (xy 83.82 151.13)
		)
	)
	(wire
		(pts
			(xy 127 34.29) (xy 127 38.1)
		)
	)
	(wire
		(pts
			(xy 22.86 83.82) (xy 22.86 86.36)
		)
	)
	(wire
		(pts
			(xy 30.48 151.13) (xy 43.18 151.13)
		)
	)
	(wire
		(pts
			(xy 200.66 40.64) (xy 212.09 40.64)
		)
	)
	(wire
		(pts
			(xy 93.98 156.21) (xy 93.98 176.53)
		)
	)
	(wire
		(pts
			(xy 127 49.53) (xy 127 52.07)
		)
	)
	(wire
		(pts
			(xy 54.61 156.21) (xy 54.61 153.67)
		)
	)
	(wire
		(pts
			(xy 233.68 78.74) (xy 255.27 78.74)
		)
	)
	(wire
		(pts
			(xy 120.65 153.67) (xy 120.65 177.8)
		)
	)
	(wire
		(pts
			(xy 198.12 40.64) (xy 200.66 40.64)
		)
	)
	(wire
		(pts
			(xy 30.48 158.75) (xy 43.18 158.75)
		)
	)
	(wire
		(pts
			(xy 111.76 49.53) (xy 111.76 52.07)
		)
	)
	(wire
		(pts
			(xy 85.09 110.49) (xy 137.16 110.49)
		)
	)
	(wire
		(pts
			(xy 151.13 88.9) (xy 161.29 88.9)
		)
	)
	(wire
		(pts
			(xy 137.16 109.22) (xy 137.16 110.49)
		)
	)
	(wire
		(pts
			(xy 200.66 40.64) (xy 200.66 44.45)
		)
	)
	(wire
		(pts
			(xy 124.46 99.06) (xy 124.46 101.6)
		)
	)
	(wire
		(pts
			(xy 167.64 138.43) (xy 203.2 138.43)
		)
	)
	(wire
		(pts
			(xy 262.89 49.53) (xy 270.51 49.53)
		)
	)
	(wire
		(pts
			(xy 22.86 96.52) (xy 22.86 93.98)
		)
	)
	(wire
		(pts
			(xy 105.41 38.1) (xy 111.76 38.1)
		)
	)
	(wire
		(pts
			(xy 213.36 80.01) (xy 196.85 80.01)
		)
	)
	(wire
		(pts
			(xy 83.82 151.13) (xy 86.36 151.13)
		)
	)
	(wire
		(pts
			(xy 40.64 83.82) (xy 40.64 86.36)
		)
	)
	(wire
		(pts
			(xy 137.16 99.06) (xy 137.16 100.33)
		)
	)
	(wire
		(pts
			(xy 80.01 156.21) (xy 93.98 156.21)
		)
	)
	(wire
		(pts
			(xy 40.64 83.82) (xy 59.69 83.82)
		)
	)
	(wire
		(pts
			(xy 198.12 83.82) (xy 199.39 83.82)
		)
	)
	(wire
		(pts
			(xy 250.19 153.67) (xy 278.13 153.67)
		)
	)
	(wire
		(pts
			(xy 250.19 146.05) (xy 278.13 146.05)
		)
	)
	(wire
		(pts
			(xy 233.68 38.1) (xy 234.95 38.1)
		)
	)
	(wire
		(pts
			(xy 85.09 88.9) (xy 86.36 88.9)
		)
	)
	(wire
		(pts
			(xy 22.86 83.82) (xy 40.64 83.82)
		)
	)
	(wire
		(pts
			(xy 135.89 176.53) (xy 144.78 176.53)
		)
	)
	(wire
		(pts
			(xy 215.9 101.6) (xy 196.85 101.6)
		)
	)
	(wire
		(pts
			(xy 85.09 83.82) (xy 85.09 88.9)
		)
	)
	(wire
		(pts
			(xy 30.48 158.75) (xy 30.48 162.56)
		)
	)
	(wire
		(pts
			(xy 266.7 138.43) (xy 269.24 138.43)
		)
	)
	(wire
		(pts
			(xy 111.76 38.1) (xy 111.76 41.91)
		)
	)
	(wire
		(pts
			(xy 124.46 88.9) (xy 137.16 88.9)
		)
	)
	(wire
		(pts
			(xy 226.06 49.53) (xy 232.41 49.53)
		)
	)
	(wire
		(pts
			(xy 232.41 49.53) (xy 232.41 48.26)
		)
	)
	(wire
		(pts
			(xy 234.95 110.49) (xy 255.27 110.49)
		)
	)
	(wire
		(pts
			(xy 212.09 35.56) (xy 212.09 40.64)
		)
	)
	(wire
		(pts
			(xy 87.63 38.1) (xy 99.06 38.1)
		)
	)
	(wire
		(pts
			(xy 213.36 73.66) (xy 213.36 80.01)
		)
	)
	(wire
		(pts
			(xy 137.16 88.9) (xy 144.78 88.9)
		)
	)
	(wire
		(pts
			(xy 137.16 88.9) (xy 137.16 91.44)
		)
	)
	(wire
		(pts
			(xy 133.35 153.67) (xy 135.89 153.67)
		)
	)
	(wire
		(pts
			(xy 233.68 83.82) (xy 255.27 83.82)
		)
	)
	(wire
		(pts
			(xy 137.16 110.49) (xy 137.16 113.03)
		)
	)
	(wire
		(pts
			(xy 167.64 130.81) (xy 203.2 130.81)
		)
	)
	(wire
		(pts
			(xy 184.15 40.64) (xy 190.5 40.64)
		)
	)
	(wire
		(pts
			(xy 74.93 88.9) (xy 85.09 88.9)
		)
	)
	(wire
		(pts
			(xy 137.16 110.49) (xy 147.32 110.49)
		)
	)
	(wire
		(pts
			(xy 238.76 30.48) (xy 241.3 30.48)
		)
	)
	(wire
		(pts
			(xy 167.64 142.24) (xy 203.2 142.24)
		)
	)
	(wire
		(pts
			(xy 232.41 49.53) (xy 233.68 49.53)
		)
	)
	(wire
		(pts
			(xy 234.95 115.57) (xy 255.27 115.57)
		)
	)
	(wire
		(pts
			(xy 116.84 139.7) (xy 116.84 142.24)
		)
	)
	(wire
		(pts
			(xy 226.06 59.69) (xy 226.06 58.42)
		)
	)
	(wire
		(pts
			(xy 171.45 38.1) (xy 171.45 30.48)
		)
	)
	(wire
		(pts
			(xy 116.84 149.86) (xy 116.84 176.53)
		)
	)
	(wire
		(pts
			(xy 111.76 88.9) (xy 124.46 88.9)
		)
	)
	(wire
		(pts
			(xy 226.06 30.48) (xy 228.6 30.48)
		)
	)
	(wire
		(pts
			(xy 241.3 30.48) (xy 241.3 38.1)
		)
	)
	(wire
		(pts
			(xy 80.01 158.75) (xy 86.36 158.75)
		)
	)
	(wire
		(pts
			(xy 158.75 165.1) (xy 161.29 165.1)
		)
	)
	(wire
		(pts
			(xy 215.9 105.41) (xy 196.85 105.41)
		)
	)
	(wire
		(pts
			(xy 147.32 100.33) (xy 147.32 101.6)
		)
	)
	(wire
		(pts
			(xy 147.32 109.22) (xy 147.32 110.49)
		)
	)
	(wire
		(pts
			(xy 167.64 134.62) (xy 203.2 134.62)
		)
	)
	(wire
		(pts
			(xy 135.89 162.56) (xy 146.05 162.56)
		)
	)
	(wire
		(pts
			(xy 97.79 153.67) (xy 97.79 156.21)
		)
	)
	(wire
		(pts
			(xy 212.09 52.07) (xy 212.09 59.69)
		)
	)
	(wire
		(pts
			(xy 226.06 48.26) (xy 226.06 49.53)
		)
	)
	(wire
		(pts
			(xy 243.84 49.53) (xy 241.3 49.53)
		)
	)
	(wire
		(pts
			(xy 254 49.53) (xy 262.89 49.53)
		)
	)
	(wire
		(pts
			(xy 233.68 88.9) (xy 255.27 88.9)
		)
	)
	(wire
		(pts
			(xy 45.72 38.1) (xy 57.15 38.1)
		)
	)
	(wire
		(pts
			(xy 254 49.53) (xy 254 52.07)
		)
	)
	(wire
		(pts
			(xy 87.63 38.1) (xy 87.63 41.91)
		)
	)
	(wire
		(pts
			(xy 87.63 49.53) (xy 87.63 52.07)
		)
	)
	(wire
		(pts
			(xy 233.68 86.36) (xy 255.27 86.36)
		)
	)
	(wire
		(pts
			(xy 135.89 147.32) (xy 135.89 153.67)
		)
	)
	(wire
		(pts
			(xy 226.06 49.53) (xy 226.06 50.8)
		)
	)
	(wire
		(pts
			(xy 120.65 185.42) (xy 120.65 186.69)
		)
	)
	(wire
		(pts
			(xy 116.84 176.53) (xy 125.73 176.53)
		)
	)
	(wire
		(pts
			(xy 167.64 146.05) (xy 203.2 146.05)
		)
	)
	(wire
		(pts
			(xy 167.64 149.86) (xy 203.2 149.86)
		)
	)
	(wire
		(pts
			(xy 198.12 92.71) (xy 198.12 93.98)
		)
	)
	(wire
		(pts
			(xy 19.05 153.67) (xy 54.61 153.67)
		)
	)
	(wire
		(pts
			(xy 255.27 102.87) (xy 236.22 102.87)
		)
	)
	(wire
		(pts
			(xy 241.3 30.48) (xy 251.46 30.48)
		)
	)
	(wire
		(pts
			(xy 100.33 173.99) (xy 100.33 176.53)
		)
	)
	(wire
		(pts
			(xy 234.95 107.95) (xy 255.27 107.95)
		)
	)
	(wire
		(pts
			(xy 250.19 130.81) (xy 257.81 130.81)
		)
	)
	(wire
		(pts
			(xy 54.61 138.43) (xy 54.61 140.97)
		)
	)
	(wire
		(pts
			(xy 233.68 81.28) (xy 255.27 81.28)
		)
	)
	(wire
		(pts
			(xy 212.09 40.64) (xy 212.09 44.45)
		)
	)
	(wire
		(pts
			(xy 200.66 52.07) (xy 200.66 59.69)
		)
	)
	(wire
		(pts
			(xy 250.19 138.43) (xy 266.7 138.43)
		)
	)
	(wire
		(pts
			(xy 19.05 151.13) (xy 30.48 151.13)
		)
	)
	(wire
		(pts
			(xy 93.98 176.53) (xy 100.33 176.53)
		)
	)
	(wire
		(pts
			(xy 96.52 88.9) (xy 99.06 88.9)
		)
	)
	(wire
		(pts
			(xy 45.72 48.26) (xy 45.72 53.34)
		)
	)
	(wire
		(pts
			(xy 97.79 163.83) (xy 97.79 166.37)
		)
	)
	(wire
		(pts
			(xy 135.89 153.67) (xy 135.89 162.56)
		)
	)
	(wire
		(pts
			(xy 167.64 153.67) (xy 203.2 153.67)
		)
	)
	(wire
		(pts
			(xy 135.89 153.67) (xy 144.78 153.67)
		)
	)
	(wire
		(pts
			(xy 161.29 88.9) (xy 162.56 88.9)
		)
	)
	(wire
		(pts
			(xy 251.46 26.67) (xy 251.46 30.48)
		)
	)
	(wire
		(pts
			(xy 53.34 96.52) (xy 53.34 88.9)
		)
	)
	(wire
		(pts
			(xy 111.76 38.1) (xy 127 38.1)
		)
	)
	(wire
		(pts
			(xy 101.6 168.91) (xy 104.14 168.91)
		)
	)
	(wire
		(pts
			(xy 54.61 153.67) (xy 62.23 153.67)
		)
	)
	(wire
		(pts
			(xy 54.61 148.59) (xy 54.61 153.67)
		)
	)
	(wire
		(pts
			(xy 86.36 158.75) (xy 86.36 162.56)
		)
	)
	(wire
		(pts
			(xy 234.95 113.03) (xy 255.27 113.03)
		)
	)
	(wire
		(pts
			(xy 120.65 153.67) (xy 125.73 153.67)
		)
	)
	(wire
		(pts
			(xy 255.27 105.41) (xy 236.22 105.41)
		)
	)
	(wire
		(pts
			(xy 45.72 38.1) (xy 45.72 34.29)
		)
	)
	(wire
		(pts
			(xy 135.89 167.64) (xy 135.89 176.53)
		)
	)
	(wire
		(pts
			(xy 269.24 130.81) (xy 275.59 130.81)
		)
	)
	(wire
		(pts
			(xy 111.76 99.06) (xy 111.76 101.6)
		)
	)
	(wire
		(pts
			(xy 22.86 48.26) (xy 22.86 53.34)
		)
	)
	(wire
		(pts
			(xy 137.16 120.65) (xy 137.16 121.92)
		)
	)
	(wire
		(pts
			(xy 137.16 121.92) (xy 137.16 123.19)
		)
	)
	(wire
		(pts
			(xy 22.86 38.1) (xy 30.48 38.1)
		)
	)
	(wire
		(pts
			(xy 87.63 34.29) (xy 87.63 38.1)
		)
	)
	(wire
		(pts
			(xy 135.89 176.53) (xy 135.89 181.61)
		)
	)
	(wire
		(pts
			(xy 54.61 156.21) (xy 54.61 161.29)
		)
	)
	(wire
		(pts
			(xy 250.19 149.86) (xy 278.13 149.86)
		)
	)
	(wire
		(pts
			(xy 54.61 168.91) (xy 54.61 171.45)
		)
	)
	(wire
		(pts
			(xy 83.82 146.05) (xy 83.82 151.13)
		)
	)
	(wire
		(pts
			(xy 74.93 93.98) (xy 85.09 93.98)
		)
	)
	(wire
		(pts
			(xy 97.79 153.67) (xy 120.65 153.67)
		)
	)
	(wire
		(pts
			(xy 133.35 176.53) (xy 135.89 176.53)
		)
	)
	(wire
		(pts
			(xy 233.68 76.2) (xy 255.27 76.2)
		)
	)
	(wire
		(pts
			(xy 99.06 88.9) (xy 111.76 88.9)
		)
	)
	(wire
		(pts
			(xy 257.81 127) (xy 257.81 130.81)
		)
	)
	(wire
		(pts
			(xy 62.23 156.21) (xy 54.61 156.21)
		)
	)
	(wire
		(pts
			(xy 241.3 49.53) (xy 241.3 48.26)
		)
	)
	(wire
		(pts
			(xy 85.09 83.82) (xy 83.82 83.82)
		)
	)
	(wire
		(pts
			(xy 99.06 91.44) (xy 99.06 88.9)
		)
	)
	(wire
		(pts
			(xy 257.81 130.81) (xy 261.62 130.81)
		)
	)
	(wire
		(pts
			(xy 22.86 81.28) (xy 22.86 83.82)
		)
	)
	(wire
		(pts
			(xy 254 49.53) (xy 251.46 49.53)
		)
	)
	(wire
		(pts
			(xy 255.27 100.33) (xy 236.22 100.33)
		)
	)
	(wire
		(pts
			(xy 198.12 83.82) (xy 196.85 83.82)
		)
	)
	(wire
		(pts
			(xy 22.86 38.1) (xy 22.86 41.91)
		)
	)
	(wire
		(pts
			(xy 250.19 134.62) (xy 255.27 134.62)
		)
	)
	(wire
		(pts
			(xy 127 41.91) (xy 127 38.1)
		)
	)
	(wire
		(pts
			(xy 228.6 83.82) (xy 207.01 83.82)
		)
	)
	(wire
		(pts
			(xy 111.76 91.44) (xy 111.76 88.9)
		)
	)
	(wire
		(pts
			(xy 203.2 109.22) (xy 203.2 113.03)
		)
	)
	(wire
		(pts
			(xy 99.06 99.06) (xy 99.06 101.6)
		)
	)
	(wire
		(pts
			(xy 85.09 93.98) (xy 85.09 110.49)
		)
	)
	(wire
		(pts
			(xy 137.16 121.92) (xy 148.59 121.92)
		)
	)
	(wire
		(pts
			(xy 93.98 151.13) (xy 96.52 151.13)
		)
	)
	(wire
		(pts
			(xy 171.45 30.48) (xy 207.01 30.48)
		)
	)
	(wire
		(pts
			(xy 30.48 144.78) (xy 30.48 151.13)
		)
	)
	(wire
		(pts
			(xy 196.85 109.22) (xy 203.2 109.22)
		)
	)
	(wire
		(pts
			(xy 19.05 158.75) (xy 30.48 158.75)
		)
	)
	(wire
		(pts
			(xy 262.89 59.69) (xy 262.89 60.96)
		)
	)
	(wire
		(pts
			(xy 74.93 83.82) (xy 76.2 83.82)
		)
	)
	(wire
		(pts
			(xy 124.46 88.9) (xy 124.46 91.44)
		)
	)
	(wire
		(pts
			(xy 45.72 40.64) (xy 45.72 38.1)
		)
	)
	(wire
		(pts
			(xy 266.7 137.16) (xy 266.7 138.43)
		)
	)
	(text "Vout = (R9/R6+1)*Vfb"
		(exclude_from_sim no)
		(at 68.072 105.156 0)
	)
	(text "0.35A"
		(exclude_from_sim no)
		(at 50.038 37.084 0)
	)
	(text "DC 12V to 5V"
		(exclude_from_sim no)
		(at 67.818 110.49 0)
	)
	(text "XIAO-ESP32C3 Core"
		(exclude_from_sim no)
		(at 227.076 160.02 0)
	)
	(text "500mA"
		(exclude_from_sim no)
		(at 246.888 29.464 0)
	)
	(text "Vin 12V"
		(exclude_from_sim no)
		(at 46.736 60.96 0)
	)
	(text "Connector"
		(exclude_from_sim no)
		(at 223.012 118.364 0)
	)
	(text "Vout 5V"
		(exclude_from_sim no)
		(at 218.694 66.294 0)
	)
	(text "700mA"
		(exclude_from_sim no)
		(at 122.428 37.084 0)
	)
	(text "700mA"
		(exclude_from_sim no)
		(at 157.48 87.884 0)
	)
	(text "700mA"
		(exclude_from_sim no)
		(at 254 130.048 0)
	)
	(text "Vin 5V"
		(exclude_from_sim no)
		(at 111.506 60.96 0)
	)
	(text "TTL to RS485"
		(exclude_from_sim no)
		(at 70.866 166.624 0)
	)
	(label "RS485_RX{slash}Himax_PA2"
		(at 19.05 151.13 0)
		(fields_autoplaced yes)
	)
	(label "SPI_MISO{slash}Himax_PB3"
		(at 278.13 146.05 180)
		(fields_autoplaced yes)
	)
	(label "RS485_TX{slash}Himax_PA3"
		(at 233.68 83.82 0)
		(fields_autoplaced yes)
	)
	(label "RS485_TX{slash}Himax_PA3"
		(at 19.05 158.75 0)
		(fields_autoplaced yes)
	)
	(label "RS485_DE{slash}Himax_PB8"
		(at 233.68 78.74 0)
		(fields_autoplaced yes)
	)
	(label "Himax_PB6"
		(at 167.64 153.67 0)
		(fields_autoplaced yes)
	)
	(label "RS485_A"
		(at 144.78 176.53 180)
		(fields_autoplaced yes)
	)
	(label "RS485_DE{slash}Himax_PB8"
		(at 19.05 153.67 0)
		(fields_autoplaced yes)
	)
	(label "SPI_MOSI{slash}Himax_PB2"
		(at 278.13 142.24 180)
		(fields_autoplaced yes)
	)
	(label "SPI_SCK{slash}Himax_PB4"
		(at 278.13 149.86 180)
		(fields_autoplaced yes)
	)
	(label "RS485_B"
		(at 215.9 105.41 180)
		(fields_autoplaced yes)
	)
	(label "MOS_G"
		(at 270.51 49.53 180)
		(fields_autoplaced yes)
	)
	(label "EXD_INT{slash}Himax_PA0"
		(at 167.64 130.81 0)
		(fields_autoplaced yes)
	)
	(label "SPI_SCK{slash}Himax_PB4"
		(at 234.95 113.03 0)
		(fields_autoplaced yes)
	)
	(label "RS485A"
		(at 104.14 176.53 0)
		(fields_autoplaced yes)
	)
	(label "SPI_CS{slash}Himax_PB11"
		(at 233.68 76.2 0)
		(fields_autoplaced yes)
	)
	(label "MOS_G"
		(at 240.03 36.83 180)
		(fields_autoplaced yes)
	)
	(label "SPI_CS{slash}Himax_PB11"
		(at 167.64 134.62 0)
		(fields_autoplaced yes)
	)
	(label "RS485_B"
		(at 144.78 153.67 180)
		(fields_autoplaced yes)
	)
	(label "RS485_RX{slash}Himax_PA2"
		(at 233.68 86.36 0)
		(fields_autoplaced yes)
	)
	(label "RS485_A"
		(at 215.9 101.6 180)
		(fields_autoplaced yes)
	)
	(label "Himax_RST"
		(at 233.68 81.28 0)
		(fields_autoplaced yes)
	)
	(label "SPI_MISO{slash}Himax_PB3"
		(at 234.95 110.49 0)
		(fields_autoplaced yes)
	)
	(label "RS485_TX{slash}Himax_PA3"
		(at 167.64 146.05 0)
		(fields_autoplaced yes)
	)
	(label "EXD_INT{slash}Himax_PA0"
		(at 233.68 73.66 0)
		(fields_autoplaced yes)
	)
	(label "Himax_PB7"
		(at 234.95 115.57 0)
		(fields_autoplaced yes)
	)
	(label "RS485_DE{slash}Himax_PB8"
		(at 167.64 138.43 0)
		(fields_autoplaced yes)
	)
	(label "Himax_PB7"
		(at 278.13 153.67 180)
		(fields_autoplaced yes)
	)
	(label "Himax_RST"
		(at 167.64 142.24 0)
		(fields_autoplaced yes)
	)
	(label "RS485_RX{slash}Himax_PA2"
		(at 167.64 149.86 0)
		(fields_autoplaced yes)
	)
	(label "EXD_INT{slash}Himax_PA0"
		(at 228.6 83.82 180)
		(fields_autoplaced yes)
	)
	(label "Himax_PB6"
		(at 233.68 88.9 0)
		(fields_autoplaced yes)
	)
	(label "SPI_MOSI{slash}Himax_PB2"
		(at 234.95 107.95 0)
		(fields_autoplaced yes)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 254 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR028"
			(at 254 67.31 0)
		)
		(property "Value" "GND"
			(at 254 65.024 0)
		)
		(property "Footprint" ""
			(at 254 60.96 0)
		)
		(property "Datasheet" ""
			(at 254 60.96 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 254 60.96 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR028")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304011053")
		(at 34.29 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 33.655 29.21 0)
		)
		(property "Value" "B5819WS SL"
			(at 33.655 31.75 0)
		)
		(property "Footprint" "Diode:SOD-323"
			(at 34.29 38.1 0)
		)
		(property "Datasheet" ""
			(at 34.29 38.1 0)
		)
		(property "Description" "SMD Diode Schottky 40V-1A;SOD-323"
			(at 34.29 38.1 0)
		)
		(property "Manufacturer" "CJ"
			(at 34.29 38.1 0)
		)
		(property "MPN" "B5819WS SL"
			(at 34.29 38.1 0)
		)
		(property "SKU" "304011053"
			(at 34.29 38.1 0)
		)
		(property "Part Type" "Schottky Diode"
			(at 34.29 38.1 0)
		)
		(property "Rating" "40V"
			(at 33.655 34.29 0)
		)
		(property "Status" "reTerminal DM"
			(at 34.29 38.1 0)
		)
		(property "Temperature" ""
			(at 34.29 38.1 0)
		)
		(property "Priority" ""
			(at 34.29 38.1 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Connector/320110007")
		(at 189.23 105.41 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J2"
			(at 185.42 104.1399 0)
		)
		(property "Value" "3P-3.5"
			(at 185.42 106.6799 0)
		)
		(property "Footprint" "Connector:H3_3d5_11_5x7mm"
			(at 189.23 105.41 0)
		)
		(property "Datasheet" ""
			(at 189.23 105.41 0)
		)
		(property "Description" "DIP Female Screw Terminal-Green;3P-3.5"
			(at 189.23 105.41 0)
		)
		(property "Manufacturer" "SENGER"
			(at 189.23 105.41 0)
		)
		(property "MPN" "GS012S-3.5mm-3P"
			(at 189.23 105.41 0)
		)
		(property "SKU" "320110007"
			(at 189.23 105.41 0)
		)
		(property "Part Type" "Connector"
			(at 189.23 105.41 0)
		)
		(property "Rating" ""
			(at 189.23 105.41 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 189.23 105.41 0)
		)
		(property "Temperature" "-40°C to 105°C"
			(at 189.23 105.41 0)
		)
		(property "Priority" ""
			(at 189.23 105.41 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "J2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304050558")
		(at 152.4 165.1 0)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D6"
			(at 149.606 154.432 0)
		)
		(property "Value" "SM712-02HTG"
			(at 154.178 158.75 0)
		)
		(property "Footprint" "Diode:SOT-23"
			(at 152.4 165.1 0)
		)
		(property "Datasheet" ""
			(at 152.4 165.1 0)
		)
		(property "Description" "SMD Diode TVS 12VWM 31VC"
			(at 152.4 165.1 0)
		)
		(property "Manufacturer" "Littelfuse"
			(at 152.4 165.1 0)
		)
		(property "MPN" "SM712-02HTG"
			(at 152.4 165.1 0)
		)
		(property "SKU" "304050558"
			(at 152.4 165.1 0)
		)
		(property "Part Type" "Diode"
			(at 152.4 165.1 0)
		)
		(property "Rating" "12V"
			(at 150.114 156.464 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 152.4 165.1 0)
		)
		(property "Temperature" "-40°C to 125°C"
			(at 152.4 165.1 0)
		)
		(property "Priority" ""
			(at 152.4 165.1 0)
		)
		(pin "2")
		(pin "1")
		(pin "3")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D6")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010028")
		(at 194.31 40.64 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R18"
			(at 189.738 38.354 0)
		)
		(property "Value" "100R"
			(at 194.31 38.354 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 194.31 40.64 0)
		)
		(property "Datasheet" ""
			(at 194.31 40.64 0)
		)
		(property "Description" "SMD RES 100R-5%-1/16W;0402"
			(at 194.31 40.64 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 194.31 40.64 0)
		)
		(property "MPN" "RC0402JR-07100RL"
			(at 194.31 40.64 0)
		)
		(property "SKU" "301010028"
			(at 194.31 40.64 0)
		)
		(property "Resistance" "100R"
			(at 194.31 40.64 0)
		)
		(property "Tolerance" ""
			(at 194.31 40.64 0)
		)
		(property "Part Type" "RES"
			(at 194.31 40.64 0)
		)
		(property "Power Rating" "5%"
			(at 198.374 38.354 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 194.31 40.64 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 194.31 40.64 0)
		)
		(property "Priority" ""
			(at 194.31 40.64 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R18")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R18")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010004")
		(at 116.84 146.05 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R10"
			(at 118.11 143.5099 90)
		)
		(property "Value" "10K"
			(at 118.11 146.0499 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 116.84 146.05 0)
		)
		(property "Datasheet" ""
			(at 116.84 146.05 0)
		)
		(property "Description" "SMD RES 10K-5%-1/16W;0402"
			(at 116.84 146.05 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 116.84 146.05 0)
		)
		(property "MPN" "RC0402JR-0710KL"
			(at 116.84 146.05 0)
		)
		(property "SKU" "301010004"
			(at 116.84 146.05 0)
		)
		(property "Resistance" "10K"
			(at 116.84 146.05 0)
		)
		(property "Tolerance" ""
			(at 116.84 146.05 0)
		)
		(property "Part Type" "RES"
			(at 116.84 146.05 0)
		)
		(property "Power Rating" "5%"
			(at 118.11 148.5899 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 116.84 146.05 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 116.84 146.05 0)
		)
		(property "Priority" ""
			(at 116.84 146.05 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R10")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304050312")
		(at 87.63 45.72 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D4"
			(at 90.17 43.1799 90)
		)
		(property "Value" "TPD1E10B06DPYR"
			(at 90.17 45.7199 90)
		)
		(property "Footprint" "Diode:ESD-0402"
			(at 87.63 45.72 0)
		)
		(property "Datasheet" ""
			(at 87.63 45.72 0)
		)
		(property "Description" "SMD Diode ESD 5.5V-6V-12pF-30KV-30KV;X1SON(2)"
			(at 87.63 45.72 0)
		)
		(property "Manufacturer" "TI"
			(at 87.63 45.72 0)
		)
		(property "MPN" "TPD1E10B06DPYR"
			(at 87.63 45.72 0)
		)
		(property "SKU" "304050312"
			(at 87.63 45.72 0)
		)
		(property "Part Type" "ESD"
			(at 87.63 45.72 0)
		)
		(property "Rating" "5.5V"
			(at 90.17 48.2599 90)
		)
		(property "Status" ""
			(at 87.63 45.72 0)
		)
		(property "Temperature" "-40°C to 125°C"
			(at 87.63 45.72 0)
		)
		(property "Priority" ""
			(at 87.63 45.72 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 87.63 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 87.63 38.1 0)
		)
		(property "Value" "EXD_+5V"
			(at 87.63 29.21 0)
		)
		(property "Footprint" ""
			(at 87.63 34.29 0)
		)
		(property "Datasheet" ""
			(at 87.63 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 87.63 34.29 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 255.27 134.62 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR030"
			(at 261.62 134.62 0)
		)
		(property "Value" "GND"
			(at 259.08 134.6199 90)
		)
		(property "Footprint" ""
			(at 255.27 134.62 0)
		)
		(property "Datasheet" ""
			(at 255.27 134.62 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 255.27 134.62 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR030")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR030")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 135.89 144.78 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TP7"
			(at 140.97 146.558 90)
		)
		(property "Value" "RS485_B"
			(at 146.304 144.526 90)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 140.97 147.32 0)
		)
		(property "Datasheet" ""
			(at 135.89 144.78 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 135.89 144.78 0)
		)
		(property "Manufacturer" ""
			(at 135.89 144.78 0)
		)
		(property "MPN" ""
			(at 135.89 144.78 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 135.89 144.78 0)
		)
		(property "Part Type" "Test Point"
			(at 135.89 144.78 0)
		)
		(property "Rating" ""
			(at 135.89 144.78 0)
		)
		(property "Status" ""
			(at 135.89 144.78 0)
		)
		(property "Temperature" ""
			(at 135.89 144.78 0)
		)
		(property "Priority" ""
			(at 135.89 144.78 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP7")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+3.3V")
		(at 266.7 137.16 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR037"
			(at 266.7 140.97 0)
		)
		(property "Value" "+3.3V"
			(at 266.7 133.35 0)
		)
		(property "Footprint" ""
			(at 266.7 137.16 0)
		)
		(property "Datasheet" ""
			(at 266.7 137.16 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 266.7 137.16 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR037")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR037")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+12V")
		(at 45.72 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 45.72 38.1 0)
		)
		(property "Value" "+12V"
			(at 45.72 29.21 0)
		)
		(property "Footprint" ""
			(at 45.72 34.29 0)
		)
		(property "Datasheet" ""
			(at 45.72 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 45.72 34.29 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 111.76 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR022"
			(at 111.76 107.95 0)
		)
		(property "Value" "GND"
			(at 111.76 106.68 0)
		)
		(property "Footprint" ""
			(at 111.76 101.6 0)
		)
		(property "Datasheet" ""
			(at 111.76 101.6 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 111.76 101.6 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR022")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR022")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 80.01 83.82 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C5"
			(at 78.232 75.946 90)
		)
		(property "Value" "100nF"
			(at 80.01 78.486 90)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 80.01 83.82 0)
		)
		(property "Datasheet" ""
			(at 80.01 83.82 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 80.01 83.82 0)
		)
		(property "Manufacturer" "TDK"
			(at 80.01 83.82 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 80.01 83.82 0)
		)
		(property "SKU" "302010043"
			(at 80.01 83.82 0)
		)
		(property "Dielectric" ""
			(at 80.01 83.82 0)
		)
		(property "Part Type" "Ceramic"
			(at 80.01 83.82 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 81.026 81.026 90)
		)
		(property "Status" "Testo PoE"
			(at 80.01 83.82 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 80.01 83.82 0)
		)
		(property "Priority" ""
			(at 80.01 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C5")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010058")
		(at 46.99 158.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 43.434 156.464 0)
		)
		(property "Value" "75R"
			(at 46.99 156.464 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 46.99 158.75 0)
		)
		(property "Datasheet" ""
			(at 46.99 158.75 0)
		)
		(property "Description" "SMD RES 75R-1%-1/10W;0402"
			(at 46.99 158.75 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 46.99 158.75 0)
		)
		(property "MPN" "RC0402FR-0775RL"
			(at 46.99 158.75 0)
		)
		(property "SKU" "301010058"
			(at 46.99 158.75 0)
		)
		(property "Resistance" "75R"
			(at 46.99 158.75 0)
		)
		(property "Tolerance" ""
			(at 46.99 158.75 0)
		)
		(property "Part Type" "RES"
			(at 46.99 158.75 0)
		)
		(property "Power Rating" "1%"
			(at 50.8 156.464 0)
		)
		(property "Status" "JetsonNano Cluster"
			(at 46.99 158.75 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 46.99 158.75 0)
		)
		(property "Priority" ""
			(at 46.99 158.75 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 203.2 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR032"
			(at 203.2 119.38 0)
		)
		(property "Value" "GND"
			(at 203.2 118.11 0)
		)
		(property "Footprint" ""
			(at 203.2 113.03 0)
		)
		(property "Datasheet" ""
			(at 203.2 113.03 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 203.2 113.03 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR032")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR032")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304011053")
		(at 148.59 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D3"
			(at 147.955 80.01 0)
		)
		(property "Value" "B5819WS SL"
			(at 147.955 82.55 0)
		)
		(property "Footprint" "Diode:SOD-323"
			(at 148.59 88.9 0)
		)
		(property "Datasheet" ""
			(at 148.59 88.9 0)
		)
		(property "Description" "SMD Diode Schottky 40V-1A;SOD-323"
			(at 148.59 88.9 0)
		)
		(property "Manufacturer" "CJ"
			(at 148.59 88.9 0)
		)
		(property "MPN" "B5819WS SL"
			(at 148.59 88.9 0)
		)
		(property "SKU" "304011053"
			(at 148.59 88.9 0)
		)
		(property "Part Type" "Schottky Diode"
			(at 148.59 88.9 0)
		)
		(property "Rating" "40V"
			(at 147.955 85.09 0)
		)
		(property "Status" "reTerminal DM"
			(at 148.59 88.9 0)
		)
		(property "Temperature" ""
			(at 148.59 88.9 0)
		)
		(property "Priority" ""
			(at 148.59 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302013260")
		(at 22.86 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C1"
			(at 25.4 87.6299 0)
		)
		(property "Value" "22uF"
			(at 25.4 90.1699 0)
		)
		(property "Footprint" "Capacitor:C0805"
			(at 22.86 90.17 0)
		)
		(property "Datasheet" ""
			(at 22.86 90.17 0)
		)
		(property "Description" "SMD CAP Ceramic 22uF-25V-20%-X5R;0805"
			(at 22.86 90.17 0)
		)
		(property "Manufacturer" "Samsung"
			(at 22.86 90.17 0)
		)
		(property "MPN" "CL21A226MAYNNNE"
			(at 22.86 90.17 0)
		)
		(property "SKU" "302013260"
			(at 22.86 90.17 0)
		)
		(property "Dielectric" ""
			(at 22.86 90.17 0)
		)
		(property "Part Type" "Ceramic"
			(at 22.86 90.17 0)
		)
		(property "Voltage Rating" "25V,X5R"
			(at 25.4 92.7099 0)
		)
		(property "Status" ""
			(at 22.86 90.17 0)
		)
		(property "Temperature" "-55°C to 85°C"
			(at 22.86 90.17 0)
		)
		(property "Priority" ""
			(at 22.86 90.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 262.89 60.96 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR036"
			(at 262.89 67.31 0)
		)
		(property "Value" "GND"
			(at 262.89 65.024 0)
		)
		(property "Footprint" ""
			(at 262.89 60.96 0)
		)
		(property "Datasheet" ""
			(at 262.89 60.96 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 262.89 60.96 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR036")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR036")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+12V")
		(at 22.86 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 22.86 38.1 0)
		)
		(property "Value" "EXD_+12V"
			(at 22.86 29.21 0)
		)
		(property "Footprint" ""
			(at 22.86 34.29 0)
		)
		(property "Datasheet" ""
			(at 22.86 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 22.86 34.29 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301011829")
		(at 137.16 116.84 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R6"
			(at 138.43 114.2999 90)
		)
		(property "Value" "13.3K"
			(at 138.43 116.8399 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 137.16 116.84 0)
		)
		(property "Datasheet" ""
			(at 137.16 116.84 0)
		)
		(property "Description" "SMD RES 13.3K-1%-1/16W;0402"
			(at 137.16 116.84 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 137.16 116.84 0)
		)
		(property "MPN" "RC0402FR-0713K3L"
			(at 137.16 116.84 0)
		)
		(property "SKU" "301011829"
			(at 137.16 116.84 0)
		)
		(property "Resistance" "13.3K"
			(at 137.16 116.84 0)
		)
		(property "Tolerance" ""
			(at 137.16 116.84 0)
		)
		(property "Part Type" "RES"
			(at 137.16 116.84 0)
		)
		(property "Power Rating" "1%"
			(at 138.43 119.3799 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 137.16 116.84 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 137.16 116.84 0)
		)
		(property "Priority" ""
			(at 137.16 116.84 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R6")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 30.48 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TP2"
			(at 32.258 163.576 90)
		)
		(property "Value" "RS485_TX"
			(at 32.004 165.608 90)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 25.4 162.56 0)
		)
		(property "Datasheet" ""
			(at 30.48 165.1 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 30.48 165.1 0)
		)
		(property "Manufacturer" ""
			(at 30.48 165.1 0)
		)
		(property "MPN" ""
			(at 30.48 165.1 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 30.48 165.1 0)
		)
		(property "Part Type" "Test Point"
			(at 30.48 165.1 0)
		)
		(property "Rating" ""
			(at 30.48 165.1 0)
		)
		(property "Status" ""
			(at 30.48 165.1 0)
		)
		(property "Temperature" ""
			(at 30.48 165.1 0)
		)
		(property "Priority" ""
			(at 30.48 165.1 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 96.52 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR015"
			(at 102.87 151.13 0)
		)
		(property "Value" "GND"
			(at 99.568 151.13 90)
		)
		(property "Footprint" ""
			(at 96.52 151.13 0)
		)
		(property "Datasheet" ""
			(at 96.52 151.13 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 96.52 151.13 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Module/XIAO-DIP-SMD")
		(at 227.33 142.24 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(property "Reference" "U3"
			(at 227.076 125.73 0)
		)
		(property "Value" "~"
			(at 226.695 127 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 227.33 142.24 0)
		)
		(property "Datasheet" ""
			(at 227.33 142.24 0)
		)
		(property "Description" ""
			(at 227.33 142.24 0)
		)
		(property "Manufacturer" ""
			(at 227.33 142.24 0)
		)
		(property "MPN" ""
			(at 227.33 142.24 0)
		)
		(property "SKU" "XIAO-DIP-SMD"
			(at 227.33 142.24 0)
		)
		(property "Part Type" ""
			(at 227.33 142.24 0)
		)
		(property "Rating" ""
			(at 227.33 142.24 0)
		)
		(property "Status" ""
			(at 227.33 142.24 0)
		)
		(property "Temperature" ""
			(at 227.33 142.24 0)
		)
		(property "Priority" ""
			(at 227.33 142.24 0)
		)
		(pin "1")
		(pin "10")
		(pin "7")
		(pin "11")
		(pin "4")
		(pin "3")
		(pin "6")
		(pin "5")
		(pin "2")
		(pin "14")
		(pin "12")
		(pin "9")
		(pin "8")
		(pin "13")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "U3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 265.43 130.81 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C13"
			(at 262.89 126.492 90)
		)
		(property "Value" "100nF"
			(at 267.97 126.492 90)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 265.43 130.81 0)
		)
		(property "Datasheet" ""
			(at 265.43 130.81 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 265.43 130.81 0)
		)
		(property "Manufacturer" "TDK"
			(at 265.43 130.81 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 265.43 130.81 0)
		)
		(property "SKU" "302010043"
			(at 265.43 130.81 0)
		)
		(property "Dielectric" ""
			(at 265.43 130.81 0)
		)
		(property "Part Type" "Ceramic"
			(at 265.43 130.81 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 265.43 128.524 90)
		)
		(property "Status" "Testo PoE"
			(at 265.43 130.81 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 265.43 130.81 0)
		)
		(property "Priority" ""
			(at 265.43 130.81 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C13")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302013260")
		(at 99.06 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C9"
			(at 101.6 92.7099 0)
		)
		(property "Value" "22uF"
			(at 101.6 95.2499 0)
		)
		(property "Footprint" "Capacitor:C0805"
			(at 99.06 95.25 0)
		)
		(property "Datasheet" ""
			(at 99.06 95.25 0)
		)
		(property "Description" "SMD CAP Ceramic 22uF-25V-20%-X5R;0805"
			(at 99.06 95.25 0)
		)
		(property "Manufacturer" "Samsung"
			(at 99.06 95.25 0)
		)
		(property "MPN" "CL21A226MAYNNNE"
			(at 99.06 95.25 0)
		)
		(property "SKU" "302013260"
			(at 99.06 95.25 0)
		)
		(property "Dielectric" ""
			(at 99.06 95.25 0)
		)
		(property "Part Type" "Ceramic"
			(at 99.06 95.25 0)
		)
		(property "Voltage Rating" "25V,X5R"
			(at 101.6 97.7899 0)
		)
		(property "Status" ""
			(at 99.06 95.25 0)
		)
		(property "Temperature" "-55°C to 85°C"
			(at 99.06 95.25 0)
		)
		(property "Priority" ""
			(at 99.06 95.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C9")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 59.69 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "TP3"
			(at 62.23 36.8299 0)
		)
		(property "Value" "12V"
			(at 62.23 39.3699 0)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 57.15 43.18 0)
		)
		(property "Datasheet" ""
			(at 59.69 38.1 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 59.69 38.1 0)
		)
		(property "Manufacturer" ""
			(at 59.69 38.1 0)
		)
		(property "MPN" ""
			(at 59.69 38.1 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 59.69 38.1 0)
		)
		(property "Part Type" "Test Point"
			(at 59.69 38.1 0)
		)
		(property "Rating" ""
			(at 59.69 38.1 0)
		)
		(property "Status" ""
			(at 59.69 38.1 0)
		)
		(property "Temperature" ""
			(at 59.69 38.1 0)
		)
		(property "Priority" ""
			(at 59.69 38.1 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 127 34.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR023"
			(at 127 38.1 0)
		)
		(property "Value" "+5V"
			(at 127 29.21 0)
		)
		(property "Footprint" ""
			(at 127 34.29 0)
		)
		(property "Datasheet" ""
			(at 127 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 127 34.29 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR023")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010005")
		(at 226.06 54.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R12"
			(at 227.33 52.0699 90)
		)
		(property "Value" "47K"
			(at 227.33 54.6099 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 226.06 54.61 0)
		)
		(property "Datasheet" ""
			(at 226.06 54.61 0)
		)
		(property "Description" "SMD RES 47K-5%-1/16W;0402"
			(at 226.06 54.61 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 226.06 54.61 0)
		)
		(property "MPN" "RC0402JR-0747KL"
			(at 226.06 54.61 0)
		)
		(property "SKU" "301010005"
			(at 226.06 54.61 0)
		)
		(property "Resistance" "47K"
			(at 226.06 54.61 0)
		)
		(property "Tolerance" ""
			(at 226.06 54.61 0)
		)
		(property "Part Type" "RES"
			(at 226.06 54.61 0)
		)
		(property "Power Rating" "5%"
			(at 227.33 57.1499 90)
		)
		(property "Status" "reSpeaker"
			(at 226.06 54.61 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 226.06 54.61 0)
		)
		(property "Priority" ""
			(at 226.06 54.61 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R12")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010006")
		(at 262.89 55.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C14"
			(at 264.668 53.8481 0)
		)
		(property "Value" "10nF"
			(at 264.668 56.134 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 262.89 55.88 0)
		)
		(property "Datasheet" ""
			(at 262.89 55.88 0)
		)
		(property "Description" "SMD CAP Ceramic 10nF-50V-10%-X7R;0402"
			(at 262.89 55.88 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 262.89 55.88 0)
		)
		(property "MPN" "CC0402KRX7R9BB103"
			(at 262.89 55.88 0)
		)
		(property "SKU" "302010006"
			(at 262.89 55.88 0)
		)
		(property "Dielectric" ""
			(at 262.89 55.88 0)
		)
		(property "Part Type" "Ceramic"
			(at 262.89 55.88 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 264.668 58.674 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 262.89 55.88 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 262.89 55.88 0)
		)
		(property "Priority" ""
			(at 262.89 55.88 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C14")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Mosfet/305030010")
		(at 233.68 30.48 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q4"
			(at 233.7113 20.32 90)
		)
		(property "Value" "CJ3407"
			(at 233.7113 22.86 90)
		)
		(property "Footprint" "Mosfet:SOT23"
			(at 233.68 30.48 0)
		)
		(property "Datasheet" ""
			(at 233.68 30.48 0)
		)
		(property "Description" "SMD MOSFET P-CH 30V-4.3A;SOT-23"
			(at 233.68 30.48 0)
		)
		(property "Manufacturer" "长电"
			(at 233.68 30.48 0)
		)
		(property "MPN" "CJ3407"
			(at 233.68 30.48 0)
		)
		(property "SKU" "305030010"
			(at 233.68 30.48 0)
		)
		(property "Part Type" "PMOS"
			(at 233.68 30.48 0)
		)
		(property "Rating" "30V;4.3A"
			(at 233.7113 25.4 90)
		)
		(property "Status" "Sensor Hub"
			(at 233.68 30.48 0)
		)
		(property "Temperature" "-55°C to 150°C"
			(at 233.68 30.48 0)
		)
		(property "Priority" ""
			(at 233.68 30.48 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "Q4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "Q4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Inductor/303010147")
		(at 91.44 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "L1"
			(at 91.44 81.28 0)
		)
		(property "Value" "10uH"
			(at 91.44 83.82 0)
		)
		(property "Footprint" "Inductor:L5040S"
			(at 91.44 88.9 0)
		)
		(property "Datasheet" ""
			(at 91.44 88.9 0)
		)
		(property "Description" "SMD Inductor 10uH-20％-2.35A;5*5*4mm"
			(at 91.44 88.9 0)
		)
		(property "Manufacturer" "Sunlord"
			(at 91.44 88.9 0)
		)
		(property "MPN" "SWPA5040S100MT"
			(at 91.44 88.9 0)
		)
		(property "SKU" "303010147"
			(at 91.44 88.9 0)
		)
		(property "Part Type" "Inductor"
			(at 91.44 88.9 0)
		)
		(property "Rating" "2.35A"
			(at 91.44 86.36 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 91.44 88.9 0)
		)
		(property "Temperature" "-40℃~+125℃"
			(at 91.44 88.9 0)
		)
		(property "Priority" ""
			(at 91.44 88.9 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "L1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "L1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+3.3V")
		(at 83.82 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 83.82 149.86 0)
		)
		(property "Value" "+3.3V"
			(at 83.82 142.24 0)
		)
		(property "Footprint" ""
			(at 83.82 146.05 0)
		)
		(property "Datasheet" ""
			(at 83.82 146.05 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 83.82 146.05 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 45.72 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 45.72 59.69 0)
		)
		(property "Value" "GND"
			(at 45.72 57.404 0)
		)
		(property "Footprint" ""
			(at 45.72 53.34 0)
		)
		(property "Datasheet" ""
			(at 45.72 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 45.72 53.34 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 257.81 127 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR033"
			(at 257.81 130.81 0)
		)
		(property "Value" "+5V"
			(at 257.81 121.92 0)
		)
		(property "Footprint" ""
			(at 257.81 127 0)
		)
		(property "Datasheet" ""
			(at 257.81 127 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 257.81 127 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR033")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR033")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 135.89 184.15 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TP8"
			(at 137.668 182.626 90)
		)
		(property "Value" "RS485_A"
			(at 137.414 184.658 90)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 130.81 181.61 0)
		)
		(property "Datasheet" ""
			(at 135.89 184.15 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 135.89 184.15 0)
		)
		(property "Manufacturer" ""
			(at 135.89 184.15 0)
		)
		(property "MPN" ""
			(at 135.89 184.15 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 135.89 184.15 0)
		)
		(property "Part Type" "Test Point"
			(at 135.89 184.15 0)
		)
		(property "Rating" ""
			(at 135.89 184.15 0)
		)
		(property "Status" ""
			(at 135.89 184.15 0)
		)
		(property "Temperature" ""
			(at 135.89 184.15 0)
		)
		(property "Priority" ""
			(at 135.89 184.15 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP8")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+12V")
		(at 201.93 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR031"
			(at 201.93 77.47 0)
		)
		(property "Value" "EXD_+12V"
			(at 201.93 68.58 0)
		)
		(property "Footprint" ""
			(at 201.93 73.66 0)
		)
		(property "Datasheet" ""
			(at 201.93 73.66 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 201.93 73.66 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR031")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR031")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+3.3V")
		(at 54.61 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR08"
			(at 54.61 142.24 0)
		)
		(property "Value" "+3.3V"
			(at 54.356 134.874 0)
		)
		(property "Footprint" ""
			(at 54.61 138.43 0)
		)
		(property "Datasheet" ""
			(at 54.61 138.43 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 54.61 138.43 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 86.36 162.56 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 86.36 168.91 0)
		)
		(property "Value" "GND"
			(at 86.36 166.624 0)
		)
		(property "Footprint" ""
			(at 86.36 162.56 0)
		)
		(property "Datasheet" ""
			(at 86.36 162.56 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 86.36 162.56 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 53.34 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR010"
			(at 53.34 102.87 0)
		)
		(property "Value" "GND"
			(at 55.372 101.346 0)
		)
		(property "Footprint" ""
			(at 53.34 96.52 0)
		)
		(property "Datasheet" ""
			(at 53.34 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 53.34 96.52 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 124.46 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C12"
			(at 128.27 92.71 0)
		)
		(property "Value" "100nF"
			(at 130.048 95.25 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 124.46 95.25 0)
		)
		(property "Datasheet" ""
			(at 124.46 95.25 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 124.46 95.25 0)
		)
		(property "Manufacturer" "TDK"
			(at 124.46 95.25 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 124.46 95.25 0)
		)
		(property "SKU" "302010043"
			(at 124.46 95.25 0)
		)
		(property "Dielectric" ""
			(at 124.46 95.25 0)
		)
		(property "Part Type" "Ceramic"
			(at 124.46 95.25 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 131.064 97.79 0)
		)
		(property "Status" "Testo PoE"
			(at 124.46 95.25 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 124.46 95.25 0)
		)
		(property "Priority" ""
			(at 124.46 95.25 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C12")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C12")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 127 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C11"
			(at 129.54 43.1799 0)
		)
		(property "Value" "100nF"
			(at 129.54 45.7199 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 127 45.72 0)
		)
		(property "Datasheet" ""
			(at 127 45.72 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 127 45.72 0)
		)
		(property "Manufacturer" "TDK"
			(at 127 45.72 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 127 45.72 0)
		)
		(property "SKU" "302010043"
			(at 127 45.72 0)
		)
		(property "Dielectric" ""
			(at 127 45.72 0)
		)
		(property "Part Type" "Ceramic"
			(at 127 45.72 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 129.54 48.2599 0)
		)
		(property "Status" "Testo PoE"
			(at 127 45.72 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 127 45.72 0)
		)
		(property "Priority" ""
			(at 127 45.72 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C11")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+3.3V")
		(at 236.22 105.41 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR042"
			(at 240.03 105.41 0)
		)
		(property "Value" "+3.3V"
			(at 230.378 105.41 90)
		)
		(property "Footprint" ""
			(at 236.22 105.41 0)
		)
		(property "Datasheet" ""
			(at 236.22 105.41 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 236.22 105.41 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR042")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 165.1 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "TP6"
			(at 167.64 87.6299 0)
		)
		(property "Value" "5V"
			(at 167.64 90.1699 0)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 162.56 93.98 0)
		)
		(property "Datasheet" ""
			(at 165.1 88.9 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 165.1 88.9 0)
		)
		(property "Manufacturer" ""
			(at 165.1 88.9 0)
		)
		(property "MPN" ""
			(at 165.1 88.9 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 165.1 88.9 0)
		)
		(property "Part Type" "Test Point"
			(at 165.1 88.9 0)
		)
		(property "Rating" ""
			(at 165.1 88.9 0)
		)
		(property "Status" ""
			(at 165.1 88.9 0)
		)
		(property "Temperature" ""
			(at 165.1 88.9 0)
		)
		(property "Priority" ""
			(at 165.1 88.9 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP6")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010041")
		(at 137.16 95.25 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R8"
			(at 138.43 92.7099 90)
		)
		(property "Value" "49.9R"
			(at 138.43 95.2499 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 137.16 95.25 0)
		)
		(property "Datasheet" ""
			(at 137.16 95.25 0)
		)
		(property "Description" "SMD RES 49.9R-1%-1/16W;0402"
			(at 137.16 95.25 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 137.16 95.25 0)
		)
		(property "MPN" "RC0402FR-0749R9L"
			(at 137.16 95.25 0)
		)
		(property "SKU" "301010041"
			(at 137.16 95.25 0)
		)
		(property "Resistance" "49.9R"
			(at 137.16 95.25 0)
		)
		(property "Tolerance" ""
			(at 137.16 95.25 0)
		)
		(property "Part Type" "RES"
			(at 137.16 95.25 0)
		)
		(property "Power Rating" "1%"
			(at 138.43 97.7899 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 137.16 95.25 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 137.16 95.25 0)
		)
		(property "Priority" ""
			(at 137.16 95.25 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R8")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Connector/320020216")
		(at 262.89 107.95 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(property "Reference" "J4"
			(at 266.7 107.188 0)
		)
		(property "Value" "Header 1x7 2.54mm"
			(at 266.7 109.2199 0)
		)
		(property "Footprint" "Connector:H7-2.54"
			(at 262.89 107.95 0)
		)
		(property "Datasheet" ""
			(at 262.89 107.95 0)
		)
		(property "Description" "DIP Black Male Header VERT;1*7P-2.54-2.54-11.6/3.0mm"
			(at 262.89 107.95 0)
		)
		(property "Manufacturer" ""
			(at 262.89 107.95 0)
		)
		(property "MPN" ""
			(at 262.89 107.95 0)
		)
		(property "SKU" "320020216"
			(at 262.89 107.95 0)
		)
		(property "Part Type" "Header"
			(at 262.89 107.95 0)
		)
		(property "Rating" ""
			(at 262.89 107.95 0)
		)
		(property "Status" "Grove AI HAT for Edge Computing"
			(at 262.89 107.95 0)
		)
		(property "Temperature" ""
			(at 262.89 107.95 0)
		)
		(property "Priority" ""
			(at 262.89 107.95 0)
		)
		(pin "3")
		(pin "4")
		(pin "1")
		(pin "7")
		(pin "6")
		(pin "2")
		(pin "5")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "J4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 151.13 121.92 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "TP4"
			(at 153.67 120.6499 0)
		)
		(property "Value" "GND"
			(at 153.67 123.1899 0)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 148.59 127 0)
		)
		(property "Datasheet" ""
			(at 151.13 121.92 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 151.13 121.92 0)
		)
		(property "Manufacturer" ""
			(at 151.13 121.92 0)
		)
		(property "MPN" ""
			(at 151.13 121.92 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 151.13 121.92 0)
		)
		(property "Part Type" "Test Point"
			(at 151.13 121.92 0)
		)
		(property "Rating" ""
			(at 151.13 121.92 0)
		)
		(property "Status" ""
			(at 151.13 121.92 0)
		)
		(property "Temperature" ""
			(at 151.13 121.92 0)
		)
		(property "Priority" ""
			(at 151.13 121.92 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 226.06 59.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR027"
			(at 226.06 66.04 0)
		)
		(property "Value" "GND"
			(at 226.06 63.754 0)
		)
		(property "Footprint" ""
			(at 226.06 59.69 0)
		)
		(property "Datasheet" ""
			(at 226.06 59.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 226.06 59.69 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR027")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 22.86 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 22.86 102.87 0)
		)
		(property "Value" "GND"
			(at 22.86 101.6 0)
		)
		(property "Footprint" ""
			(at 22.86 96.52 0)
		)
		(property "Datasheet" ""
			(at 22.86 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 22.86 96.52 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 161.29 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR026"
			(at 161.29 87.63 0)
		)
		(property "Value" "+5V"
			(at 161.29 78.74 0)
		)
		(property "Footprint" ""
			(at 161.29 83.82 0)
		)
		(property "Datasheet" ""
			(at 161.29 83.82 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 161.29 83.82 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR026")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Switch/311030001")
		(at 179.07 40.64 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 180.6448 34.29 0)
		)
		(property "Value" "MK-12C02 G1.5"
			(at 180.6448 36.83 0)
		)
		(property "Footprint" "Switch:SW7-SMD-L6.7X2.7X3.2MM"
			(at 179.07 40.64 0)
		)
		(property "Datasheet" ""
			(at 179.07 40.64 0)
		)
		(property "Description" "SMD TopToggle Switch SPDT;7P-L6.7*W2.7*H3.2mm"
			(at 179.07 40.64 0)
		)
		(property "Manufacturer" "DeYiLong"
			(at 179.07 40.64 0)
		)
		(property "MPN" "MK-12C02 G1.5"
			(at 179.07 40.64 0)
		)
		(property "SKU" "311030001"
			(at 179.07 40.64 0)
		)
		(property "Part Type" "Switch"
			(at 179.07 40.64 0)
		)
		(property "Rating" ""
			(at 179.07 40.64 0)
		)
		(property "Status" "HA Voice KIT"
			(at 179.07 40.64 0)
		)
		(property "Temperature" ""
			(at 179.07 40.64 0)
		)
		(property "Priority" ""
			(at 179.07 40.64 0)
		)
		(pin "P3")
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "P4")
		(pin "P1")
		(pin "P2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Connector/320020216")
		(at 262.89 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "J3"
			(at 266.7 80.0099 0)
		)
		(property "Value" "Header 1x7 2.54mm"
			(at 266.7 82.5499 0)
		)
		(property "Footprint" "Connector:H7-2.54"
			(at 262.89 81.28 0)
		)
		(property "Datasheet" ""
			(at 262.89 81.28 0)
		)
		(property "Description" "DIP Black Male Header VERT;1*7P-2.54-2.54-11.6/3.0mm"
			(at 262.89 81.28 0)
		)
		(property "Manufacturer" ""
			(at 262.89 81.28 0)
		)
		(property "MPN" ""
			(at 262.89 81.28 0)
		)
		(property "SKU" "320020216"
			(at 262.89 81.28 0)
		)
		(property "Part Type" "Header"
			(at 262.89 81.28 0)
		)
		(property "Rating" ""
			(at 262.89 81.28 0)
		)
		(property "Status" "Grove AI HAT for Edge Computing"
			(at 262.89 81.28 0)
		)
		(property "Temperature" ""
			(at 262.89 81.28 0)
		)
		(property "Priority" ""
			(at 262.89 81.28 0)
		)
		(pin "3")
		(pin "4")
		(pin "1")
		(pin "7")
		(pin "6")
		(pin "2")
		(pin "5")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "J3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010005")
		(at 212.09 48.26 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R16"
			(at 213.36 45.7199 90)
		)
		(property "Value" "47K"
			(at 213.36 48.2599 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 212.09 48.26 0)
		)
		(property "Datasheet" ""
			(at 212.09 48.26 0)
		)
		(property "Description" "SMD RES 47K-5%-1/16W;0402"
			(at 212.09 48.26 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 212.09 48.26 0)
		)
		(property "MPN" "RC0402JR-0747KL"
			(at 212.09 48.26 0)
		)
		(property "SKU" "301010005"
			(at 212.09 48.26 0)
		)
		(property "Resistance" "47K"
			(at 212.09 48.26 0)
		)
		(property "Tolerance" ""
			(at 212.09 48.26 0)
		)
		(property "Part Type" "RES"
			(at 212.09 48.26 0)
		)
		(property "Power Rating" "5%"
			(at 213.36 50.7999 90)
		)
		(property "Status" "reSpeaker"
			(at 212.09 48.26 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 212.09 48.26 0)
		)
		(property "Priority" ""
			(at 212.09 48.26 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R16")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R16")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 104.14 168.91 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR046"
			(at 110.49 168.91 0)
		)
		(property "Value" "GND"
			(at 108.966 168.656 90)
		)
		(property "Footprint" ""
			(at 104.14 168.91 0)
		)
		(property "Datasheet" ""
			(at 104.14 168.91 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 104.14 168.91 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR046")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR046")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304050312")
		(at 198.12 88.9 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D7"
			(at 200.914 86.868 90)
		)
		(property "Value" "TPD1E10B06DPYR"
			(at 200.914 89.408 90)
		)
		(property "Footprint" "Diode:ESD-0402"
			(at 198.12 88.9 0)
		)
		(property "Datasheet" ""
			(at 198.12 88.9 0)
		)
		(property "Description" "SMD Diode ESD 5.5V-6V-12pF-30KV-30KV;X1SON(2)"
			(at 198.12 88.9 0)
		)
		(property "Manufacturer" "TI"
			(at 198.12 88.9 0)
		)
		(property "MPN" "TPD1E10B06DPYR"
			(at 198.12 88.9 0)
		)
		(property "SKU" "304050312"
			(at 198.12 88.9 0)
		)
		(property "Part Type" "ESD"
			(at 198.12 88.9 0)
		)
		(property "Rating" "5.5V"
			(at 200.914 91.948 90)
		)
		(property "Status" ""
			(at 198.12 88.9 0)
		)
		(property "Temperature" "-40°C to 125°C"
			(at 198.12 88.9 0)
		)
		(property "Priority" ""
			(at 198.12 88.9 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D7")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 212.09 59.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR041"
			(at 212.09 66.04 0)
		)
		(property "Value" "GND"
			(at 212.09 63.754 0)
		)
		(property "Footprint" ""
			(at 212.09 59.69 0)
		)
		(property "Datasheet" ""
			(at 212.09 59.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 212.09 59.69 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR041")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 54.61 171.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 54.61 177.8 0)
		)
		(property "Value" "GND"
			(at 54.61 176.53 0)
		)
		(property "Footprint" ""
			(at 54.61 171.45 0)
		)
		(property "Datasheet" ""
			(at 54.61 171.45 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 54.61 171.45 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 22.86 53.34 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR019"
			(at 22.86 59.69 0)
		)
		(property "Value" "GND"
			(at 22.86 57.404 0)
		)
		(property "Footprint" ""
			(at 22.86 53.34 0)
		)
		(property "Datasheet" ""
			(at 22.86 53.34 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 22.86 53.34 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR019")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR019")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010010")
		(at 54.61 144.78 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R4"
			(at 55.88 142.2399 90)
		)
		(property "Value" "4.7K"
			(at 55.88 144.7799 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 54.61 144.78 0)
		)
		(property "Datasheet" ""
			(at 54.61 144.78 0)
		)
		(property "Description" "SMD RES 4.7K-5%-1/16W;0402"
			(at 54.61 144.78 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 54.61 144.78 0)
		)
		(property "MPN" "RC0402JR-074K7L"
			(at 54.61 144.78 0)
		)
		(property "SKU" "301010010"
			(at 54.61 144.78 0)
		)
		(property "Resistance" "4.7K"
			(at 54.61 144.78 0)
		)
		(property "Tolerance" ""
			(at 54.61 144.78 0)
		)
		(property "Part Type" "RES"
			(at 54.61 144.78 0)
		)
		(property "Power Rating" "5%"
			(at 55.88 147.3199 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 54.61 144.78 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 54.61 144.78 0)
		)
		(property "Priority" ""
			(at 54.61 144.78 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302013260")
		(at 45.72 44.45 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C3"
			(at 48.26 41.9099 0)
		)
		(property "Value" "22uF"
			(at 48.26 44.4499 0)
		)
		(property "Footprint" "Capacitor:C0805"
			(at 45.72 44.45 0)
		)
		(property "Datasheet" ""
			(at 45.72 44.45 0)
		)
		(property "Description" "SMD CAP Ceramic 22uF-25V-20%-X5R;0805"
			(at 45.72 44.45 0)
		)
		(property "Manufacturer" "Samsung"
			(at 45.72 44.45 0)
		)
		(property "MPN" "CL21A226MAYNNNE"
			(at 45.72 44.45 0)
		)
		(property "SKU" "302013260"
			(at 45.72 44.45 0)
		)
		(property "Dielectric" ""
			(at 45.72 44.45 0)
		)
		(property "Part Type" "Ceramic"
			(at 45.72 44.45 0)
		)
		(property "Voltage Rating" "25V,X5R"
			(at 48.26 46.9899 0)
		)
		(property "Status" ""
			(at 45.72 44.45 0)
		)
		(property "Temperature" "-55°C to 85°C"
			(at 45.72 44.45 0)
		)
		(property "Priority" ""
			(at 45.72 44.45 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Switch/311030001")
		(at 97.79 171.45 90)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW2"
			(at 91.694 168.91 90)
		)
		(property "Value" "MK-12C02 G1.5"
			(at 86.614 171.45 90)
		)
		(property "Footprint" "Switch:SW7-SMD-L6.7X2.7X3.2MM"
			(at 97.79 171.45 0)
		)
		(property "Datasheet" ""
			(at 97.79 171.45 0)
		)
		(property "Description" "SMD TopToggle Switch SPDT;7P-L6.7*W2.7*H3.2mm"
			(at 97.79 171.45 0)
		)
		(property "Manufacturer" "DeYiLong"
			(at 97.79 171.45 0)
		)
		(property "MPN" "MK-12C02 G1.5"
			(at 97.79 171.45 0)
		)
		(property "SKU" "311030001"
			(at 97.79 171.45 0)
		)
		(property "Part Type" "Switch"
			(at 97.79 171.45 0)
		)
		(property "Rating" ""
			(at 97.79 171.45 0)
		)
		(property "Status" "HA Voice KIT"
			(at 97.79 171.45 0)
		)
		(property "Temperature" ""
			(at 97.79 171.45 0)
		)
		(property "Priority" ""
			(at 97.79 171.45 0)
		)
		(pin "2")
		(pin "P2")
		(pin "P3")
		(pin "P1")
		(pin "1")
		(pin "P4")
		(pin "3")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Ic/310031254")
		(at 67.31 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 67.31 76.2 0)
		)
		(property "Value" "TPS54302"
			(at 67.31 78.74 0)
		)
		(property "Footprint" "Ic:SOT23-6"
			(at 72.39 83.82 0)
		)
		(property "Datasheet" ""
			(at 72.39 83.82 0)
		)
		(property "Description" "SMD IC PMIC;SOT23-6"
			(at 67.31 88.9 0)
		)
		(property "Manufacturer" "TI"
			(at 67.31 88.9 0)
		)
		(property "MPN" "TPS54302"
			(at 67.31 88.9 0)
		)
		(property "SKU" "310031254"
			(at 67.31 88.9 0)
		)
		(property "Part Type" ""
			(at 67.31 88.9 0)
		)
		(property "Rating" ""
			(at 67.31 88.9 0)
		)
		(property "Status" ""
			(at 67.31 88.9 0)
		)
		(property "Temperature" ""
			(at 67.31 88.9 0)
		)
		(property "Priority" ""
			(at 67.31 88.9 0)
		)
		(pin "2")
		(pin "6")
		(pin "5")
		(pin "4")
		(pin "1")
		(pin "3")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "U1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304011053")
		(at 102.87 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D2"
			(at 102.235 29.21 0)
		)
		(property "Value" "B5819WS SL"
			(at 102.235 31.75 0)
		)
		(property "Footprint" "Diode:SOD-323"
			(at 102.87 38.1 0)
		)
		(property "Datasheet" ""
			(at 102.87 38.1 0)
		)
		(property "Description" "SMD Diode Schottky 40V-1A;SOD-323"
			(at 102.87 38.1 0)
		)
		(property "Manufacturer" "CJ"
			(at 102.87 38.1 0)
		)
		(property "MPN" "B5819WS SL"
			(at 102.87 38.1 0)
		)
		(property "SKU" "304011053"
			(at 102.87 38.1 0)
		)
		(property "Part Type" "Schottky Diode"
			(at 102.87 38.1 0)
		)
		(property "Rating" "40V"
			(at 102.235 34.29 0)
		)
		(property "Status" "reTerminal DM"
			(at 102.87 38.1 0)
		)
		(property "Temperature" ""
			(at 102.87 38.1 0)
		)
		(property "Priority" ""
			(at 102.87 38.1 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010456")
		(at 137.16 105.41 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R9"
			(at 138.43 102.8699 90)
		)
		(property "Value" "100K"
			(at 138.43 105.4099 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 137.16 105.41 0)
		)
		(property "Datasheet" ""
			(at 137.16 105.41 0)
		)
		(property "Description" "SMD RES 100K-1%-1/16W;0402"
			(at 137.16 105.41 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 137.16 105.41 0)
		)
		(property "MPN" "RC0402FR-07100KL"
			(at 137.16 105.41 0)
		)
		(property "SKU" "301010456"
			(at 137.16 105.41 0)
		)
		(property "Resistance" "100K"
			(at 137.16 105.41 0)
		)
		(property "Tolerance" ""
			(at 137.16 105.41 0)
		)
		(property "Part Type" "RES"
			(at 137.16 105.41 0)
		)
		(property "Power Rating" "1%"
			(at 138.43 107.9499 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 137.16 105.41 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 137.16 105.41 0)
		)
		(property "Priority" ""
			(at 137.16 105.41 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R9")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 30.48 142.24 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TP1"
			(at 32.512 141.732 90)
		)
		(property "Value" "RS485_RX"
			(at 32.258 143.764 90)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 35.56 144.78 0)
		)
		(property "Datasheet" ""
			(at 30.48 142.24 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 30.48 142.24 0)
		)
		(property "Manufacturer" ""
			(at 30.48 142.24 0)
		)
		(property "MPN" ""
			(at 30.48 142.24 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 30.48 142.24 0)
		)
		(property "Part Type" "Test Point"
			(at 30.48 142.24 0)
		)
		(property "Rating" ""
			(at 30.48 142.24 0)
		)
		(property "Status" ""
			(at 30.48 142.24 0)
		)
		(property "Temperature" ""
			(at 30.48 142.24 0)
		)
		(property "Priority" ""
			(at 30.48 142.24 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010005")
		(at 254 55.88 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R15"
			(at 255.27 53.3399 90)
		)
		(property "Value" "47K"
			(at 255.27 55.8799 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 254 55.88 0)
		)
		(property "Datasheet" ""
			(at 254 55.88 0)
		)
		(property "Description" "SMD RES 47K-5%-1/16W;0402"
			(at 254 55.88 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 254 55.88 0)
		)
		(property "MPN" "RC0402JR-0747KL"
			(at 254 55.88 0)
		)
		(property "SKU" "301010005"
			(at 254 55.88 0)
		)
		(property "Resistance" "47K"
			(at 254 55.88 0)
		)
		(property "Tolerance" ""
			(at 254 55.88 0)
		)
		(property "Part Type" "RES"
			(at 254 55.88 0)
		)
		(property "Power Rating" "5%"
			(at 255.27 58.4199 90)
		)
		(property "Status" "reSpeaker"
			(at 254 55.88 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 254 55.88 0)
		)
		(property "Priority" ""
			(at 254 55.88 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R15")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R15")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 275.59 130.81 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR038"
			(at 281.94 130.81 0)
		)
		(property "Value" "GND"
			(at 278.638 130.81 90)
		)
		(property "Footprint" ""
			(at 275.59 130.81 0)
		)
		(property "Datasheet" ""
			(at 275.59 130.81 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 275.59 130.81 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR038")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR038")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010444")
		(at 129.54 176.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R14"
			(at 125.476 173.99 0)
		)
		(property "Value" "10R"
			(at 129.54 173.99 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 129.54 176.53 0)
		)
		(property "Datasheet" ""
			(at 129.54 176.53 0)
		)
		(property "Description" "SMD RES 10R-1%-1/16W;0402"
			(at 129.54 176.53 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 129.54 176.53 0)
		)
		(property "MPN" "RC0402FR-0710RL"
			(at 129.54 176.53 0)
		)
		(property "SKU" "301010444"
			(at 129.54 176.53 0)
		)
		(property "Resistance" "10R"
			(at 129.54 176.53 0)
		)
		(property "Tolerance" ""
			(at 129.54 176.53 0)
		)
		(property "Part Type" "RES"
			(at 129.54 176.53 0)
		)
		(property "Power Rating" "1%"
			(at 133.604 173.99 0)
		)
		(property "Status" "IOT Enabling Dongle Board"
			(at 129.54 176.53 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 129.54 176.53 0)
		)
		(property "Priority" ""
			(at 129.54 176.53 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R14")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R14")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 198.12 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR039"
			(at 198.12 100.33 0)
		)
		(property "Value" "GND"
			(at 198.12 97.79 0)
		)
		(property "Footprint" ""
			(at 198.12 93.98 0)
		)
		(property "Datasheet" ""
			(at 198.12 93.98 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 198.12 93.98 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR039")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR039")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+12V")
		(at 22.86 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 22.86 85.09 0)
		)
		(property "Value" "+12V"
			(at 22.86 76.2 0)
		)
		(property "Footprint" ""
			(at 22.86 81.28 0)
		)
		(property "Datasheet" ""
			(at 22.86 81.28 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+12V\""
			(at 22.86 81.28 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 137.16 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR016"
			(at 137.16 129.54 0)
		)
		(property "Value" "GND"
			(at 137.16 127 0)
		)
		(property "Footprint" ""
			(at 137.16 123.19 0)
		)
		(property "Datasheet" ""
			(at 137.16 123.19 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 137.16 123.19 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR016")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302011019")
		(at 147.32 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C7"
			(at 149.86 102.8699 0)
		)
		(property "Value" "75pF"
			(at 149.86 105.4099 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 147.32 105.41 0)
		)
		(property "Datasheet" ""
			(at 147.32 105.41 0)
		)
		(property "Description" "SMD CAP Ceramic 75pF-50V-5%-NPO;0402"
			(at 147.32 105.41 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 147.32 105.41 0)
		)
		(property "MPN" "CC0402JRNPO9BN750"
			(at 147.32 105.41 0)
		)
		(property "SKU" "302011019"
			(at 147.32 105.41 0)
		)
		(property "Dielectric" ""
			(at 147.32 105.41 0)
		)
		(property "Part Type" "Ceramic"
			(at 147.32 105.41 0)
		)
		(property "Voltage Rating" "50V,NP0"
			(at 149.86 107.9499 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 147.32 105.41 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 147.32 105.41 0)
		)
		(property "Priority" ""
			(at 147.32 105.41 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C7")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 161.29 165.1 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR024"
			(at 167.64 165.1 0)
		)
		(property "Value" "GND"
			(at 165.1 165.0999 90)
		)
		(property "Footprint" ""
			(at 161.29 165.1 0)
		)
		(property "Datasheet" ""
			(at 161.29 165.1 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 161.29 165.1 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR024")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR024")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 124.46 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR025"
			(at 124.46 107.95 0)
		)
		(property "Value" "GND"
			(at 124.46 106.68 0)
		)
		(property "Footprint" ""
			(at 124.46 101.6 0)
		)
		(property "Datasheet" ""
			(at 124.46 101.6 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 124.46 101.6 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR025")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR025")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010034")
		(at 46.99 151.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 43.18 148.59 0)
		)
		(property "Value" "33R"
			(at 46.99 148.59 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 46.99 151.13 0)
		)
		(property "Datasheet" ""
			(at 46.99 151.13 0)
		)
		(property "Description" "SMD RES 33R-5%-1/16W;0402"
			(at 46.99 151.13 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 46.99 151.13 0)
		)
		(property "MPN" "RC0402JR-0733RL"
			(at 46.99 151.13 0)
		)
		(property "SKU" "301010034"
			(at 46.99 151.13 0)
		)
		(property "Resistance" "33R"
			(at 46.99 151.13 0)
		)
		(property "Tolerance" ""
			(at 46.99 151.13 0)
		)
		(property "Part Type" "RES"
			(at 46.99 151.13 0)
		)
		(property "Power Rating" "5%"
			(at 50.8 148.59 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 46.99 151.13 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 46.99 151.13 0)
		)
		(property "Priority" ""
			(at 46.99 151.13 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 40.64 96.52 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 40.64 102.87 0)
		)
		(property "Value" "GND"
			(at 40.64 101.6 0)
		)
		(property "Footprint" ""
			(at 40.64 96.52 0)
		)
		(property "Datasheet" ""
			(at 40.64 96.52 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 40.64 96.52 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Transistor/305050111")
		(at 233.68 43.18 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q2"
			(at 242.824 40.64 0)
		)
		(property "Value" "BC856S"
			(at 242.824 42.672 0)
		)
		(property "Footprint" "Transistor:SOT-363"
			(at 238.76 43.18 0)
		)
		(property "Datasheet" ""
			(at 238.76 43.18 0)
		)
		(property "Description" "SMD Transistor Array 2 PNP -65V-100mA"
			(at 238.76 43.18 0)
		)
		(property "Manufacturer" "CJ"
			(at 233.68 43.18 0)
		)
		(property "MPN" "BC856S"
			(at 233.68 43.18 0)
		)
		(property "SKU" "305050111"
			(at 233.68 43.18 0)
		)
		(property "Part Type" "PNP"
			(at 233.68 43.18 0)
		)
		(property "Rating" "65V-100mA"
			(at 242.824 44.704 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 233.68 43.18 0)
		)
		(property "Temperature" ""
			(at 233.68 43.18 0)
		)
		(property "Priority" ""
			(at 233.68 43.18 0)
		)
		(pin "3")
		(pin "6")
		(pin "2")
		(pin "4")
		(pin "5")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 251.46 26.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR029"
			(at 251.46 30.48 0)
		)
		(property "Value" "EXD_+5V"
			(at 251.46 21.59 0)
		)
		(property "Footprint" ""
			(at 251.46 26.67 0)
		)
		(property "Datasheet" ""
			(at 251.46 26.67 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 251.46 26.67 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR029")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR029")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 181.61 46.99 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR047"
			(at 181.61 53.34 0)
		)
		(property "Value" "GND"
			(at 181.61 51.054 0)
		)
		(property "Footprint" ""
			(at 181.61 46.99 0)
		)
		(property "Datasheet" ""
			(at 181.61 46.99 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 181.61 46.99 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR047")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR047")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 127 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR045"
			(at 127 58.42 0)
		)
		(property "Value" "GND"
			(at 127 57.15 0)
		)
		(property "Footprint" ""
			(at 127 52.07 0)
		)
		(property "Datasheet" ""
			(at 127 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 127 52.07 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR045")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR045")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 111.76 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR020"
			(at 111.76 58.42 0)
		)
		(property "Value" "GND"
			(at 111.76 57.15 0)
		)
		(property "Footprint" ""
			(at 111.76 52.07 0)
		)
		(property "Datasheet" ""
			(at 111.76 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 111.76 52.07 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR020")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR020")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Diode/304040144")
		(at 22.86 44.45 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D5"
			(at 26.67 42.2274 90)
		)
		(property "Value" "SMBJ15CATR7"
			(at 26.67 44.7674 90)
		)
		(property "Footprint" "Diode:DO-214AA_SMB"
			(at 26.67 45.085 0)
		)
		(property "Datasheet" ""
			(at 22.86 44.45 0)
		)
		(property "Description" "SMD Diode TVS 15V-600W"
			(at 22.86 44.45 0)
		)
		(property "Manufacturer" "Brightking"
			(at 22.86 44.45 0)
		)
		(property "MPN" "SMBJ15CATR7"
			(at 22.86 44.45 0)
		)
		(property "SKU" "304040144"
			(at 22.86 44.45 0)
		)
		(property "Part Type" "Diode"
			(at 22.86 44.45 0)
		)
		(property "Rating" "15V-600W"
			(at 26.67 47.3074 90)
		)
		(property "Status" "SenseCAP A1102"
			(at 22.86 44.45 0)
		)
		(property "Temperature" "-55℃ to 150℃"
			(at 22.86 44.45 0)
		)
		(property "Priority" ""
			(at 22.86 44.45 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "D5")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "D5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010034")
		(at 203.2 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R17"
			(at 199.136 81.788 0)
		)
		(property "Value" "33R"
			(at 203.454 81.788 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 203.2 83.82 0)
		)
		(property "Datasheet" ""
			(at 203.2 83.82 0)
		)
		(property "Description" "SMD RES 33R-5%-1/16W;0402"
			(at 203.2 83.82 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 203.2 83.82 0)
		)
		(property "MPN" "RC0402JR-0733RL"
			(at 203.2 83.82 0)
		)
		(property "SKU" "301010034"
			(at 203.2 83.82 0)
		)
		(property "Resistance" "33R"
			(at 203.2 83.82 0)
		)
		(property "Tolerance" ""
			(at 203.2 83.82 0)
		)
		(property "Part Type" "RES"
			(at 203.2 83.82 0)
		)
		(property "Power Rating" "5%"
			(at 207.264 81.788 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 203.2 83.82 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 203.2 83.82 0)
		)
		(property "Priority" ""
			(at 203.2 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R17")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R17")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010444")
		(at 129.54 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R13"
			(at 125.476 151.13 0)
		)
		(property "Value" "10R"
			(at 129.54 151.13 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 129.54 153.67 0)
		)
		(property "Datasheet" ""
			(at 129.54 153.67 0)
		)
		(property "Description" "SMD RES 10R-1%-1/16W;0402"
			(at 129.54 153.67 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 129.54 153.67 0)
		)
		(property "MPN" "RC0402FR-0710RL"
			(at 129.54 153.67 0)
		)
		(property "SKU" "301010444"
			(at 129.54 153.67 0)
		)
		(property "Resistance" "10R"
			(at 129.54 153.67 0)
		)
		(property "Tolerance" ""
			(at 129.54 153.67 0)
		)
		(property "Part Type" "RES"
			(at 129.54 153.67 0)
		)
		(property "Power Rating" "1%"
			(at 133.604 151.13 0)
		)
		(property "Status" "IOT Enabling Dongle Board"
			(at 129.54 153.67 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 129.54 153.67 0)
		)
		(property "Priority" ""
			(at 129.54 153.67 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R13")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Misc/TP35C_SMD")
		(at 271.78 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "TP13"
			(at 274.32 137.16 0)
		)
		(property "Value" "3V3"
			(at 274.066 139.192 0)
		)
		(property "Footprint" "Misc:TP-D35MIL"
			(at 269.24 143.51 0)
		)
		(property "Datasheet" ""
			(at 271.78 138.43 0)
		)
		(property "Description" "Test Point;TP35C_SMD"
			(at 271.78 138.43 0)
		)
		(property "Manufacturer" ""
			(at 271.78 138.43 0)
		)
		(property "MPN" ""
			(at 271.78 138.43 0)
		)
		(property "SKU" "TP35C_SMD"
			(at 271.78 138.43 0)
		)
		(property "Part Type" "Test Point"
			(at 271.78 138.43 0)
		)
		(property "Rating" ""
			(at 271.78 138.43 0)
		)
		(property "Status" ""
			(at 271.78 138.43 0)
		)
		(property "Temperature" ""
			(at 271.78 138.43 0)
		)
		(property "Priority" ""
			(at 271.78 138.43 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "TP13")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "TP13")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 236.22 100.33 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR044"
			(at 240.03 100.33 0)
		)
		(property "Value" "+5V"
			(at 233.172 100.33 90)
		)
		(property "Footprint" ""
			(at 236.22 100.33 0)
		)
		(property "Datasheet" ""
			(at 236.22 100.33 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 236.22 100.33 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR044")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR044")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302013260")
		(at 111.76 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C10"
			(at 114.3 92.7099 0)
		)
		(property "Value" "22uF"
			(at 114.3 95.2499 0)
		)
		(property "Footprint" "Capacitor:C0805"
			(at 111.76 95.25 0)
		)
		(property "Datasheet" ""
			(at 111.76 95.25 0)
		)
		(property "Description" "SMD CAP Ceramic 22uF-25V-20%-X5R;0805"
			(at 111.76 95.25 0)
		)
		(property "Manufacturer" "Samsung"
			(at 111.76 95.25 0)
		)
		(property "MPN" "CL21A226MAYNNNE"
			(at 111.76 95.25 0)
		)
		(property "SKU" "302013260"
			(at 111.76 95.25 0)
		)
		(property "Dielectric" ""
			(at 111.76 95.25 0)
		)
		(property "Part Type" "Ceramic"
			(at 111.76 95.25 0)
		)
		(property "Voltage Rating" "25V,X5R"
			(at 114.3 97.7899 0)
		)
		(property "Status" ""
			(at 111.76 95.25 0)
		)
		(property "Temperature" "-55°C to 85°C"
			(at 111.76 95.25 0)
		)
		(property "Priority" ""
			(at 111.76 95.25 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C10")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Connector/320110007")
		(at 189.23 80.01 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 185.42 78.7399 0)
		)
		(property "Value" "3P-3.5"
			(at 185.42 81.2799 0)
		)
		(property "Footprint" "Connector:H3_3d5_11_5x7mm"
			(at 189.23 80.01 0)
		)
		(property "Datasheet" ""
			(at 189.23 80.01 0)
		)
		(property "Description" "DIP Female Screw Terminal-Green;3P-3.5"
			(at 189.23 80.01 0)
		)
		(property "Manufacturer" "SENGER"
			(at 189.23 80.01 0)
		)
		(property "MPN" "GS012S-3.5mm-3P"
			(at 189.23 80.01 0)
		)
		(property "SKU" "320110007"
			(at 189.23 80.01 0)
		)
		(property "Part Type" "Connector"
			(at 189.23 80.01 0)
		)
		(property "Rating" ""
			(at 189.23 80.01 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 189.23 80.01 0)
		)
		(property "Temperature" "-40°C to 105°C"
			(at 189.23 80.01 0)
		)
		(property "Priority" ""
			(at 189.23 80.01 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "J1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010519")
		(at 111.76 45.72 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "C8"
			(at 114.3 43.1799 0)
		)
		(property "Value" "10uF"
			(at 114.3 45.7199 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 111.76 45.72 0)
		)
		(property "Datasheet" ""
			(at 111.76 45.72 0)
		)
		(property "Description" "SMD CAP Ceramic 10uF-10V-20%-X5R;0402"
			(at 111.76 45.72 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 111.76 45.72 0)
		)
		(property "MPN" "CC0402MRX5R6BB106"
			(at 111.76 45.72 0)
		)
		(property "SKU" "302010519"
			(at 111.76 45.72 0)
		)
		(property "Dielectric" ""
			(at 111.76 45.72 0)
		)
		(property "Part Type" "10uF"
			(at 111.76 45.72 0)
		)
		(property "Voltage Rating" "10V,X5R"
			(at 114.3 48.2599 0)
		)
		(property "Status" "XIAO"
			(at 111.76 45.72 0)
		)
		(property "Temperature" "-55°C to 85°C"
			(at 111.76 45.72 0)
		)
		(property "Priority" ""
			(at 111.76 45.72 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C8")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power:+3.3V")
		(at 116.84 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR017"
			(at 116.84 143.51 0)
		)
		(property "Value" "+3.3V"
			(at 116.84 135.89 0)
		)
		(property "Footprint" ""
			(at 116.84 139.7 0)
		)
		(property "Datasheet" ""
			(at 116.84 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3.3V\""
			(at 116.84 139.7 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR017")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 120.65 186.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR018"
			(at 120.65 193.04 0)
		)
		(property "Value" "GND"
			(at 120.904 190.754 0)
		)
		(property "Footprint" ""
			(at 120.65 186.69 0)
		)
		(property "Datasheet" ""
			(at 120.65 186.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 120.65 186.69 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR018")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR018")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 236.22 102.87 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR043"
			(at 229.87 102.87 0)
		)
		(property "Value" "GND"
			(at 233.426 102.87 90)
		)
		(property "Footprint" ""
			(at 236.22 102.87 0)
		)
		(property "Datasheet" ""
			(at 236.22 102.87 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 236.22 102.87 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR043")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR043")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010004")
		(at 120.65 181.61 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R11"
			(at 121.92 179.0699 90)
		)
		(property "Value" "10K"
			(at 121.92 181.6099 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 120.65 181.61 0)
		)
		(property "Datasheet" ""
			(at 120.65 181.61 0)
		)
		(property "Description" "SMD RES 10K-5%-1/16W;0402"
			(at 120.65 181.61 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 120.65 181.61 0)
		)
		(property "MPN" "RC0402JR-0710KL"
			(at 120.65 181.61 0)
		)
		(property "SKU" "301010004"
			(at 120.65 181.61 0)
		)
		(property "Resistance" "10K"
			(at 120.65 181.61 0)
		)
		(property "Tolerance" ""
			(at 120.65 181.61 0)
		)
		(property "Part Type" "RES"
			(at 120.65 181.61 0)
		)
		(property "Power Rating" "5%"
			(at 121.92 184.1499 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 120.65 181.61 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 120.65 181.61 0)
		)
		(property "Priority" ""
			(at 120.65 181.61 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R11")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R11")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010010")
		(at 54.61 165.1 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp yes)
		(fields_autoplaced yes)
		(property "Reference" "R5"
			(at 55.88 162.5599 90)
		)
		(property "Value" "4.7K"
			(at 55.88 165.0999 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 54.61 165.1 0)
		)
		(property "Datasheet" ""
			(at 54.61 165.1 0)
		)
		(property "Description" "SMD RES 4.7K-5%-1/16W;0402"
			(at 54.61 165.1 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 54.61 165.1 0)
		)
		(property "MPN" "RC0402JR-074K7L"
			(at 54.61 165.1 0)
		)
		(property "SKU" "301010010"
			(at 54.61 165.1 0)
		)
		(property "Resistance" "4.7K"
			(at 54.61 165.1 0)
		)
		(property "Tolerance" ""
			(at 54.61 165.1 0)
		)
		(property "Part Type" "RES"
			(at 54.61 165.1 0)
		)
		(property "Power Rating" "5%"
			(at 55.88 167.6399 90)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 54.61 165.1 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 54.61 165.1 0)
		)
		(property "Priority" ""
			(at 54.61 165.1 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R5")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010006")
		(at 200.66 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C4"
			(at 202.438 46.2281 0)
		)
		(property "Value" "10nF"
			(at 202.438 48.514 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 200.66 48.26 0)
		)
		(property "Datasheet" ""
			(at 200.66 48.26 0)
		)
		(property "Description" "SMD CAP Ceramic 10nF-50V-10%-X7R;0402"
			(at 200.66 48.26 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 200.66 48.26 0)
		)
		(property "MPN" "CC0402KRX7R9BB103"
			(at 200.66 48.26 0)
		)
		(property "SKU" "302010006"
			(at 200.66 48.26 0)
		)
		(property "Dielectric" ""
			(at 200.66 48.26 0)
		)
		(property "Part Type" "Ceramic"
			(at 200.66 48.26 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 202.438 51.054 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 200.66 48.26 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 200.66 48.26 0)
		)
		(property "Priority" ""
			(at 200.66 48.26 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C4")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 171.45 24.13 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR034"
			(at 171.45 27.94 0)
		)
		(property "Value" "+5V"
			(at 171.45 19.05 0)
		)
		(property "Footprint" ""
			(at 171.45 24.13 0)
		)
		(property "Datasheet" ""
			(at 171.45 24.13 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 171.45 24.13 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR034")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR034")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 40.64 90.17 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C2"
			(at 43.688 87.63 0)
		)
		(property "Value" "100nF"
			(at 45.466 90.17 0)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 40.64 90.17 0)
		)
		(property "Datasheet" ""
			(at 40.64 90.17 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 40.64 90.17 0)
		)
		(property "Manufacturer" "TDK"
			(at 40.64 90.17 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 40.64 90.17 0)
		)
		(property "SKU" "302010043"
			(at 40.64 90.17 0)
		)
		(property "Dielectric" ""
			(at 40.64 90.17 0)
		)
		(property "Part Type" "Ceramic"
			(at 40.64 90.17 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 46.482 92.71 0)
		)
		(property "Status" "Testo PoE"
			(at 40.64 90.17 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 40.64 90.17 0)
		)
		(property "Priority" ""
			(at 40.64 90.17 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:+5V")
		(at 213.36 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR035"
			(at 213.36 77.47 0)
		)
		(property "Value" "EXD_+5V"
			(at 213.36 68.58 0)
		)
		(property "Footprint" ""
			(at 213.36 73.66 0)
		)
		(property "Datasheet" ""
			(at 213.36 73.66 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 213.36 73.66 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR035")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR035")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 99.06 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR021"
			(at 99.06 107.95 0)
		)
		(property "Value" "GND"
			(at 99.06 106.68 0)
		)
		(property "Footprint" ""
			(at 99.06 101.6 0)
		)
		(property "Datasheet" ""
			(at 99.06 101.6 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 99.06 101.6 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR021")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR021")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 87.63 52.07 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 87.63 58.42 0)
		)
		(property "Value" "GND"
			(at 87.63 57.15 0)
		)
		(property "Footprint" ""
			(at 87.63 52.07 0)
		)
		(property "Datasheet" ""
			(at 87.63 52.07 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 87.63 52.07 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Capacitors/302010043")
		(at 90.17 151.13 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "C6"
			(at 87.63 146.812 90)
		)
		(property "Value" "100nF"
			(at 92.71 146.812 90)
		)
		(property "Footprint" "Capacitor:C0402"
			(at 90.17 151.13 0)
		)
		(property "Datasheet" ""
			(at 90.17 151.13 0)
		)
		(property "Description" "SMD CAP Ceramic 100nF-50V-10%-X7R;0402"
			(at 90.17 151.13 0)
		)
		(property "Manufacturer" "TDK"
			(at 90.17 151.13 0)
		)
		(property "MPN" "C1005X7R1H104K"
			(at 90.17 151.13 0)
		)
		(property "SKU" "302010043"
			(at 90.17 151.13 0)
		)
		(property "Dielectric" ""
			(at 90.17 151.13 0)
		)
		(property "Part Type" "Ceramic"
			(at 90.17 151.13 0)
		)
		(property "Voltage Rating" "50V,X7R"
			(at 90.17 148.844 90)
		)
		(property "Status" "Testo PoE"
			(at 90.17 151.13 0)
		)
		(property "Temperature" "-55°C to 125°C"
			(at 90.17 151.13 0)
		)
		(property "Priority" ""
			(at 90.17 151.13 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "C6")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "C6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010626")
		(at 97.79 160.02 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R7"
			(at 99.06 157.4799 90)
		)
		(property "Value" "120R"
			(at 99.06 160.0199 90)
		)
		(property "Footprint" "Resistor:R0402"
			(at 97.79 160.02 0)
		)
		(property "Datasheet" ""
			(at 97.79 160.02 0)
		)
		(property "Description" "SMD RES;120R-1%-1/16W-0402"
			(at 97.79 160.02 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 97.79 160.02 0)
		)
		(property "MPN" "RC0402FR-07120RL"
			(at 97.79 160.02 0)
		)
		(property "SKU" "301010626"
			(at 97.79 160.02 0)
		)
		(property "Resistance" "120R"
			(at 97.79 160.02 0)
		)
		(property "Tolerance" ""
			(at 97.79 160.02 0)
		)
		(property "Part Type" "RES"
			(at 97.79 160.02 0)
		)
		(property "Power Rating" "1%"
			(at 99.06 162.5599 90)
		)
		(property "Status" "reTerminal DM"
			(at 97.79 160.02 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 97.79 160.02 0)
		)
		(property "Priority" ""
			(at 97.79 160.02 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R7")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Mosfet/305030010")
		(at 212.09 30.48 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "Q1"
			(at 212.09 21.336 90)
		)
		(property "Value" "CJ3407"
			(at 212.09 23.622 90)
		)
		(property "Footprint" "Mosfet:SOT23"
			(at 212.09 30.48 0)
		)
		(property "Datasheet" ""
			(at 212.09 30.48 0)
		)
		(property "Description" "SMD MOSFET P-CH 30V-4.3A;SOT-23"
			(at 212.09 30.48 0)
		)
		(property "Manufacturer" "长电"
			(at 212.09 30.48 0)
		)
		(property "MPN" "CJ3407"
			(at 212.09 30.48 0)
		)
		(property "SKU" "305030010"
			(at 212.09 30.48 0)
		)
		(property "Part Type" "PMOS"
			(at 212.09 30.48 0)
		)
		(property "Rating" "30V;4.3A"
			(at 212.09 25.654 90)
		)
		(property "Status" "Sensor Hub"
			(at 212.09 30.48 0)
		)
		(property "Temperature" "-55°C to 150°C"
			(at 212.09 30.48 0)
		)
		(property "Priority" ""
			(at 212.09 30.48 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Power_Gnd:GND")
		(at 200.66 59.69 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR07"
			(at 200.66 66.04 0)
		)
		(property "Value" "GND"
			(at 200.66 63.754 0)
		)
		(property "Footprint" ""
			(at 200.66 59.69 0)
		)
		(property "Datasheet" ""
			(at 200.66 59.69 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 200.66 59.69 0)
		)
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Ic/310071191")
		(at 71.12 153.67 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 71.12 143.51 0)
		)
		(property "Value" "TP8485E-SR"
			(at 71.12 146.05 0)
		)
		(property "Footprint" "Ic:SOIC8-1.27-5X4MM"
			(at 64.77 158.75 0)
		)
		(property "Datasheet" ""
			(at 64.77 158.75 0)
		)
		(property "Description" "SMD IC Interface RS485/422"
			(at 64.77 158.75 0)
		)
		(property "Manufacturer" "3PEAK"
			(at 71.12 153.67 0)
		)
		(property "MPN" "TP8485E-SR"
			(at 71.12 153.67 0)
		)
		(property "SKU" "310071191"
			(at 71.12 153.67 0)
		)
		(property "Part Type" "IC"
			(at 71.12 153.67 0)
		)
		(property "Rating" ""
			(at 71.12 153.67 0)
		)
		(property "Status" "SenseCAP A1102"
			(at 71.12 153.67 0)
		)
		(property "Temperature" "-40°C to 125°C"
			(at 71.12 153.67 0)
		)
		(property "Priority" ""
			(at 71.12 153.67 0)
		)
		(pin "3")
		(pin "6")
		(pin "8")
		(pin "2")
		(pin "7")
		(pin "1")
		(pin "5")
		(pin "4")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "U2")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Seeed_libdb:Resistors/301010028")
		(at 247.65 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 243.586 47.244 0)
		)
		(property "Value" "100R"
			(at 247.65 47.244 0)
		)
		(property "Footprint" "Resistor:R0402"
			(at 247.65 49.53 0)
		)
		(property "Datasheet" ""
			(at 247.65 49.53 0)
		)
		(property "Description" "SMD RES 100R-5%-1/16W;0402"
			(at 247.65 49.53 0)
		)
		(property "Manufacturer" "YAGEO"
			(at 247.65 49.53 0)
		)
		(property "MPN" "RC0402JR-07100RL"
			(at 247.65 49.53 0)
		)
		(property "SKU" "301010028"
			(at 247.65 49.53 0)
		)
		(property "Resistance" "100R"
			(at 247.65 49.53 0)
		)
		(property "Tolerance" ""
			(at 247.65 49.53 0)
		)
		(property "Part Type" "RES"
			(at 247.65 49.53 0)
		)
		(property "Power Rating" "5%"
			(at 251.714 47.244 0)
		)
		(property "Status" "BeagleBone Carrier Board"
			(at 247.65 49.53 0)
		)
		(property "Temperature" "-55°C to 155°C"
			(at 247.65 49.53 0)
		)
		(property "Priority" ""
			(at 247.65 49.53 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "Seeed Studio XIAO-RS485-Expansion-Board"
				(path
					(reference "R3")
					(unit 1)
				)
			)
			(project "SenseCAP A1102 - RS485 Vision AI Sensor"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)