(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top")
		(31 "B.Cu" signal "Bottom")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Paste Mask Bottom")
		(35 "F.Paste" user "Paste Mask Top")
		(36 "B.SilkS" user "Silkscreen Bottom")
		(37 "F.SilkS" user "Silkscreen Top")
		(38 "B.Mask" user "Solder Mask Bottom")
		(39 "F.Mask" user "Solder Mask Top")
		(40 "Dwgs.User" user "Layer_10")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Layer_11")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Layer_13")
		(49 "F.Fab" user "Layer_12")
		(50 "User.1" user "Assembly Drawing Top")
		(51 "User.2" user "Assembly Drawing Bottom")
		(52 "User.3" user "Layer_3")
		(53 "User.4" user "Layer_4")
		(54 "User.5" user "Layer_5")
		(55 "User.6" user "Layer_6")
		(56 "User.7" user "Layer_7")
		(57 "User.8" user "Layer_8")
		(58 "User.9" user "Layer_9")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin -676.855516 351.783105)
		(grid_origin -676.855516 351.783105)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "WAKEUP_IN")
	(net 2 "VDD_5V")
	(net 3 "SPI_MOSI")
	(net 4 "SPI_MISO")
	(net 5 "SPI_INT")
	(net 6 "SPI_CS")
	(net 7 "SPI_CLK")
	(net 8 "RESET")
	(net 9 "PB09_A7_D7_RX")
	(net 10 "PB08_A6_D6_TX")
	(net 11 "PA9_A5_D5_SCL")
	(net 12 "PA8_A4_D4_SDA")
	(net 13 "PA7_A8_D8_SCK")
	(net 14 "PA6_A10_D10_MOSI")
	(net 15 "PA5_A9_D9_MISO")
	(net 16 "PA4_A1_D1")
	(net 17 "PA11_A3_D3")
	(net 18 "PA10_A2_D2")
	(net 19 "PA02_A0_D0")
	(net 20 "N34312580")
	(net 21 "N34312575")
	(net 22 "N34312570")
	(net 23 "N34312565")
	(net 24 "N34311591")
	(net 25 "N34310667")
	(net 26 "N34310640")
	(net 27 "N34310613")
	(net 28 "N34310586")
	(net 29 "N34310504")
	(net 30 "N34310477")
	(net 31 "N34310055")
	(net 32 "N34310043")
	(net 33 "N34310028")
	(net 34 "MOD_5V")
	(net 35 "MOD_3V3")
	(net 36 "GND")
	(net 37 "BUSY")
	(net 38 "ANT_WIFI_MOD")
	(net 39 "ANT_WIFI")
	(net 40 "3V3")
	(footprint "R0402"
		(layer "F.Cu")
		(at 166.822284 101.922005 135)
		(property "Reference" "R1"
			(at 0 0.18669 135)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.829995 1.478895 135)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.450003 0 135)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 0.450003 0 135)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_WIFI_MOD")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.855084 104.055605)
		(property "Reference" "R24"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "N34310667")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 157.752484 96.216805 180)
		(property "Reference" "R10"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "PA4_A1_D1")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 154.782684 113.148805 -90)
		(property "Reference" "C7"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "FB0603"
		(layer "F.Cu")
		(at 162.453484 96.892805 180)
		(property "Reference" "FB2"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FB0603"
			(at -2.60807 0.513153 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VDD_5V")
		)
		(pad "2" smd rect
			(at 0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_5V")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 166.134484 111.556805)
		(property "Reference" "R5"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "N34312565")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 152.926484 96.623205 -90)
		(property "Reference" "R18"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "N34310477")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.855084 101.109205)
		(property "Reference" "R20"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "N34310586")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.804284 106.443205 180)
		(property "Reference" "R25"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "N34311591")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
	)
	(footprint "CON_U.FL-R-SMT-1"
		(layer "F.Cu")
		(at 167.201254 106.436805 180)
		(property "Reference" "CN1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CON_U.FL-R-SMT-1"
			(at -1.2 2.661106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 1.7 270)
			(size 1.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 1.475 0 270)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "3" smd rect
			(at -1.475 0 270)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 168.109024 106.436805) (xy 168.078094 106.671755) (xy 167.987404 106.890685) (xy 167.843144 107.078695)
					(xy 167.655134 107.222955) (xy 167.436204 107.313645) (xy 167.201254 107.344575) (xy 166.966304 107.313645)
					(xy 166.747374 107.222955) (xy 166.559364 107.078695) (xy 166.415104 106.890685) (xy 166.324414 106.671755)
					(xy 166.293484 106.436805) (xy 166.301254 106.436805) (xy 166.301254 105.136805) (xy 168.101254 105.136805)
					(xy 168.101254 106.436805)
				)
			)
		)
	)
	(footprint "FB0603"
		(layer "F.Cu")
		(at 149.804284 110.659605 -90)
		(property "Reference" "FB1"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FB0603"
			(at -2.60807 0.513153 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7874 0 270)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "3V3")
		)
		(pad "2" smd rect
			(at 0.7874 0 270)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 166.134484 110.591605)
		(property "Reference" "R4"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "N34312570")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.855084 102.074405)
		(property "Reference" "R22"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "N34310613")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 156.713084 113.148805 -90)
		(property "Reference" "R14"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "SPI_CLK")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "PA7_A8_D8_SCK")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 164.688684 96.435605 90)
		(property "Reference" "C3"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "VDD_5V")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 160.015084 113.154805 -90)
		(property "Reference" "R8"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "N34310055")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 162.250284 113.154805 -90)
		(property "Reference" "R6"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34310028")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 157.752484 97.131205 180)
		(property "Reference" "R9"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.855084 103.090405)
		(property "Reference" "R23"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "N34310640")
		)
	)
	(footprint "CN_ESP32S3_XIAO_DIP14"
		(layer "F.Cu")
		(at 130.422084 105.003605 90)
		(property "Reference" "CN2"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CN_ESP32S3_XIAO_DIP14"
			(at -31.44615 3.234723 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -7.61888 -0.75)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 1.79)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 4.33)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 6.87)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 9.41)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 11.95)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61888 14.49)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88112) (xy 1.5 1.88112) (xy 1.50647 0) (xy 1.4807 -0.1958) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.53491) (xy 1.12824 -0.65513) (xy 0.94579 -0.7307) (xy 0.75 -0.75648) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65513) (xy 0.21509 -0.53491) (xy 0.09488 -0.37824) (xy 0.0193 -0.1958) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 -0.75)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 1.79)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 4.33)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 6.87)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 9.41)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 11.95)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -7.61624 14.49)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.88376) (xy 1.5 1.88376) (xy 1.50647 0) (xy 1.4807 -0.19579) (xy 1.40513 -0.37824)
						(xy 1.28491 -0.5349) (xy 1.12824 -0.65512) (xy 0.94579 -0.7307) (xy 0.75 -0.75647) (xy 0.55421 -0.7307)
						(xy 0.37176 -0.65512) (xy 0.21509 -0.5349) (xy 0.09488 -0.37824) (xy 0.0193 -0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 -0.75)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 1.79)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 4.33)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 6.87)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 9.41)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 11.95)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61624 14.49)
			(size 0.000001 0.000001)
			(layers "B.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88376) (xy 1.5 -1.88376) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37824)
						(xy 1.28491 0.53491) (xy 1.12824 0.65512) (xy 0.94579 0.7307) (xy 0.75 0.75647) (xy 0.55421 0.7307)
						(xy 0.37176 0.65512) (xy 0.21509 0.53491) (xy 0.09488 0.37824) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 -0.75)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 1.79)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 4.33)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 6.87)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 9.41)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 11.95)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at 7.61887 14.49)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.88113) (xy 1.5 -1.88113) (xy 1.50647 0) (xy 1.4807 0.19579) (xy 1.40513 0.37823)
						(xy 1.28491 0.5349) (xy 1.12824 0.65512) (xy 0.94579 0.73069) (xy 0.75 0.75647) (xy 0.55421 0.73069)
						(xy 0.37176 0.65512) (xy 0.21509 0.5349) (xy 0.09488 0.37823) (xy 0.0193 0.19579) (xy -0.00647 0)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" thru_hole oval
			(at -7.874 0 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "PA02_A0_D0")
		)
		(pad "2" thru_hole oval
			(at -7.874 2.54 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "PA4_A1_D1")
		)
		(pad "3" thru_hole oval
			(at -7.874 5.08 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "PA10_A2_D2")
		)
		(pad "4" thru_hole oval
			(at -7.874 7.62 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "PA11_A3_D3")
		)
		(pad "5" thru_hole oval
			(at -7.874 10.16 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "PA8_A4_D4_SDA")
		)
		(pad "6" thru_hole oval
			(at -7.874 12.7 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "PA9_A5_D5_SCL")
		)
		(pad "7" thru_hole oval
			(at -7.874 15.24 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "PB08_A6_D6_TX")
		)
		(pad "8" thru_hole oval
			(at 7.874 15.24 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "PB09_A7_D7_RX")
		)
		(pad "9" thru_hole oval
			(at 7.874 12.7 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "PA7_A8_D8_SCK")
		)
		(pad "10" thru_hole oval
			(at 7.874 10.16 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "PA5_A9_D9_MISO")
		)
		(pad "11" thru_hole oval
			(at 7.874 7.62 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "PA6_A10_D10_MOSI")
		)
		(pad "12" thru_hole oval
			(at 7.874 5.08 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "3V3")
		)
		(pad "13" thru_hole oval
			(at 7.874 2.54 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "GND")
		)
		(pad "14" thru_hole oval
			(at 7.874 0 90)
			(size 2.032 1.524)
			(drill oval 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VDD_5V")
		)
	)
	(footprint "HEADER_PIN_SIP7_2MM54"
		(layer "F.Cu")
		(at 145.662084 93.824805 -90)
		(property "Reference" "CN4"
			(at 4.0332 -2.559384 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HEADER_PIN_SIP7_2MM54"
			(at 0.508 -2.070894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "PB09_A7_D7_RX")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "PA7_A8_D8_SCK")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "PA5_A9_D9_MISO")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "PA6_A10_D10_MOSI")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "3V3")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24 270)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VDD_5V")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 157.678284 113.154805 -90)
		(property "Reference" "R12"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SPI_MISO")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "PA5_A9_D9_MISO")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 167.635084 103.395205)
		(property "Reference" "C1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 90)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 0.475 0 90)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 160.319884 96.588005 90)
		(property "Reference" "C6"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 156.076084 96.623205 -90)
		(property "Reference" "R13"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "PA02_A0_D0")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RESET")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 155.060084 96.623205 -90)
		(property "Reference" "R17"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "PA8_A4_D4_SDA")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "BUSY")
		)
	)
	(footprint "FGH100M-H"
		(layer "F.Cu")
		(at 157.775484 104.892605 -90)
		(property "Reference" "UM1"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FGH100M-H"
			(at -4.7 0.257216 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -5.725 -5.85)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy -0.125 -0.125) (xy -0.7 -0.125) (xy -0.7 0.575) (xy 0 0.575)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -4.25 -4.45)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 1.42) (xy -1.62 1.42) (xy -1.62 -0.2) (xy -0.2 -0.2)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -5.5 -5.5 270)
			(size 0.25 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "2" smd rect
			(at -5.5 -4.4 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -5.5 -3.3 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -5.5 -2.2 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_5V")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at -5.5 -1.1 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at -5.5 0 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at -5.5 1.1 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at -5.5 2.2 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RESET")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at -5.5 3.3 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "10" smd rect
			(at -5.5 4.4 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "BUSY")
			(solder_mask_margin 0.05)
		)
		(pad "11" smd rect
			(at -5.5 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "N34310477")
			(solder_mask_margin 0.05)
		)
		(pad "12" smd rect
			(at -4.4 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "N34310504")
			(solder_mask_margin 0.05)
		)
		(pad "13" smd rect
			(at -3.3 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "N34310586")
			(solder_mask_margin 0.05)
		)
		(pad "14" smd rect
			(at -2.2 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "N34310613")
			(solder_mask_margin 0.05)
		)
		(pad "15" smd rect
			(at -1.1 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "N34310640")
			(solder_mask_margin 0.05)
		)
		(pad "16" smd rect
			(at 0 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "N34310667")
			(solder_mask_margin 0.05)
		)
		(pad "17" smd rect
			(at 1.1 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
			(solder_mask_margin 0.05)
		)
		(pad "18" smd rect
			(at 2.2 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "19" smd rect
			(at 3.3 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "N34311591")
			(solder_mask_margin 0.05)
		)
		(pad "20" smd rect
			(at 4.4 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "SPI_CS")
			(solder_mask_margin 0.05)
		)
		(pad "21" smd rect
			(at 5.5 5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "22" smd rect
			(at 5.5 4.4 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
			(solder_mask_margin 0.05)
		)
		(pad "23" smd rect
			(at 5.5 3.3 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "SPI_MOSI")
			(solder_mask_margin 0.05)
		)
		(pad "24" smd rect
			(at 5.5 2.2 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "SPI_CLK")
			(solder_mask_margin 0.05)
		)
		(pad "25" smd rect
			(at 5.5 1.1 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SPI_MISO")
			(solder_mask_margin 0.05)
		)
		(pad "26" smd rect
			(at 5.5 0 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SPI_INT")
			(solder_mask_margin 0.05)
		)
		(pad "27" smd rect
			(at 5.5 -1.1 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "28" smd rect
			(at 5.5 -2.2 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "N34310055")
			(solder_mask_margin 0.05)
		)
		(pad "29" smd rect
			(at 5.5 -3.3 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "N34310043")
			(solder_mask_margin 0.05)
		)
		(pad "30" smd rect
			(at 5.5 -4.4 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34310028")
			(solder_mask_margin 0.05)
		)
		(pad "31" smd rect
			(at 5.5 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "32" smd rect
			(at 4.4 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "N34312565")
			(solder_mask_margin 0.05)
		)
		(pad "33" smd rect
			(at 3.3 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "N34312570")
			(solder_mask_margin 0.05)
		)
		(pad "34" smd rect
			(at 2.2 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "N34312575")
			(solder_mask_margin 0.05)
		)
		(pad "35" smd rect
			(at 1.1 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "36" smd rect
			(at 0 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "N34312580")
			(solder_mask_margin 0.05)
		)
		(pad "37" smd rect
			(at -1.1 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "38" smd rect
			(at -2.2 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "39" smd rect
			(at -3.3 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "40" smd rect
			(at -4.4 -5.5 270)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_WIFI_MOD")
			(solder_mask_margin 0.05)
		)
		(pad "41" smd rect
			(at -3.64 -3.64 270)
			(size 0.25 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "42" smd rect
			(at -1.82 -3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "43" smd rect
			(at 0 -3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "44" smd rect
			(at 1.82 -3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "45" smd rect
			(at 3.64 -3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "46" smd rect
			(at -3.64 -1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "47" smd rect
			(at -1.82 -1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "48" smd rect
			(at 0 -1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "49" smd rect
			(at 1.82 -1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "50" smd rect
			(at 3.64 -1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "51" smd rect
			(at -3.64 0 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "52" smd rect
			(at -1.82 0 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "53" smd rect
			(at 0 0 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "54" smd rect
			(at 1.82 0 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "55" smd rect
			(at 3.64 0 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "56" smd rect
			(at -3.64 1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "57" smd rect
			(at -1.82 1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "58" smd rect
			(at 0 1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "59" smd rect
			(at 1.82 1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "60" smd rect
			(at 3.64 1.82 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "61" smd rect
			(at -3.64 3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "62" smd rect
			(at -1.82 3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "63" smd rect
			(at 0 3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "64" smd rect
			(at 1.82 3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "65" smd rect
			(at 3.64 3.64 270)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 166.158384 109.626405)
		(property "Reference" "R3"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "N34312575")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.804284 107.408405 180)
		(property "Reference" "R21"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "SPI_CS")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "PA11_A3_D3")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 149.855084 108.424405)
		(property "Reference" "C4"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 90)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 90)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 149.855084 100.093205)
		(property "Reference" "R19"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "N34310504")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 166.134484 108.559605)
		(property "Reference" "R2"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "N34312580")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 166.111084 100.550405 45)
		(property "Reference" "C2"
			(at 0 0.18669 45)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.782322 1.50701 45)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475006 0 135)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_WIFI_MOD")
		)
		(pad "2" smd rect
			(at 0.475006 0 135)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "HEADER_PIN_SIP7_2MM54"
		(layer "F.Cu")
		(at 130.422084 116.182405 90)
		(property "Reference" "CN3"
			(at 2.0176 17.850184 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HEADER_PIN_SIP7_2MM54"
			(at 0.508 -1.993106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "PA02_A0_D0")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "PA4_A1_D1")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "PA10_A2_D2")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "PA11_A3_D3")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "PA8_A4_D4_SDA")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "PA9_A5_D5_SCL")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24 90)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "PB08_A6_D6_TX")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 154.094884 96.623205 -90)
		(property "Reference" "R15"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "BUSY")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 153.688484 113.133205 -90)
		(property "Reference" "C8"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 161.132684 113.154805 -90)
		(property "Reference" "R7"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "N34310043")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 158.795884 113.154805 -90)
		(property "Reference" "R11"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SPI_INT")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "PA10_A2_D2")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 155.798684 113.148805 -90)
		(property "Reference" "R16"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "SPI_MOSI")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "PA6_A10_D10_MOSI")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 159.253084 96.588005 90)
		(property "Reference" "C5"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 149.905884 105.071605 180)
		(property "Reference" "C9"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "GND")
		)
	)
	(gr_line
		(start 167.500174 92.503595)
		(end 167.501084 92.503605)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.501084 94.452805)
		(end 127.501084 115.452805)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.501084 115.452805)
		(end 169.501088 94.452799)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 129.501084 117.503605)
		(end 167.501084 117.503605)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 169.501117 115.454095)
		(mid 168.932932 116.900265)
		(end 167.501084 117.503605)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127.50111 94.451894)
		(mid 128.105056 93.071214)
		(end 129.501084 92.503605)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.501084 115.452805)
		(end 127.501051 115.454095)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 167.500174 92.503595)
		(mid 168.896881 93.071441)
		(end 169.501088 94.452799)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.501084 117.503605)
		(mid 128.069259 116.900244)
		(end 127.501051 115.454095)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.501084 92.503605)
		(end 129.501084 92.503605)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.50111 94.451894)
		(end 127.501084 94.452805)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.501117 115.454095)
		(end 169.501084 115.452805)
		(layer "Edge.Cuts")
	)
	(gr_text "D6"
		(at 146.829356 108.899605 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 133.834356 98.711605 90)
		(layer "B.SilkS")
	)
	(gr_text "D0"
		(at 131.511356 108.937605 90)
		(layer "B.SilkS")
	)
	(gr_text "D1"
		(at 133.966356 108.964605 90)
		(layer "B.SilkS")
	)
	(gr_text "D2"
		(at 136.543356 108.932605 90)
		(layer "B.SilkS")
	)
	(gr_text "D10"
		(at 138.962356 98.711605 90)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 136.411356 98.679605 90)
		(layer "B.SilkS")
	)
	(gr_text "D7"
		(at 146.697356 98.646605 90)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 131.379356 98.684605 90)
		(layer "B.SilkS")
	)
	(gr_text "D8"
		(at 144.146356 98.614605 90)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 144.278356 108.867605 90)
		(layer "B.SilkS")
	)
	(gr_text "D4"
		(at 141.701356 108.899605 90)
		(layer "B.SilkS")
	)
	(gr_text "D9"
		(at 141.569356 98.646605 90)
		(layer "B.SilkS")
	)
	(gr_text "D3"
		(at 139.094356 108.964605 90)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 146.624152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "D8"
		(at 144.210152 101.163605 90)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 136.413152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 131.282152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 146.750152 101.061605 90)
		(layer "F.SilkS")
	)
	(gr_text "D9"
		(at 141.518152 101.163605 90)
		(layer "F.SilkS")
	)
	(gr_text "D10"
		(at 138.978152 102.179605 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 131.314152 101.203605 90)
		(layer "F.SilkS")
	)
	(gr_text "D1"
		(at 133.873152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 136.488152 102.026605 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 133.925152 102.867605 90)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 141.493152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 138.800152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "D5"
		(at 144.033152 111.254605 90)
		(layer "F.SilkS")
	)
	(gr_text "Wi-Fi Halow"
		(at 153.215084 95.259317 0)
		(layer "F.SilkS")
	)
	(zone
		(net 36)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 126.104084 91.287605) (xy 126.104084 119.227605) (xy 170.554084 119.227605) (xy 170.554084 91.287605)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 162.781684 101.092005) (xy 164.966084 101.092005) (xy 166.490084 102.616005) (xy 166.490244 105.766015)
				(xy 166.529034 105.859665) (xy 166.647734 106.014365) (xy 166.802424 106.133055) (xy 166.982564 106.207675)
				(xy 167.175884 106.233125) (xy 167.369204 106.207675) (xy 167.549344 106.133055) (xy 167.704044 106.014365)
				(xy 167.822744 105.859665) (xy 167.862024 105.764815) (xy 167.861684 105.765605) (xy 167.861684 101.945405)
				(xy 165.839884 99.923605) (xy 162.780344 99.921695) (xy 162.751384 99.933685) (xy 162.614094 100.039045)
				(xy 162.508734 100.176335) (xy 162.442504 100.336225) (xy 162.419924 100.507805) (xy 162.442504 100.679385)
				(xy 162.508734 100.839275) (xy 162.614094 100.976575) (xy 162.751384 101.081925) (xy 162.781404 101.094355)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.500174 92.567095) (xy 167.46285 92.554968) (xy 167.439782 92.523218) (xy 167.439782 92.483973)
				(xy 167.462849 92.452223) (xy 167.500174 92.440095) (xy 167.765257 92.457178) (xy 168.025955 92.508146)
				(xy 168.277954 92.592157) (xy 168.517084 92.70782) (xy 168.739389 92.853221) (xy 168.94119 93.025955)
				(xy 169.11915 93.223164) (xy 169.270323 93.441586) (xy 169.392209 93.677605) (xy 169.48279 93.927317)
				(xy 169.540567 94.186591) (xy 169.564586 94.451136) (xy 169.564566 94.451136) (xy 169.55342 94.488766)
				(xy 169.522285 94.512657) (xy 169.483053 94.513684) (xy 169.45071 94.491456) (xy 169.43761 94.454462)
				(xy 169.43763 94.454461) (xy 169.434329 94.329599) (xy 169.395787 94.08278) (xy 169.325881 93.842949)
				(xy 169.225769 93.614076) (xy 169.097105 93.399947) (xy 168.94202 93.204105) (xy 168.76308 93.029791)
				(xy 168.563244 92.879888) (xy 168.345819 92.756876) (xy 168.114403 92.662791) (xy 167.872824 92.59919)
				(xy 167.62508 92.567125) (xy 167.500174 92.567095)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.775384 115.444939) (xy 168.80975 115.479305) (xy 168.80975 115.527905) (xy 168.775384 115.562271)
				(xy 168.751084 115.567105) (xy 166.251084 115.567105) (xy 166.226784 115.562271) (xy 166.192418 115.527905)
				(xy 166.192418 115.479305) (xy 166.226784 115.444939) (xy 166.251084 115.440105) (xy 168.751084 115.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.501084 117.440105) (xy 129.538408 117.452232) (xy 129.561476 117.483982) (xy 129.561476 117.523228)
				(xy 129.538408 117.554978) (xy 129.501084 117.567105) (xy 129.227496 117.548893) (xy 128.958736 117.494579)
				(xy 128.699546 117.405121) (xy 128.4545 117.282098) (xy 128.227923 117.12768) (xy 128.023812 116.944593)
				(xy 127.845769 116.736067) (xy 127.696937 116.505782) (xy 127.579941 116.257802) (xy 127.496846 115.996503)
				(xy 127.449119 115.726495) (xy 127.437601 115.452543) (xy 127.43757 115.452543) (xy 127.450606 115.415526)
				(xy 127.482911 115.393241) (xy 127.522144 115.394201) (xy 127.553321 115.418038) (xy 127.564532 115.455647)
				(xy 127.564563 115.455648) (xy 127.561363 115.584558) (xy 127.589287 115.840941) (xy 127.650947 116.09136)
				(xy 127.745255 116.331397) (xy 127.870547 116.556816) (xy 128.024612 116.763639) (xy 128.204731 116.948217)
				(xy 128.407726 117.107292) (xy 128.630014 117.238058) (xy 128.867674 117.338206) (xy 129.116511 117.405969)
				(xy 129.372135 117.440153) (xy 129.501084 117.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.775384 115.444939) (xy 151.80975 115.479305) (xy 151.80975 115.527905) (xy 151.775384 115.562271)
				(xy 151.751084 115.567105) (xy 149.251084 115.567105) (xy 149.226784 115.562271) (xy 149.192418 115.527905)
				(xy 149.192418 115.479305) (xy 149.226784 115.444939) (xy 149.251084 115.440105) (xy 151.751084 115.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.525384 117.444939) (xy 167.55975 117.479305) (xy 167.55975 117.527905) (xy 167.525384 117.562271)
				(xy 167.501084 117.567105) (xy 129.501084 117.567105) (xy 129.476784 117.562271) (xy 129.442418 117.527905)
				(xy 129.442418 117.479305) (xy 129.476784 117.444939) (xy 129.501084 117.440105) (xy 167.501084 117.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.442418 94.428505) (xy 169.476784 94.394139) (xy 169.525384 94.394139) (xy 169.55975 94.428505)
				(xy 169.564584 94.452805) (xy 169.564584 115.452805) (xy 169.55975 115.477105) (xy 169.525384 115.511471)
				(xy 169.476784 115.511471) (xy 169.442418 115.477105) (xy 169.437584 115.452805) (xy 169.437584 94.452805)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.775384 94.444939) (xy 168.80975 94.479305) (xy 168.80975 94.527905) (xy 168.775384 94.562271)
				(xy 168.751084 94.567105) (xy 166.251084 94.567105) (xy 166.226784 94.562271) (xy 166.192418 94.527905)
				(xy 166.192418 94.479305) (xy 166.226784 94.444939) (xy 166.251084 94.440105) (xy 168.751084 94.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.775384 94.444939) (xy 151.80975 94.479305) (xy 151.80975 94.527905) (xy 151.775384 94.562271)
				(xy 151.751084 94.567105) (xy 149.251084 94.567105) (xy 149.226784 94.562271) (xy 149.192418 94.527905)
				(xy 149.192418 94.479305) (xy 149.226784 94.444939) (xy 149.251084 94.440105) (xy 151.751084 94.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.525384 92.444939) (xy 167.55975 92.479305) (xy 167.55975 92.527905) (xy 167.525384 92.562271)
				(xy 167.501084 92.567105) (xy 129.501084 92.567105) (xy 129.476784 92.562271) (xy 129.442418 92.527905)
				(xy 129.442418 92.479305) (xy 129.476784 92.444939) (xy 129.501084 92.440105) (xy 167.501084 92.440105)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.442418 94.428505) (xy 127.476784 94.394139) (xy 127.525384 94.394139) (xy 127.55975 94.428505)
				(xy 127.564584 94.452805) (xy 127.564584 115.452805) (xy 127.55975 115.477105) (xy 127.525384 115.511471)
				(xy 127.476784 115.511471) (xy 127.442418 115.477105) (xy 127.437584 115.452805) (xy 127.437584 94.452805)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.437636 115.455647) (xy 169.448847 115.418038) (xy 169.480024 115.394201) (xy 169.519257 115.393241)
				(xy 169.551562 115.415526) (xy 169.564598 115.452543) (xy 169.564597 115.452543) (xy 169.553079 115.726498)
				(xy 169.505351 115.99651) (xy 169.422255 116.257813) (xy 169.305257 116.505797) (xy 169.156423 116.736085)
				(xy 168.978378 116.944614) (xy 168.774264 117.127704) (xy 168.547683 117.282124) (xy 168.302634 117.405149)
				(xy 168.04344 117.494608) (xy 167.774676 117.548923) (xy 167.501084 117.567135) (xy 167.501084 117.567105)
				(xy 167.46376 117.554978) (xy 167.440692 117.523228) (xy 167.440692 117.483982) (xy 167.46376 117.452232)
				(xy 167.501084 117.440105) (xy 167.501084 117.440135) (xy 167.630035 117.440184) (xy 167.885663 117.406)
				(xy 168.134504 117.338235) (xy 168.372168 117.238085) (xy 168.59446 117.107318) (xy 168.797458 116.94824)
				(xy 168.97758 116.763659) (xy 169.131647 116.556833) (xy 169.256941 116.33141) (xy 169.351251 116.091369)
				(xy 169.412912 115.840946) (xy 169.440836 115.584559) (xy 169.437635 115.455647)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.564588 94.453557) (xy 127.551487 94.490551) (xy 127.519144 94.512779) (xy 127.479912 94.511751)
				(xy 127.448777 94.48786) (xy 127.437632 94.450231) (xy 127.461643 94.185811) (xy 127.519397 93.92666)
				(xy 127.609938 93.677067) (xy 127.731768 93.441161) (xy 127.882871 93.222844) (xy 128.060748 93.025729)
				(xy 128.262455 92.853077) (xy 128.484655 92.707745) (xy 128.723672 92.592137) (xy 128.975551 92.508166)
				(xy 129.236126 92.457221) (xy 129.501084 92.440145) (xy 129.501084 92.440105) (xy 129.538408 92.452232)
				(xy 129.561476 92.483982) (xy 129.561476 92.523228) (xy 129.538408 92.554978) (xy 129.501084 92.567105)
				(xy 129.501084 92.567145) (xy 129.376241 92.567176) (xy 129.128622 92.599226) (xy 128.887165 92.662795)
				(xy 128.655865 92.756832) (xy 128.438549 92.879782) (xy 128.238813 93.029609) (xy 128.059962 93.203835)
				(xy 127.904953 93.399578) (xy 127.776353 93.613598) (xy 127.676289 93.842355) (xy 127.606416 94.082064)
				(xy 127.56789 94.328759) (xy 127.564589 94.453558)
			)
		)
	)
	(zone
		(net 36)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 126.358084 91.541605) (xy 126.358084 118.719605) (xy 170.046084 118.719605) (xy 170.046084 91.541605)
			)
		)
	)
)
