(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top")
		(31 "B.Cu" signal "Bottom")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Paste Mask Bottom")
		(35 "F.Paste" user "Paste Mask Top")
		(36 "B.SilkS" user "Silkscreen Bottom")
		(37 "F.SilkS" user "Silkscreen Top")
		(38 "B.Mask" user "Solder Mask Bottom")
		(39 "F.Mask" user "Solder Mask Top")
		(40 "Dwgs.User" user "Layer_10")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Layer_11")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Layer_13")
		(49 "F.Fab" user "Layer_12")
		(50 "User.1" user "Assembly Drawing Top")
		(51 "User.2" user "Assembly Drawing Bottom")
		(52 "User.3" user "Layer_3")
		(53 "User.4" user "Layer_4")
		(54 "User.5" user "Layer_5")
		(55 "User.6" user "Layer_6")
		(56 "User.7" user "Layer_7")
		(57 "User.8" user "Layer_8")
		(58 "User.9" user "Layer_9")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin -57.8739 337.4536)
		(grid_origin -57.8739 337.4536)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "WAKEUP_IN")
	(net 2 "SPI_MOSI")
	(net 3 "SPI_MISO")
	(net 4 "SPI_INT")
	(net 5 "SPI_CS")
	(net 6 "SPI_CLK")
	(net 7 "RESET")
	(net 8 "PCIE_3V3")
	(net 9 "N33866136")
	(net 10 "N33862302")
	(net 11 "N33846703")
	(net 12 "N33846697")
	(net 13 "N33846695")
	(net 14 "N33846693")
	(net 15 "N33846691")
	(net 16 "N33846689")
	(net 17 "N33846648")
	(net 18 "N33846450")
	(net 19 "N33846429")
	(net 20 "N33846406")
	(net 21 "N33846306")
	(net 22 "N33846279")
	(net 23 "N33846257")
	(net 24 "N33846219")
	(net 25 "MOD_WAKEUP_IN")
	(net 26 "MOD_SPI_SCK")
	(net 27 "MOD_SPI_MOSI")
	(net 28 "MOD_SPI_MISO")
	(net 29 "MOD_SPI_CS")
	(net 30 "MOD_RESET")
	(net 31 "MOD_INT")
	(net 32 "MOD_BUSY")
	(net 33 "MOD_5V")
	(net 34 "MOD_3V3")
	(net 35 "GND")
	(net 36 "BUSY")
	(net 37 "ANT_WIFI")
	(net 38 "ANT_MOD")
	(footprint "C0402M"
		(layer "F.Cu")
		(at 160.5165 108.1672 -90)
		(property "Reference" "C14"
			(at 0.33057 -1.245354 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "N33866136")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 141.9491 113.6692 90)
		(property "Reference" "R13"
			(at -2.19258 0.102354 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "MOD_RESET")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "RESET")
		)
	)
	(footprint "SOT-23-5"
		(layer "F.Cu")
		(at 155.8361 106.8936 90)
		(property "Reference" "U1"
			(at -3.204 0.502894 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOT-23-5"
			(at -1.0781 2.987484 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.5 1 90)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N33862302")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "3" smd rect
			(at 1.5 -1 90)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at -1.5 -1 90)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
		(pad "5" smd rect
			(at -1.5 1 90)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 135.8785 113.1456 180)
		(property "Reference" "C9"
			(at 2.25646 -0.203954 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 138.9265 96.534 90)
		(property "Reference" "R11"
			(at -0.16216 -4.495046 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SPI_INT")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "MOD_INT")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 135.8277 114.4664 180)
		(property "Reference" "C12"
			(at 3.5306 -0.391408 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 128.5887 110.1164 -90)
		(property "Reference" "C1"
			(at 1.9994 -0.203954 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "FGH100M-H"
		(layer "F.Cu")
		(at 139.7727 105.2444 90)
		(property "Reference" "UM1"
			(at 6.004546 -8.14046 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FGH100M-H"
			(at -4.7 0.342784 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" smd custom
			(at -5.725 -5.85)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0.125 0.125) (xy 0.7 0.125) (xy 0.7 -0.575) (xy 0 -0.575)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "" smd custom
			(at -4.25 -4.45)
			(size 0.000001 0.000001)
			(layers "F.Cu")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0 0) (xy 0 -1.42) (xy 1.62 -1.42) (xy 1.62 0.2) (xy 0.2 0.2)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "1" smd circle
			(at -5.5 -5.5 90)
			(size 0.25 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 90)
		)
		(pad "2" smd rect
			(at -5.5 -4.4 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "3" smd rect
			(at -5.5 -3.3 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "4" smd rect
			(at -5.5 -2.2 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
			(solder_mask_margin 0.05)
		)
		(pad "5" smd rect
			(at -5.5 -1.1 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "6" smd rect
			(at -5.5 0 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
			(solder_mask_margin 0.05)
		)
		(pad "7" smd rect
			(at -5.5 1.1 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "8" smd rect
			(at -5.5 2.2 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "RESET")
			(solder_mask_margin 0.05)
		)
		(pad "9" smd rect
			(at -5.5 3.3 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "10" smd rect
			(at -5.5 4.4 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "BUSY")
			(solder_mask_margin 0.05)
		)
		(pad "11" smd rect
			(at -5.5 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "N33846648")
			(solder_mask_margin 0.05)
		)
		(pad "12" smd rect
			(at -4.4 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "N33846689")
			(solder_mask_margin 0.05)
		)
		(pad "13" smd rect
			(at -3.3 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "N33846691")
			(solder_mask_margin 0.05)
		)
		(pad "14" smd rect
			(at -2.2 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "N33846693")
			(solder_mask_margin 0.05)
		)
		(pad "15" smd rect
			(at -1.1 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "N33846695")
			(solder_mask_margin 0.05)
		)
		(pad "16" smd rect
			(at 0 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "N33846697")
			(solder_mask_margin 0.05)
		)
		(pad "17" smd rect
			(at 1.1 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
			(solder_mask_margin 0.05)
		)
		(pad "18" smd rect
			(at 2.2 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "19" smd rect
			(at 3.3 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "N33846703")
			(solder_mask_margin 0.05)
		)
		(pad "20" smd rect
			(at 4.4 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SPI_CS")
			(solder_mask_margin 0.05)
		)
		(pad "21" smd rect
			(at 5.5 5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "22" smd rect
			(at 5.5 4.4 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
			(solder_mask_margin 0.05)
		)
		(pad "23" smd rect
			(at 5.5 3.3 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "SPI_MOSI")
			(solder_mask_margin 0.05)
		)
		(pad "24" smd rect
			(at 5.5 2.2 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "SPI_CLK")
			(solder_mask_margin 0.05)
		)
		(pad "25" smd rect
			(at 5.5 1.1 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "SPI_MISO")
			(solder_mask_margin 0.05)
		)
		(pad "26" smd rect
			(at 5.5 0 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "SPI_INT")
			(solder_mask_margin 0.05)
		)
		(pad "27" smd rect
			(at 5.5 -1.1 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "28" smd rect
			(at 5.5 -2.2 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "N33846450")
			(solder_mask_margin 0.05)
		)
		(pad "29" smd rect
			(at 5.5 -3.3 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "N33846429")
			(solder_mask_margin 0.05)
		)
		(pad "30" smd rect
			(at 5.5 -4.4 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "N33846406")
			(solder_mask_margin 0.05)
		)
		(pad "31" smd rect
			(at 5.5 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "32" smd rect
			(at 4.4 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "N33846306")
			(solder_mask_margin 0.05)
		)
		(pad "33" smd rect
			(at 3.3 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "N33846279")
			(solder_mask_margin 0.05)
		)
		(pad "34" smd rect
			(at 2.2 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "N33846257")
			(solder_mask_margin 0.05)
		)
		(pad "35" smd rect
			(at 1.1 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "36" smd rect
			(at 0 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "N33846219")
			(solder_mask_margin 0.05)
		)
		(pad "37" smd rect
			(at -1.1 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.05)
		)
		(pad "38" smd rect
			(at -2.2 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "39" smd rect
			(at -3.3 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "40" smd rect
			(at -4.4 -5.5 90)
			(size 0.7 0.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_MOD")
			(solder_mask_margin 0.05)
		)
		(pad "41" smd rect
			(at -3.64 -3.64 90)
			(size 0.25 0.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "42" smd rect
			(at -1.82 -3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "43" smd rect
			(at 0 -3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "44" smd rect
			(at 1.82 -3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "45" smd rect
			(at 3.64 -3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "46" smd rect
			(at -3.64 -1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "47" smd rect
			(at -1.82 -1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "48" smd rect
			(at 0 -1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "49" smd rect
			(at 1.82 -1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "50" smd rect
			(at 3.64 -1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "51" smd rect
			(at -3.64 0 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "52" smd rect
			(at -1.82 0 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "53" smd rect
			(at 0 0 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "54" smd rect
			(at 1.82 0 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "55" smd rect
			(at 3.64 0 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "56" smd rect
			(at -3.64 1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "57" smd rect
			(at -1.82 1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "58" smd rect
			(at 0 1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "59" smd rect
			(at 1.82 1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "60" smd rect
			(at 3.64 1.82 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "61" smd rect
			(at -3.64 3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "62" smd rect
			(at -1.82 3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "63" smd rect
			(at 0 3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "64" smd rect
			(at 1.82 3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
		(pad "65" smd rect
			(at 3.64 3.64 90)
			(size 1.62 1.62)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(solder_mask_margin 0.05)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 139.3583 114.2788)
		(property "Reference" "R10"
			(at -0.45879 2.140964 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "MOD_WAKEUP_IN")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 148.0689 103.4936 90)
		(property "Reference" "C7"
			(at -0.53682 1.296164 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "CON_U.FL-R-SMT-1"
		(layer "F.Cu")
		(at 125.4391 109.6592 90)
		(property "Reference" "CN1"
			(at -2.890254 -0.50415 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CON_U.FL-R-SMT-1"
			(at -1.2 2.738894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 0 1.7 180)
			(size 1.25 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 1.475 0 180)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "3" smd rect
			(at -1.475 0 180)
			(size 2.2 1.05)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 125.4391 110.56355) (xy 125.26267 110.54618) (xy 125.09302 110.49471) (xy 124.93667 110.41114)
					(xy 124.79962 110.29867) (xy 124.68716 110.16163) (xy 124.60358 110.00528) (xy 124.55212 109.83563)
					(xy 124.53475 109.6592) (xy 124.55212 109.48277) (xy 124.60358 109.31312) (xy 124.68716 109.15677)
					(xy 124.79962 109.01972) (xy 124.93667 108.90725) (xy 125.09302 108.82368) (xy 125.26267 108.77222)
					(xy 125.4391 108.75484) (xy 125.4391 108.7592) (xy 126.7391 108.7592) (xy 126.7391 110.5592) (xy 125.4391 110.5592)
				)
			)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 106.3044 180)
		(property "Reference" "R23"
			(at -1.64987 -0.110954 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "N33846695")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 130.1635 109.6592)
		(property "Reference" "R1"
			(at -0.17277 1.277354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "ANT_WIFI")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_MOD")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 131.2811 100.82 180)
		(property "Reference" "R5"
			(at 1.84099 -0.159754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "N33846306")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 157.6261 96.7336 90)
		(property "Reference" "C8"
			(at -1.96482 0.159364 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "PL_SWPA4018"
		(layer "F.Cu")
		(at 158.2761 102.1936 -90)
		(property "Reference" "L1"
			(at 0.395205 -2.2912 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PL_SWPA4018"
			(at -1.28 1.640575 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.4 0)
			(size 3.4 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 1.4 0)
			(size 3.4 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N33862302")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 160.2761 101.5536) (xy 160.2761 102.8336) (xy 156.2961 102.8336) (xy 156.2961 101.5536)
				)
			)
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 131.0961 118.0136)
		(property "Reference" "MK1"
			(at -0.35724 -2.047836 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 131.2811 103.0552 180)
		(property "Reference" "R3"
			(at 1.84099 -0.159754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "N33846257")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 135.2943 96.5528 90)
		(property "Reference" "R6"
			(at -0.13824 -4.063246 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "N33846406")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "TP_1MM25"
		(layer "F.Cu")
		(at 163.3461 108.0336)
		(property "Reference" "TP2"
			(at 1.730454 0.3848 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TP_1MM25"
			(at -1.0414 1.385094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.25 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 131.1261 92.6036)
		(property "Reference" "MK4"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 137.6819 96.5528 90)
		(property "Reference" "R8"
			(at -0.14579 -4.317246 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "N33846450")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 143.7525 96.534 90)
		(property "Reference" "R16"
			(at -0.32423 3.886964 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "SPI_MOSI")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "MOD_SPI_MOSI")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 110.726 180)
		(property "Reference" "R18"
			(at -1.47161 -0.261354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "N33846648")
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 167.9079 117.4382)
		(property "Reference" "MK2"
			(at -0.38607 -1.844636 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 152.2361 107.4052 90)
		(property "Reference" "C11"
			(at -3.4036 0.518408 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 144.1843 113.72 90)
		(property "Reference" "R17"
			(at -2.19258 0.203954 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "MOD_BUSY")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "BUSY")
		)
	)
	(footprint "SOD123FL"
		(layer "F.Cu")
		(at 158.8909 107.1004 -90)
		(property "Reference" "D2"
			(at 3.937 -0.419894 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SOD123FL"
			(at -1.8288 2.170906 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.66872 0)
			(size 1.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N33862302")
		)
		(pad "2" smd rect
			(at 1.66872 0)
			(size 1.3 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 153.5569 107.456 90)
		(property "Reference" "C16"
			(at -2.37286 0.229354 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "MOD_5V")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 154.2173 101.868 -90)
		(property "Reference" "C15"
			(at 0.6604 1.844595 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 136.5135 96.5528 90)
		(property "Reference" "R7"
			(at -0.14579 -4.215646 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "N33846429")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "FB0603"
		(layer "F.Cu")
		(at 160.2625 97.3468 180)
		(property "Reference" "FB1"
			(at 0.69556 -1.600954 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FB0603"
			(at -2.60807 0.513153 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "2" smd rect
			(at 0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
	)
	(footprint "CON_MINI_PCIE_A"
		(layer "F.Cu")
		(at 170.7261 108.8536)
		(property "Reference" "CN2"
			(at -0.417146 -5.11803 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CON_MINI_PCIE_A"
			(at -38.7 -16.124366 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.85 7.95)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at 1.85 7.55)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "3" smd rect
			(at 1.85 7.15)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at 1.85 6.75)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "5" smd rect
			(at 1.85 6.35)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 1.85 5.95)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "7" smd rect
			(at 1.85 5.55)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at 1.85 5.15)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "9" smd rect
			(at 1.85 4.75)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "10" smd rect
			(at 1.85 4.35)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 31 "MOD_INT")
		)
		(pad "11" smd rect
			(at 1.85 3.95)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "12" smd rect
			(at 1.85 3.55)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "13" smd rect
			(at 1.85 3.15)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "14" smd rect
			(at 1.85 2.75)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "15" smd rect
			(at 1.85 2.35)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "16" smd rect
			(at 1.85 1.95)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "17" smd rect
			(at 1.85 -1.65)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "18" smd rect
			(at 1.85 -2.05)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "19" smd rect
			(at 1.85 -2.45)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "20" smd rect
			(at 1.85 -2.85)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "21" smd rect
			(at 1.85 -3.25)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "22" smd rect
			(at 1.85 -3.65)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 30 "MOD_RESET")
		)
		(pad "23" smd rect
			(at 1.85 -4.05)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "24" smd rect
			(at 1.85 -4.45)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "25" smd rect
			(at 1.85 -4.85)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "26" smd rect
			(at 1.85 -5.25)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "27" smd rect
			(at 1.85 -5.65)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "28" smd rect
			(at 1.85 -6.05)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "29" smd rect
			(at 1.85 -6.45)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "30" smd rect
			(at 1.85 -6.85)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "31" smd rect
			(at 1.85 -7.25)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "MOD_BUSY")
		)
		(pad "32" smd rect
			(at 1.85 -7.65)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "33" smd rect
			(at 1.85 -8.05)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "MOD_WAKEUP_IN")
		)
		(pad "34" smd rect
			(at 1.85 -8.45)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "35" smd rect
			(at 1.85 -8.85)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "36" smd rect
			(at 1.85 -9.25)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "37" smd rect
			(at 1.85 -9.65)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "38" smd rect
			(at 1.85 -10.05)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "39" smd rect
			(at 1.85 -10.45)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "40" smd rect
			(at 1.85 -10.85)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "41" smd rect
			(at 1.85 -11.25)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "42" smd rect
			(at 1.85 -11.65)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "43" smd rect
			(at 1.85 -12.05)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "44" smd rect
			(at 1.85 -12.45)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "45" smd rect
			(at 1.85 -12.85)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "MOD_SPI_SCK")
		)
		(pad "46" smd rect
			(at 1.85 -13.25)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "47" smd rect
			(at 1.85 -13.65)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "MOD_SPI_MISO")
		)
		(pad "48" smd rect
			(at 1.85 -14.05)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "49" smd rect
			(at 1.85 -14.45)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "MOD_SPI_MOSI")
		)
		(pad "50" smd rect
			(at 1.85 -14.85)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "GND")
		)
		(pad "51" smd rect
			(at 1.85 -15.25)
			(size 2.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "MOD_SPI_CS")
		)
		(pad "52" smd rect
			(at 1.85 -15.65)
			(size 2.3 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "53" thru_hole rect
			(at -44.8 -15.95)
			(size 5 5)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "GND")
		)
		(pad "54" thru_hole rect
			(at -44.8 8.25)
			(size 5 5)
			(drill 2.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "GND")
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 168.7969 91.9112)
		(property "Reference" "MK3"
			(at -0.17847 2.312164 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 139.3583 113.3136)
		(property "Reference" "R9"
			(at -0.33484 2.140964 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "WAKEUP_IN")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 146.3961 96.6336 90)
		(property "Reference" "C6"
			(at -0.27726 3.427764 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 142.0127 96.5528 90)
		(property "Reference" "R14"
			(at -0.29514 1.029364 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "SPI_CLK")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "MOD_SPI_SCK")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 107.3544 180)
		(property "Reference" "R22"
			(at -1.59907 -0.229354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "N33846693")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 131.2811 105.1888 180)
		(property "Reference" "R2"
			(at 1.84099 -0.159754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "N33846219")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 156.2261 96.7836 90)
		(property "Reference" "C5"
			(at -2.37002 0.252564 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 109.6544 180)
		(property "Reference" "R19"
			(at -1.52997 -0.215354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "N33846689")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 140.1457 96.534 90)
		(property "Reference" "R12"
			(at -0.28099 1.092964 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "SPI_MISO")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "MOD_SPI_MISO")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 108.4908 180)
		(property "Reference" "R20"
			(at -1.64987 -0.210554 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "N33846691")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 131.2811 101.9376 180)
		(property "Reference" "R4"
			(at 1.84855 -0.159754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "N33846279")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 145.1495 113.72 90)
		(property "Reference" "R15"
			(at -2.19258 0.203954 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "BUSY")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 145.1749 96.6356 90)
		(property "Reference" "C3"
			(at -0.28282 3.531364 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -1.94564 -5.056892 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 160.5165 106.1352 -90)
		(property "Reference" "R26"
			(at 0.4572 -1.639094 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "N33862302")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "N33866136")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 100.74431)
		(property "Reference" "R21"
			(at -0.13631 -2.050556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "SPI_CS")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "MOD_SPI_CS")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 101.8844)
		(property "Reference" "R25"
			(at -0.15353 -2.073046 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "N33846703")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 148.4261 105.2744 180)
		(property "Reference" "R24"
			(at -1.64231 -0.023354 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "N33846697")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 162.6241 96.6476 90)
		(property "Reference" "C13"
			(at -2.31761 0.204554 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "TP_1MM25"
		(layer "F.Cu")
		(at 154.1061 97.5536)
		(property "Reference" "TP1"
			(at -1.094536 0.30658 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TP_1MM25"
			(at -1.0414 1.385094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.25 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 131.73119 110.1164 -90)
		(property "Reference" "C2"
			(at 2.11822 -0.109464 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "ANT_MOD")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 155.4873 101.7156 -90)
		(property "Reference" "C10"
			(at 0.43422 2.384375 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "MOD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 163.9201 96.6864 90)
		(property "Reference" "C4"
			(at -2.42398 0.280154 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "C0603"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "PCIE_3V3")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "GND")
		)
	)
	(gr_line
		(start 171.57748 117.8536)
		(end 171.577678 117.853601)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.7761 120.0036)
		(end 123.0261 120.0036)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.777511 118.650979)
		(mid 171.01164 118.085761)
		(end 171.577678 117.853601)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.745 108.1036)
		(end 170.74466 108.103587)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.7761 118.66745)
		(end 170.7761 120.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.57941 92.1536)
		(end 173.9761 92.1536)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.9761 92.1536)
		(end 173.9761 108.1036)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.74466 109.603613)
		(mid 169.974729 108.8536)
		(end 170.74466 108.103587)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.579414 92.153605)
		(mid 171.011546 91.920137)
		(end 170.7761 91.35309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.7761 91.35367)
		(end 170.7761 91.35309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.77751 118.65169)
		(end 170.7761 118.66745)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.74486 109.6036)
		(end 173.9761 109.6036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.9761 117.8536)
		(end 171.57748 117.8536)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.74466 109.603613)
		(end 170.74486 109.6036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.777511 118.650979)
		(end 170.77751 118.65169)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.579414 92.153605)
		(end 171.57941 92.1536)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.0261 90.01422)
		(end 123.02836 90.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.9761 108.1036)
		(end 170.745 108.1036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.9761 109.6036)
		(end 173.9761 117.8536)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.7761 90.0036)
		(end 170.7761 91.35367)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.02836 90.0036)
		(end 170.7761 90.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.0261 120.0036)
		(end 123.0261 90.01422)
		(layer "Edge.Cuts")
	)
	(gr_text "Wio-WM6108"
		(at 141.9745 118.904034 0)
		(layer "F.SilkS")
	)
	(gr_text "Wi-Fi Halow"
		(at 126.639167 106.5924 90)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 134.44602 108.9038) (xy 126.6583 108.9038) (xy 126.6583 110.3262) (xy 134.44572 110.32751) (xy 134.49555 110.33407)
				(xy 134.68166 110.30957) (xy 134.85509 110.23774) (xy 135.00401 110.12346) (xy 135.11829 109.97454)
				(xy 135.19012 109.80111) (xy 135.21462 109.615) (xy 135.19012 109.42889) (xy 135.11829 109.25546)
				(xy 135.00401 109.10654) (xy 134.85509 108.99226) (xy 134.68166 108.92043) (xy 134.49555 108.89593)
				(xy 134.44572 108.90249)
			)
		)
	)
	(zone
		(net 35)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 122.5181 89.422) (xy 122.5181 120.7148) (xy 171.4385 120.7148) (xy 171.4385 89.422)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.995921 117.753952) (xy 174.032546 117.769123) (xy 174.060577 117.797154) (xy 174.075748 117.833779)
				(xy 174.075748 117.873421) (xy 174.060577 117.910046) (xy 174.032546 117.938077) (xy 173.995921 117.953248)
				(xy 173.9761 117.9552) (xy 171.57748 117.9552) (xy 171.557659 117.953248) (xy 171.521034 117.938077)
				(xy 171.493003 117.910046) (xy 171.477832 117.873421) (xy 171.477832 117.833779) (xy 171.493003 117.797154)
				(xy 171.521034 117.769123) (xy 171.557659 117.753952) (xy 171.57748 117.752) (xy 173.9761 117.752)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.579057 92.052006) (xy 171.629904 92.065439) (xy 171.667223 92.102496) (xy 171.681013 92.153248)
				(xy 171.66758 92.204095) (xy 171.630523 92.241414) (xy 171.579771 92.255204) (xy 171.579771 92.255203)
				(xy 171.403328 92.238412) (xy 171.233574 92.187446) (xy 171.077061 92.104273) (xy 170.939831 91.992104)
				(xy 170.827181 91.855267) (xy 170.74346 91.699047) (xy 170.6919 91.529472) (xy 170.674491 91.353089)
				(xy 170.6745 91.353089) (xy 170.688112 91.302289) (xy 170.725301 91.265101) (xy 170.776101 91.25149)
				(xy 170.826901 91.265102) (xy 170.864089 91.302291) (xy 170.8777 91.353091) (xy 170.877691 91.353091)
				(xy 170.877705 91.422082) (xy 170.904682 91.5574) (xy 170.957596 91.684833) (xy 171.034404 91.799459)
				(xy 171.132143 91.896856) (xy 171.247038 91.973262) (xy 171.374654 92.02573) (xy 171.510067 92.052232)
				(xy 171.579057 92.052005)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.676452 118.647629) (xy 170.691623 118.611004) (xy 170.719654 118.582973) (xy 170.756279 118.567802)
				(xy 170.795921 118.567802) (xy 170.832546 118.582973) (xy 170.860577 118.611004) (xy 170.875748 118.647629)
				(xy 170.8777 118.66745) (xy 170.8777 120.0036) (xy 170.875748 120.023421) (xy 170.860577 120.060046)
				(xy 170.832546 120.088077) (xy 170.795921 120.103248) (xy 170.756279 120.103248) (xy 170.719654 120.088077)
				(xy 170.691623 120.060046) (xy 170.676452 120.023421) (xy 170.6745 120.0036) (xy 170.6745 118.66745)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.995921 109.503952) (xy 174.032546 109.519123) (xy 174.060577 109.547154) (xy 174.075748 109.583779)
				(xy 174.075748 109.623421) (xy 174.060577 109.660046) (xy 174.032546 109.688077) (xy 173.995921 109.703248)
				(xy 173.9761 109.7052) (xy 170.74486 109.7052) (xy 170.725039 109.703248) (xy 170.688414 109.688077)
				(xy 170.660383 109.660046) (xy 170.645212 109.623421) (xy 170.645212 109.583779) (xy 170.660383 109.547154)
				(xy 170.688414 109.519123) (xy 170.725039 109.503952) (xy 170.74486 109.502) (xy 173.9761 109.502)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.93502 89.963472) (xy 122.957482 89.930807) (xy 122.990734 89.909224) (xy 123.029714 89.902009)
				(xy 123.068488 89.91026) (xy 123.101153 89.932722) (xy 123.122736 89.965974) (xy 123.129951 90.004954)
				(xy 123.127735 90.024747) (xy 123.125475 90.035368) (xy 123.11944 90.054348) (xy 123.096978 90.087013)
				(xy 123.063726 90.108596) (xy 123.024746 90.115811) (xy 122.985972 90.10756) (xy 122.953307 90.085098)
				(xy 122.931724 90.051846) (xy 122.924509 90.012866) (xy 122.926725 89.993072) (xy 122.928985 89.982452)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.876452 109.583779) (xy 173.891623 109.547154) (xy 173.919654 109.519123) (xy 173.956279 109.503952)
				(xy 173.995921 109.503952) (xy 174.032546 109.519123) (xy 174.060577 109.547154) (xy 174.075748 109.583779)
				(xy 174.0777 109.6036) (xy 174.0777 117.8536) (xy 174.075748 117.873421) (xy 174.060577 117.910046)
				(xy 174.032546 117.938077) (xy 173.995921 117.953248) (xy 173.956279 117.953248) (xy 173.919654 117.938077)
				(xy 173.891623 117.910046) (xy 173.876452 117.873421) (xy 173.8745 117.8536) (xy 173.8745 109.6036)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.876452 92.133779) (xy 173.891623 92.097154) (xy 173.919654 92.069123) (xy 173.956279 92.053952)
				(xy 173.995921 92.053952) (xy 174.032546 92.069123) (xy 174.060577 92.097154) (xy 174.075748 92.133779)
				(xy 174.0777 92.1536) (xy 174.0777 108.1036) (xy 174.075748 108.123421) (xy 174.060577 108.160046)
				(xy 174.032546 108.188077) (xy 173.995921 108.203248) (xy 173.956279 108.203248) (xy 173.919654 108.188077)
				(xy 173.891623 108.160046) (xy 173.876452 108.123421) (xy 173.8745 108.1036) (xy 173.8745 92.1536)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.926452 89.994399) (xy 122.941623 89.957774) (xy 122.969654 89.929743) (xy 123.006279 89.914572)
				(xy 123.045921 89.914572) (xy 123.082546 89.929743) (xy 123.110577 89.957774) (xy 123.125748 89.994399)
				(xy 123.1277 90.01422) (xy 123.1277 120.0036) (xy 123.125748 120.023421) (xy 123.110577 120.060046)
				(xy 123.082546 120.088077) (xy 123.045921 120.103248) (xy 123.006279 120.103248) (xy 122.969654 120.088077)
				(xy 122.941623 120.060046) (xy 122.926452 120.023421) (xy 122.9245 120.0036) (xy 122.9245 90.01422)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.680025 118.623068) (xy 170.698399 118.587941) (xy 170.728816 118.562519) (xy 170.766648 118.550672)
				(xy 170.806132 118.554205) (xy 170.841259 118.572579) (xy 170.866681 118.602996) (xy 170.878528 118.640828)
				(xy 170.878706 118.660744) (xy 170.877296 118.676504) (xy 170.873585 118.696072) (xy 170.855211 118.731199)
				(xy 170.824794 118.756621) (xy 170.786962 118.768468) (xy 170.747478 118.764935) (xy 170.712351 118.746561)
				(xy 170.686929 118.716144) (xy 170.675082 118.678312) (xy 170.674904 118.658396) (xy 170.676314 118.642636)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.879111 118.650803) (xy 170.865587 118.701626) (xy 170.828463 118.738879) (xy 170.777687 118.752579)
				(xy 170.726864 118.739055) (xy 170.689611 118.701931) (xy 170.675911 118.651155) (xy 170.693007 118.475246)
				(xy 170.744239 118.306097) (xy 170.827623 118.150265) (xy 170.939925 118.013793) (xy 171.076791 117.901972)
				(xy 171.232915 117.819137) (xy 171.402243 117.768499) (xy 171.578211 117.752022) (xy 171.578211 117.752002)
				(xy 171.628939 117.765881) (xy 171.665932 117.803264) (xy 171.679277 117.854134) (xy 171.665398 117.904862)
				(xy 171.628015 117.941855) (xy 171.577145 117.9552) (xy 171.577145 117.95522) (xy 171.508451 117.954889)
				(xy 171.373586 117.981102) (xy 171.246472 118.033234) (xy 171.132037 118.109262) (xy 171.034718 118.20624)
				(xy 170.958287 118.320407) (xy 170.905709 118.447337) (xy 170.879022 118.582109) (xy 170.879111 118.650803)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.795921 119.903952) (xy 170.832546 119.919123) (xy 170.860577 119.947154) (xy 170.875748 119.983779)
				(xy 170.875748 120.023421) (xy 170.860577 120.060046) (xy 170.832546 120.088077) (xy 170.795921 120.103248)
				(xy 170.7761 120.1052) (xy 123.0261 120.1052) (xy 123.006279 120.103248) (xy 122.969654 120.088077)
				(xy 122.941623 120.060046) (xy 122.926452 120.023421) (xy 122.926452 119.983779) (xy 122.941623 119.947154)
				(xy 122.969654 119.919123) (xy 123.006279 119.903952) (xy 123.0261 119.902) (xy 170.7761 119.902)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.995921 108.003952) (xy 174.032546 108.019123) (xy 174.060577 108.047154) (xy 174.075748 108.083779)
				(xy 174.075748 108.123421) (xy 174.060577 108.160046) (xy 174.032546 108.188077) (xy 173.995921 108.203248)
				(xy 173.9761 108.2052) (xy 170.745 108.2052) (xy 170.725179 108.203248) (xy 170.688554 108.188077)
				(xy 170.660523 108.160046) (xy 170.645352 108.123421) (xy 170.645352 108.083779) (xy 170.660523 108.047154)
				(xy 170.688554 108.019123) (xy 170.725179 108.003952) (xy 170.745 108.002) (xy 173.9761 108.002)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.676452 89.983779) (xy 170.691623 89.947154) (xy 170.719654 89.919123) (xy 170.756279 89.903952)
				(xy 170.795921 89.903952) (xy 170.832546 89.919123) (xy 170.860577 89.947154) (xy 170.875748 89.983779)
				(xy 170.8777 90.0036) (xy 170.8777 91.35367) (xy 170.875748 91.373491) (xy 170.860577 91.410116)
				(xy 170.832546 91.438147) (xy 170.795921 91.453318) (xy 170.756279 91.453318) (xy 170.719654 91.438147)
				(xy 170.691623 91.410116) (xy 170.676452 91.373491) (xy 170.6745 91.35367) (xy 170.6745 90.0036)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.995921 92.053952) (xy 174.032546 92.069123) (xy 174.060577 92.097154) (xy 174.075748 92.133779)
				(xy 174.075748 92.173421) (xy 174.060577 92.210046) (xy 174.032546 92.238077) (xy 173.995921 92.253248)
				(xy 173.9761 92.2552) (xy 171.57941 92.2552) (xy 171.559589 92.253248) (xy 171.522964 92.238077)
				(xy 171.494933 92.210046) (xy 171.479762 92.173421) (xy 171.479762 92.133779) (xy 171.494933 92.097154)
				(xy 171.522964 92.069123) (xy 171.559589 92.053952) (xy 171.57941 92.052) (xy 173.9761 92.052)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.795921 89.903952) (xy 170.832546 89.919123) (xy 170.860577 89.947154) (xy 170.875748 89.983779)
				(xy 170.875748 90.023421) (xy 170.860577 90.060046) (xy 170.832546 90.088077) (xy 170.795921 90.103248)
				(xy 170.7761 90.1052) (xy 123.02836 90.1052) (xy 123.008539 90.103248) (xy 122.971914 90.088077)
				(xy 122.943883 90.060046) (xy 122.928712 90.023421) (xy 122.928712 89.983779) (xy 122.943883 89.947154)
				(xy 122.971914 89.919123) (xy 123.008539 89.903952) (xy 123.02836 89.902) (xy 170.7761 89.902)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.741998 109.502048) (xy 170.793137 109.514324) (xy 170.831287 109.550525) (xy 170.846225 109.600951)
				(xy 170.833949 109.65209) (xy 170.797748 109.69024) (xy 170.747322 109.705178) (xy 170.747322 109.705177)
				(xy 170.578009 109.692693) (xy 170.414535 109.64688) (xy 170.263391 109.569561) (xy 170.130581 109.463804)
				(xy 170.021381 109.333812) (xy 169.940127 109.184746) (xy 169.890047 109.022528) (xy 169.87313 108.8536)
				(xy 169.890047 108.684672) (xy 169.940127 108.522454) (xy 170.021381 108.373388) (xy 170.130581 108.243396)
				(xy 170.263391 108.137639) (xy 170.414535 108.06032) (xy 170.578009 108.014507) (xy 170.747322 108.002023)
				(xy 170.747322 108.002022) (xy 170.797748 108.01696) (xy 170.833949 108.05511) (xy 170.846225 108.106249)
				(xy 170.831287 108.156675) (xy 170.793137 108.192876) (xy 170.741998 108.205152) (xy 170.741998 108.205153)
				(xy 170.667718 108.203343) (xy 170.522134 108.233148) (xy 170.387063 108.295107) (xy 170.269506 108.38601)
				(xy 170.175554 108.501145) (xy 170.110077 108.634545) (xy 170.076467 108.779298) (xy 170.076467 108.927902)
				(xy 170.110077 109.072655) (xy 170.175554 109.206055) (xy 170.269506 109.32119) (xy 170.387063 109.412093)
				(xy 170.522134 109.474052) (xy 170.667718 109.503857) (xy 170.741998 109.502047)
			)
		)
	)
	(zone
		(net 35)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 122.0609 88.9648) (xy 122.0609 121.172) (xy 171.4385 121.172) (xy 171.4385 88.9648)
			)
		)
	)
)
