(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top")
		(31 "B.Cu" signal "Bottom")
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user "Paste Mask Bottom")
		(35 "F.Paste" user "Paste Mask Top")
		(36 "B.SilkS" user "Silkscreen Bottom")
		(37 "F.SilkS" user "Silkscreen Top")
		(38 "B.Mask" user "Solder Mask Bottom")
		(39 "F.Mask" user "Solder Mask Top")
		(40 "Dwgs.User" user "Layer_10")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "Layer_11")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user "Layer_13")
		(49 "F.Fab" user "Layer_12")
		(50 "User.1" user "Assembly Drawing Top")
		(51 "User.2" user "Assembly Drawing Bottom")
		(52 "User.3" user "Layer_3")
		(53 "User.4" user "Layer_4")
		(54 "User.5" user "Layer_5")
		(55 "User.6" user "Layer_6")
		(56 "User.7" user "Layer_7")
		(57 "User.8" user "Layer_8")
		(58 "User.9" user "Layer_9")
	)
	(setup
		(pad_to_mask_clearance 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin -697.85271 351.80747)
		(grid_origin -697.85271 351.80747)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "W55_XTOUT")
	(net 2 "W55_XTIN")
	(net 3 "W55_INT")
	(net 4 "VDD_68V")
	(net 5 "VDD_5V")
	(net 6 "RJ45_VB2")
	(net 7 "RJ45_VB1")
	(net 8 "RJ45_VA2")
	(net 9 "RJ45_VA1")
	(net 10 "RJ45_TX2+")
	(net 11 "RJ45_TX2-")
	(net 12 "RJ45_RX2+")
	(net 13 "RJ45_RX2-")
	(net 14 "PWRGND")
	(net 15 "POE_5V")
	(net 16 "POE_12V")
	(net 17 "NET_TXOP")
	(net 18 "NET_TXON")
	(net 19 "NET_TXCT")
	(net 20 "NET_RXIP")
	(net 21 "NET_RXIN")
	(net 22 "NET_RXCT")
	(net 23 "NET_LINK")
	(net 24 "NET_ACTIVE")
	(net 25 "N34439840")
	(net 26 "N34439826")
	(net 27 "N34434887")
	(net 28 "N34429103")
	(net 29 "N34403312")
	(net 30 "N34403291")
	(net 31 "N34403260")
	(net 32 "N34403229")
	(net 33 "N34403215")
	(net 34 "N34403052")
	(net 35 "N34402995")
	(net 36 "N34401469")
	(net 37 "N34401387")
	(net 38 "N34401385")
	(net 39 "N34395173")
	(net 40 "N34395146")
	(net 41 "N34395115")
	(net 42 "N34394983")
	(net 43 "N34394975")
	(net 44 "N34394924")
	(net 45 "N34394891")
	(net 46 "N34391021")
	(net 47 "N34390191")
	(net 48 "N34390189")
	(net 49 "GND_ETH")
	(net 50 "GND")
	(net 51 "ESP32_EN")
	(net 52 "D19_SPI_MOSI1")
	(net 53 "D18_SPI_MISO1")
	(net 54 "D17_SPI_SCK1")
	(net 55 "D16_ADC")
	(net 56 "D15_I2S_TX1")
	(net 57 "D14_I2S_RX1")
	(net 58 "D13_I2S_WS")
	(net 59 "D12_I2S_SCK")
	(net 60 "D11_I2S_SD")
	(net 61 "AVDD_3V3")
	(net 62 "A9_D9_MISO")
	(net 63 "A8_D8_SCK")
	(net 64 "A7_D7_RX")
	(net 65 "A6_D6_TX")
	(net 66 "A5_D5_SCL")
	(net 67 "A4_D4_SDA")
	(net 68 "A3_D3")
	(net 69 "A2_D2")
	(net 70 "A10_D10_MOSI")
	(net 71 "A1_D1")
	(net 72 "A0_D0")
	(net 73 "3V3")
	(footprint "POE_MQ7813T120"
		(layer "F.Cu")
		(at 155.0011 96.70362)
		(property "Reference" "UM1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "POE_MQ7813T120"
			(at 0.338894 1 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at -11.43 7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "POE_12V")
		)
		(pad "2" thru_hole oval
			(at -8.89 7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "POE_12V")
		)
		(pad "3" thru_hole oval
			(at 8.89 7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
		)
		(pad "4" thru_hole oval
			(at 11.43 7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole oval
			(at 11.43 -7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "N34434887")
		)
		(pad "6" thru_hole oval
			(at 8.89 -7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "N34434887")
		)
		(pad "7" thru_hole oval
			(at -8.89 -7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "PWRGND")
		)
		(pad "8" thru_hole oval
			(at -11.43 -7.62 90)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "PWRGND")
		)
	)
	(footprint "TP_1MM2"
		(layer "F.Cu")
		(at 139.1401 104.61722)
		(property "Reference" "TP2"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP_1MM2"
			(at -1.0414 1.385094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 152.99635 90.23774)
		(property "Reference" "MK2"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 146.1251 121.33042 90)
		(property "Reference" "R7"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "N34394891")
		)
	)
	(footprint "CN_ESP32_XIAO_PLUS_24P"
		(layer "F.Cu")
		(at 109.5371 105.00362 90)
		(property "Reference" "CN1"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CN_ESP32_XIAO_PLUS_24P"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd oval
			(at -9.144 0 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "A0_D0")
		)
		(pad "2" smd oval
			(at -9.144 2.54 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "A1_D1")
		)
		(pad "3" smd oval
			(at -9.144 5.08 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "A2_D2")
		)
		(pad "4" smd oval
			(at -9.144 7.62 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "A3_D3")
		)
		(pad "5" smd oval
			(at -9.144 10.16 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "A4_D4_SDA")
		)
		(pad "6" smd oval
			(at -9.144 12.7 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "A5_D5_SCL")
		)
		(pad "7" smd oval
			(at -9.144 15.24 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "A6_D6_TX")
		)
		(pad "8" smd oval
			(at 9.144 15.24 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "A7_D7_RX")
		)
		(pad "9" smd oval
			(at 9.144 12.7 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "A8_D8_SCK")
		)
		(pad "10" smd oval
			(at 9.144 10.16 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "A9_D9_MISO")
		)
		(pad "11" smd oval
			(at 9.144 7.62 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "A10_D10_MOSI")
		)
		(pad "12" smd oval
			(at 9.144 5.08 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "13" smd oval
			(at 9.144 2.54 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "14" smd oval
			(at 9.144 0 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "VDD_5V")
		)
		(pad "15" smd oval
			(at -9.144 1.27 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "D11_I2S_SD")
		)
		(pad "16" smd oval
			(at -9.144 3.81 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "D12_I2S_SCK")
		)
		(pad "17" smd oval
			(at -9.144 6.35 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "D13_I2S_WS")
		)
		(pad "18" smd oval
			(at -9.144 8.89 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "D14_I2S_RX1")
		)
		(pad "19" smd oval
			(at -9.144 11.43 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "D15_I2S_TX1")
		)
		(pad "20" smd oval
			(at -9.144 13.97 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "D16_ADC")
		)
		(pad "21" smd oval
			(at 9.144 13.97 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "D19_SPI_MOSI1")
		)
		(pad "22" smd oval
			(at 9.144 11.43 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "D18_SPI_MISO1")
		)
		(pad "23" smd oval
			(at 9.144 8.89 90)
			(size 2.3368 0.9036)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "D17_SPI_SCK1")
		)
		(pad "25" smd circle
			(at -1.27 1.4086 90)
			(size 1.1938 1.1938)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "ESP32_EN")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "SOT-23"
		(layer "F.Cu")
		(at 154.4563 120.46682 -90)
		(property "Reference" "Q1"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SOT-23"
			(at -1 -1.938894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "SOT-23"
			(at 1.40845 -0.3747 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at -0.9525 0.9906 270)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "N34401469")
		)
		(pad "2" smd rect
			(at 0.9525 0.9906 270)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "3" smd rect
			(at 0 -1.0414)
			(size 1.27 0.9144)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "N34401387")
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 186.2063 105.04902)
		(property "Reference" "MK1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 172.0585 92.62842 -90)
		(property "Reference" "C33"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_68V")
		)
		(pad "2" smd rect
			(at 0.71 0 270)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "PWRGND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 129.8183 104.97282 180)
		(property "Reference" "C35"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -1.3 1.538792 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 158.07758 115.53592)
		(property "Reference" "C16"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 20 "NET_RXIP")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "N34403052")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 143.2295 106.64922 180)
		(property "Reference" "C11"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 40 "N34395146")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 171.0425 102.91002)
		(property "Reference" "C22"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "N34403291")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "RJ45_VB1")
		)
	)
	(footprint "HEADER_PIN_SIP2_2MM54"
		(layer "F.Cu")
		(at 137.9209 95.54942)
		(property "Reference" "CN6"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HEADER_PIN_SIP2_2MM54"
			(at 0.508 -1.993106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VDD_5V")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.1 1.6)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "POE_5V")
		)
	)
	(footprint "LED0603"
		(layer "F.Cu")
		(at 160.0011 119.80362 180)
		(property "Reference" "D1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED0603"
			(at -1 1.664995 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.8 0 270)
			(size 1 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "N34401385")
		)
		(pad "2" smd rect
			(at 0.8 0 270)
			(size 1 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "N34401387")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 170.9425 101.61002 180)
		(property "Reference" "R23"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34403215")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "N34403312")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 143.2295 107.51282 180)
		(property "Reference" "R11"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "N34395173")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 141.6039 107.30962 90)
		(property "Reference" "C29"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 152.3735 112.44042)
		(property "Reference" "C9"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "PL_FTC252012"
		(layer "F.Cu")
		(at 171.1695 89.02162)
		(property "Reference" "L2"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PL_FTC252012"
			(at -1.8 2.679425 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.95 0 90)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "N34434887")
		)
		(pad "2" smd rect
			(at 0.95 0 90)
			(size 2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_68V")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 170.8095 88.04162) (xy 171.5295 88.04162) (xy 171.5295 90.02162) (xy 170.8095 90.02162)
				)
			)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 151.8655 118.53642 90)
		(property "Reference" "R17"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NET_TXON")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 170.9425 96.51002 180)
		(property "Reference" "R21"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34403215")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "N34403260")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 139.2417 101.41682 90)
		(property "Reference" "C26"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "MBS_4P"
		(layer "F.Cu")
		(at 175.6907 91.89182 -90)
		(property "Reference" "D3"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MBS_4P"
			(at -1.9 2.274366 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd oval
			(at 3.15 1.25 270)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RJ45_VA2")
		)
		(pad "2" smd oval
			(at 3.15 -1.25 270)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "RJ45_VA1")
		)
		(pad "3" smd oval
			(at -3.15 -1.25 270)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_68V")
		)
		(pad "4" smd oval
			(at -3.15 1.25 270)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "PWRGND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 185.0887 116.96162 -90)
		(property "Reference" "C24"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 49 "GND_ETH")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 158.38238 109.64312 -90)
		(property "Reference" "ED2"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NET_TXOP")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NET_TXON")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 140.9943 109.69722)
		(property "Reference" "C31"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 130.6819 109.34162 180)
		(property "Reference" "C34"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 152.3735 111.37362)
		(property "Reference" "R10"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "N34394983")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 171.1425 95.21002)
		(property "Reference" "C21"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "N34403260")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RJ45_VA2")
		)
	)
	(footprint "MBS_4P"
		(layer "F.Cu")
		(at 182.6757 91.96802 -45)
		(property "Reference" "D4"
			(at 0 0.18669 315)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MBS_4P"
			(at -1.899996 2.274364 135)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -45)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd oval
			(at 3.149998 1.250002 315)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RJ45_VB2")
		)
		(pad "2" smd oval
			(at 3.149998 -1.250002 315)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "RJ45_VB1")
		)
		(pad "3" smd oval
			(at -3.149998 -1.250002 315)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_68V")
		)
		(pad "4" smd oval
			(at -3.149998 1.250002 315)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "PWRGND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 153.8975 114.82802 90)
		(property "Reference" "R15"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "NET_RXCT")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "NET_RXIN")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 130.6819 107.86842 180)
		(property "Reference" "C36"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.538792 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 153.8975 113.02802 -90)
		(property "Reference" "R16"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "NET_RXCT")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "NET_RXIP")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 129.8183 102.22962 180)
		(property "Reference" "C37"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 146.2775 107.00482 90)
		(property "Reference" "C6"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "N34395115")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 138.8861 113.02462 180)
		(property "Reference" "C8"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 270)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 144.9567 106.80162 90)
		(property "Reference" "C2"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 173.7095 115.69162 90)
		(property "Reference" "R26"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "NET_ACTIVE")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "N34439826")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 134.1363 112.44042 90)
		(property "Reference" "C25"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 48 "N34390189")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "N34390191")
		)
	)
	(footprint "H1102NL"
		(layer "F.Cu")
		(at 165.2259 112.79602 -90)
		(property "Reference" "LT1"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "H1102NL"
			(at -2.52 -1.369824 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -4.445 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NET_TXOP")
		)
		(pad "2" smd rect
			(at -3.175 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "NET_TXCT")
		)
		(pad "3" smd rect
			(at -1.905 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NET_TXON")
		)
		(pad "4" smd rect
			(at -0.635 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at 0.635 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "6" smd rect
			(at 1.905 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "N34403052")
		)
		(pad "7" smd rect
			(at 3.175 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "NET_RXCT")
		)
		(pad "8" smd rect
			(at 4.445 4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "N34402995")
		)
		(pad "9" smd rect
			(at 4.445 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "RJ45_RX2-")
		)
		(pad "10" smd rect
			(at 3.175 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "RJ45_VA2")
		)
		(pad "11" smd rect
			(at 1.905 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "RJ45_RX2+")
		)
		(pad "12" smd rect
			(at 0.635 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "13" smd rect
			(at -0.635 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "14" smd rect
			(at -1.905 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "RJ45_TX2-")
		)
		(pad "15" smd rect
			(at -3.175 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "RJ45_VA1")
		)
		(pad "16" smd rect
			(at -4.445 -4.5)
			(size 2 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "RJ45_TX2+")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 139.7243 119.04442 -90)
		(property "Reference" "R12"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "W55_INT")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 138.8607 111.98322 180)
		(property "Reference" "C7"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.8 1.461106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "TP_1MM2"
		(layer "F.Cu")
		(at 149.8843 109.24002)
		(property "Reference" "TP3"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP_1MM2"
			(at -1.0414 1.385094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 162.54798 119.95552)
		(property "Reference" "C15"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "NET_RXCT")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 157.41718 108.01752 90)
		(property "Reference" "C17"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "NET_TXCT")
		)
	)
	(footprint "C1206"
		(layer "F.Cu")
		(at 179.1451 115.84402 180)
		(property "Reference" "C19"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C1206"
			(at -2.1 0.880176 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.4 0 180)
			(size 1.7 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "GND_ETH")
		)
		(pad "2" smd rect
			(at 1.4 0 180)
			(size 1.7 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34403215")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 152.3227 116.80922 180)
		(property "Reference" "R19"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NET_TXOP")
		)
	)
	(footprint "W5500_LQFP48"
		(layer "F.Cu")
		(at 145.3123 114.42162 180)
		(property "Reference" "U1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "W5500_LQFP48"
			(at -3.08 -1.605644 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd oval
			(at -4.5 -2.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "NET_TXON")
		)
		(pad "2" smd oval
			(at -4.5 -2.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "NET_TXOP")
		)
		(pad "3" smd oval
			(at -4.5 -1.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "4" smd oval
			(at -4.5 -1.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "5" smd oval
			(at -4.5 -0.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "NET_RXIN")
		)
		(pad "6" smd oval
			(at -4.5 -0.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "NET_RXIP")
		)
		(pad "7" smd oval
			(at -4.5 0.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd oval
			(at -4.5 0.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "9" smd oval
			(at -4.5 1.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "10" smd oval
			(at -4.5 1.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "N34394983")
		)
		(pad "11" smd oval
			(at -4.5 2.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "12" smd oval
			(at -4.5 2.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "13" smd oval
			(at -2.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "14" smd oval
			(at -2.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "15" smd oval
			(at -1.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "16" smd oval
			(at -1.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "17" smd oval
			(at -0.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "18" smd oval
			(at -0.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "19" smd oval
			(at 0.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "20" smd oval
			(at 0.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "N34395115")
		)
		(pad "21" smd oval
			(at 1.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "22" smd oval
			(at 1.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "N34395146")
		)
		(pad "23" smd oval
			(at 2.25 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "N34395173")
		)
		(pad "24" smd oval
			(at 2.75 4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "25" smd oval
			(at 4.5 2.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "NET_LINK")
		)
		(pad "26" smd oval
			(at 4.5 2.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "27" smd oval
			(at 4.5 1.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "NET_ACTIVE")
		)
		(pad "28" smd oval
			(at 4.5 1.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "29" smd oval
			(at 4.5 0.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "30" smd oval
			(at 4.5 0.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "W55_XTIN")
		)
		(pad "31" smd oval
			(at 4.5 -0.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "W55_XTOUT")
		)
		(pad "32" smd oval
			(at 4.5 -0.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "A1_D1")
		)
		(pad "33" smd oval
			(at 4.5 -1.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "A8_D8_SCK")
		)
		(pad "34" smd oval
			(at 4.5 -1.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "A9_D9_MISO")
		)
		(pad "35" smd oval
			(at 4.5 -2.25 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "A10_D10_MOSI")
		)
		(pad "36" smd oval
			(at 4.5 -2.75 180)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "W55_INT")
		)
		(pad "37" smd oval
			(at 2.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "N34394975")
		)
		(pad "38" smd oval
			(at 2.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
		(pad "39" smd oval
			(at 1.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
		(pad "40" smd oval
			(at 1.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
		(pad "41" smd oval
			(at 0.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
		(pad "42" smd oval
			(at 0.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
		(pad "43" smd oval
			(at -0.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "N34394891")
		)
		(pad "44" smd oval
			(at -0.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "N34394891")
		)
		(pad "45" smd oval
			(at -1.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "N34394891")
		)
		(pad "46" smd oval
			(at -1.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "47" smd oval
			(at -2.25 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "48" smd oval
			(at -2.75 -4.5 270)
			(size 1.5 0.26)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 136.2699 113.45642 180)
		(property "Reference" "C3"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 2 "W55_XTIN")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 128.5483 115.94562 180)
		(property "Reference" "R24"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "N34391021")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 140.1307 107.30962 90)
		(property "Reference" "C28"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.71 0 90)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 149.8843 106.90322 90)
		(property "Reference" "C18"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 128.5483 114.98042 180)
		(property "Reference" "C27"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "N34391021")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 141.8579 121.27962)
		(property "Reference" "R9"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "N34394975")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 144.4995 121.27962 90)
		(property "Reference" "R8"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "N34394924")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 152.8307 113.96442 -90)
		(property "Reference" "ED3"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "NET_RXIP")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "NET_RXIN")
		)
	)
	(footprint "LED0603"
		(layer "F.Cu")
		(at 172.4395 119.70482 180)
		(property "Reference" "D2"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED0603"
			(at -1 1.664995 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.8 0 270)
			(size 1 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "N34429103")
		)
		(pad "2" smd rect
			(at 0.8 0 270)
			(size 1 0.7112)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 129.8183 101.31522 180)
		(property "Reference" "C42"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "HEADER_PIN_SIP10_2MM54"
		(layer "F.Cu")
		(at 113.7011 89.20362 90)
		(property "Reference" "CN3"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HEADER_PIN_SIP10_2MM54"
			(at 2.286 1.054894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VDD_5V")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "3V3")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "D17_SPI_SCK1")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "D18_SPI_MISO1")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "D19_SPI_MOSI1")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "A7_D7_RX")
			(thermal_bridge_angle 90)
		)
		(pad "8" thru_hole circle
			(at 0 17.78 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "A6_D6_TX")
			(thermal_bridge_angle 90)
		)
		(pad "9" thru_hole circle
			(at 0 20.32 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "A4_D4_SDA")
			(thermal_bridge_angle 90)
		)
		(pad "10" thru_hole circle
			(at 0 22.86 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "A5_D5_SCL")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 143.2803 121.33042 90)
		(property "Reference" "C5"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "N34394975")
		)
	)
	(footprint "TP_1MM2"
		(layer "F.Cu")
		(at 138.8607 93.08562)
		(property "Reference" "TP1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TP_1MM2"
			(at -1.0414 1.385094 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "POE_5V")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 138.2511 114.67562 -90)
		(property "Reference" "R6"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "W55_XTIN")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "W55_XTOUT")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 171.0425 100.41002)
		(property "Reference" "C23"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "N34403312")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "RJ45_VB2")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 170.1027 121.02562)
		(property "Reference" "R27"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "NET_LINK")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "N34439840")
		)
	)
	(footprint "PL_MWSA0402"
		(layer "F.Cu")
		(at 136.4223 108.73202)
		(property "Reference" "L1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PL_MWSA0402"
			(at -1.8 2.679425 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -1.9 0 90)
			(size 2.2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "N34390191")
		)
		(pad "2" smd rect
			(at 1.9 0 90)
			(size 2.2 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "POE_5V")
		)
	)
	(footprint "SOT-23-6"
		(layer "F.Cu")
		(at 131.3931 111.88162)
		(property "Reference" "U2"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SOT-23-6"
			(at 0.8128 -1.393805 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at 1.5 1)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "N34390191")
		)
		(pad "3" smd rect
			(at 1.5 -1)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
		)
		(pad "4" smd rect
			(at -1.5 -1)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "N34391021")
		)
		(pad "5" smd rect
			(at -1.5 0)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
		)
		(pad "6" smd rect
			(at -1.5 1)
			(size 1.016 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "N34390189")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 170.6869 92.57762 -90)
		(property "Reference" "C32"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.461106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "VDD_68V")
		)
		(pad "2" smd rect
			(at 0.475 0)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "PWRGND")
		)
	)
	(footprint "CON_RJ45_9803"
		(layer "F.Cu")
		(at 190.5011 105.00362 90)
		(property "Reference" "CN5"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CON_RJ45_9803"
			(at -1.7 -16.445548 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at -6.35 -5.4 90)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "" np_thru_hole circle
			(at 6.35 -5.4 90)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "F&B.Cu" "*.Mask")
			(thermal_bridge_angle 90)
		)
		(pad "1" thru_hole circle
			(at 3.57 -7.94 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "RJ45_TX2+")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 2.52901 -9.72 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "RJ45_TX2-")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 1.51301 -7.94 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "RJ45_RX2+")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0.49701 -9.72 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RJ45_VB1")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at -0.51899 -7.94 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RJ45_VB1")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at -1.53499 -9.72 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "RJ45_RX2-")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at -2.55099 -7.94 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RJ45_VB2")
			(thermal_bridge_angle 90)
		)
		(pad "8" thru_hole circle
			(at -3.57 -9.72 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RJ45_VB2")
			(thermal_bridge_angle 90)
		)
		(pad "9" thru_hole circle
			(at 6.86 -14.52 90)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "N34439840")
			(thermal_bridge_angle 90)
		)
		(pad "10" thru_hole circle
			(at 4.57 -14.52 90)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "3V3")
			(thermal_bridge_angle 90)
		)
		(pad "11" thru_hole circle
			(at -4.57 -14.52 90)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "N34439826")
			(thermal_bridge_angle 90)
		)
		(pad "12" thru_hole circle
			(at -6.86 -14.52 90)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "3V3")
			(thermal_bridge_angle 90)
		)
		(pad "13" thru_hole oval
			(at 8.12 -8.96 180)
			(size 3 2)
			(drill oval 2 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "GND_ETH")
		)
		(pad "14" thru_hole oval
			(at -8.12 -8.96 180)
			(size 3 2)
			(drill oval 2 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "GND_ETH")
		)
	)
	(footprint "EC_R6MM3_P2MM5"
		(layer "F.Cu")
		(at 131.7233 97.02262 180)
		(property "Reference" "CE1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "EC_R6MM3_P2MM5"
			(at -0.118894 -2.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "POE_12V")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 158.07758 116.55192)
		(property "Reference" "C14"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 21 "NET_RXIN")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "N34402995")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 134.3395 115.18362 90)
		(property "Reference" "C4"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 1 "W55_XTOUT")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 128.5483 114.01522)
		(property "Reference" "R25"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "N34391021")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 136.5239 111.83082 -90)
		(property "Reference" "C41"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 148.9191 106.95402 90)
		(property "Reference" "C10"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 129.8183 104.05842 180)
		(property "Reference" "C38"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 152.0179 110.45922)
		(property "Reference" "C1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 170.9425 104.11002 180)
		(property "Reference" "R22"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34403215")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "N34403291")
		)
	)
	(footprint "SWITCH_TSC017A06526A03"
		(layer "F.Cu")
		(at 181.0011 121.05362)
		(property "Reference" "CN4"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SWITCH_TSC017A06526A03"
			(at 2.6 -0.661106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.5 -1.85)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "ESP32_EN")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 1.5 -1.85)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "FB0603"
		(layer "F.Cu")
		(at 152.0179 107.61442 180)
		(property "Reference" "FB1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FB0603"
			(at -2.60807 0.513153 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.7874 0 180)
			(size 0.9652 0.762)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 170.9425 99.11002 180)
		(property "Reference" "R20"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "N34403215")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "N34403229")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 137.4383 111.83082 -90)
		(property "Reference" "C40"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 15 "POE_5V")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 158.5711 121.12722)
		(property "Reference" "R1"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "N34401385")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 177.58478 119.70152 90)
		(property "Reference" "ED1"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "ESP32_EN")
		)
	)
	(footprint "MARK"
		(layer "F.Cu")
		(at 109.8031 110.48462)
		(property "Reference" "MK3"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MARK"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.016 1.016)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.508)
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 129.8691 106.14122 180)
		(property "Reference" "C30"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -0.8 1.461106 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.71 0 180)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 129.8183 103.14402 180)
		(property "Reference" "C39"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.429226 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 16 "POE_12V")
		)
		(pad "2" smd rect
			(at 0.45 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "C0402M"
		(layer "F.Cu")
		(at 147.8523 106.95402 90)
		(property "Reference" "C13"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402M"
			(at -0.8 1.538894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.475 0 180)
			(size 0.65 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "R0603"
		(layer "F.Cu")
		(at 152.1195 109.18922)
		(property "Reference" "R18"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0603"
			(at -1.3 1.735005 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.8 0)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.8 0)
			(size 0.84 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "NET_TXCT")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 172.9475 118.43482)
		(property "Reference" "R5"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "N34429103")
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 140.6895 119.04442 -90)
		(property "Reference" "R13"
			(at 0 0.18669 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.401106 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "A1_D1")
		)
		(pad "2" smd rect
			(at 0.45 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "3V3")
		)
	)
	(footprint "C0603"
		(layer "F.Cu")
		(at 171.0425 97.81002)
		(property "Reference" "C20"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0603"
			(at -1.3 1.661208 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "N34403229")
		)
		(pad "2" smd rect
			(at 0.71 0)
			(size 0.86 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "RJ45_VA1")
		)
	)
	(footprint "HEADER_PIN_SIP10_2MM54"
		(layer "F.Cu")
		(at 113.7011 120.80362 90)
		(property "Reference" "CN2"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HEADER_PIN_SIP10_2MM54"
			(at 2.286 1.054894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "A0_D0")
			(thermal_bridge_angle 90)
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "D11_I2S_SD")
			(thermal_bridge_angle 90)
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "D12_I2S_SCK")
			(thermal_bridge_angle 90)
		)
		(pad "5" thru_hole circle
			(at 0 10.16 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "D13_I2S_WS")
			(thermal_bridge_angle 90)
		)
		(pad "6" thru_hole circle
			(at 0 12.7 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "D14_I2S_RX1")
			(thermal_bridge_angle 90)
		)
		(pad "7" thru_hole circle
			(at 0 15.24 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "D15_I2S_TX1")
			(thermal_bridge_angle 90)
		)
		(pad "8" thru_hole circle
			(at 0 17.78 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "A2_D2")
			(thermal_bridge_angle 90)
		)
		(pad "9" thru_hole circle
			(at 0 20.32 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "A3_D3")
			(thermal_bridge_angle 90)
		)
		(pad "10" thru_hole circle
			(at 0 22.86 90)
			(size 1.5748 1.5748)
			(drill 0.889)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "D16_ADC")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "R0402"
		(layer "F.Cu")
		(at 152.3227 120.67002 90)
		(property "Reference" "R2"
			(at 0 0.18669 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R0402"
			(at -0.83 1.478894 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "A0_D0")
		)
		(pad "2" smd rect
			(at 0.45 0 90)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "N34401469")
		)
	)
	(footprint "EC_R6MM3_P2MM5"
		(layer "F.Cu")
		(at 134.9237 103.06782 180)
		(property "Reference" "CE2"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "EC_R6MM3_P2MM5"
			(at -0.118894 -2.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "POE_12V")
			(thermal_bridge_angle 90)
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "GND")
			(thermal_bridge_angle 90)
		)
	)
	(footprint "C0402"
		(layer "F.Cu")
		(at 152.2211 115.79322)
		(property "Reference" "C12"
			(at 0 0.18669 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C0402"
			(at -0.78232 1.507014 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0)
			(net 61 "AVDD_3V3")
		)
		(pad "2" smd rect
			(at 0.45 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
	)
	(footprint "CRYSTAL_S2520"
		(layer "F.Cu")
		(at 136.2699 115.18362 180)
		(property "Reference" "X1"
			(at 0 0.18669 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CRYSTAL_S2520"
			(at -0.11 1.448792 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd rect
			(at -0.925 0.725 180)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "W55_XTIN")
		)
		(pad "2" smd rect
			(at 0.925 0.725 180)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(pad "3" smd rect
			(at 0.925 -0.725 180)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "W55_XTOUT")
		)
		(pad "4" smd rect
			(at -0.925 -0.725 180)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "GND")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 137.4699 116.08362) (xy 135.0699 116.08362) (xy 135.0699 114.28362) (xy 137.4699 114.28362)
				)
			)
		)
	)
	(gr_line
		(start 190.5011 89.20363)
		(end 190.5011 89.20362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.5011 89.20363)
		(end 106.5011 120.80362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.5011 87.20362)
		(end 108.5011 87.20362)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 108.5011 122.80362)
		(mid 107.086898 122.217834)
		(end 106.5011 120.80362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5011 120.80362)
		(end 190.5011 89.20363)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.5011 89.20362)
		(mid 107.086869 87.789378)
		(end 108.5011 87.20362)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.5011 89.20362)
		(end 106.5011 89.20363)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.5011 122.80362)
		(end 188.5011 122.80362)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 188.5011 87.20362)
		(mid 189.915289 87.789413)
		(end 190.5011 89.20362)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 190.5011 120.80362)
		(mid 189.915332 122.217869)
		(end 188.5011 122.80362)
		(layer "Edge.Cuts")
	)
	(gr_text "XIAO W5500 Ethernet Adapter"
		(at 171.2711 115.178975 360)
		(layer "B.SilkS")
	)
	(gr_text "D16"
		(at 137.195121 117.03782 90)
		(layer "B.SilkS")
	)
	(gr_text "D2"
		(at 132.182243 117.59662 90)
		(layer "B.SilkS")
	)
	(gr_text "D7"
		(at 129.667643 90.44402 90)
		(layer "B.SilkS")
	)
	(gr_text "D3"
		(at 134.604321 117.64742 90)
		(layer "B.SilkS")
	)
	(gr_text "D15"
		(at 129.667643 116.96162 90)
		(layer "B.SilkS")
	)
	(gr_text "POE Enable"
		(at 152.4751 97.729175 360)
		(layer "B.SilkS")
	)
	(gr_text "D6"
		(at 132.207643 90.46942 90)
		(layer "B.SilkS")
	)
	(gr_text "D0"
		(at 116.942243 117.62202 90)
		(layer "B.SilkS")
	)
	(gr_text "without 12V POE"
		(at 170.5799 121.610575 360)
		(layer "B.SilkS")
	)
	(gr_text "D14"
		(at 127.076843 116.96162 90)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 114.376843 90.49482 90)
		(layer "B.SilkS")
	)
	(gr_text "D13"
		(at 124.536843 116.91082 90)
		(layer "B.SilkS")
	)
	(gr_text "D17"
		(at 121.996843 90.44402 90)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 119.482243 90.46942 90)
		(layer "B.SilkS")
	)
	(gr_text "D11"
		(at 119.456843 116.96162 90)
		(layer "B.SilkS")
	)
	(gr_text "D18"
		(at 124.562243 90.44402 90)
		(layer "B.SilkS")
	)
	(gr_text "D4"
		(at 134.696843 90.46942 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 114.447643 116.25582 90)
		(layer "B.SilkS")
	)
	(gr_text "D12"
		(at 121.996843 116.91082 90)
		(layer "B.SilkS")
	)
	(gr_text "with 12V POE"
		(at 170.5799 118.511775 360)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 116.815243 90.46942 90)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 137.313043 90.46942 90)
		(layer "B.SilkS")
	)
	(gr_text "D19"
		(at 127.102243 90.44402 90)
		(layer "B.SilkS")
	)
	(gr_text "D5"
		(at 137.313043 92.85702 90)
		(layer "F.SilkS")
	)
	(gr_text "D14"
		(at 127.122243 119.20222 90)
		(layer "F.SilkS")
	)
	(gr_text "D7"
		(at 129.667643 92.83162 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 114.320643 119.15142 90)
		(layer "F.SilkS")
	)
	(gr_text "D19"
		(at 127.127643 93.61902 90)
		(layer "F.SilkS")
	)
	(gr_text "D18"
		(at 124.587643 93.61902 90)
		(layer "F.SilkS")
	)
	(gr_text "D4"
		(at 134.696843 92.85702 90)
		(layer "F.SilkS")
	)
	(gr_text "VDD_68V"
		(at 161.8731 92.249163 0)
		(layer "F.SilkS")
	)
	(gr_text "D6"
		(at 132.207643 92.85702 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 116.962243 94.15782 90)
		(layer "F.SilkS")
	)
	(gr_text "D15"
		(at 129.713043 119.20222 90)
		(layer "F.SilkS")
	)
	(gr_text "D3"
		(at 134.573521 119.25302 90)
		(layer "F.SilkS")
	)
	(gr_text "D0"
		(at 116.962243 119.15142 90)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 167.132643 102.58522 90)
		(layer "F.SilkS")
	)
	(gr_text "POWER"
		(at 171.2965 122.373563 0)
		(layer "F.SilkS")
	)
	(gr_text "USER"
		(at 159.6887 122.398963 0)
		(layer "F.SilkS")
	)
	(gr_text "D2"
		(at 132.151443 119.20222 90)
		(layer "F.SilkS")
	)
	(gr_text "PWRGND"
		(at 141.6801 92.350763 0)
		(layer "F.SilkS")
	)
	(gr_text "D17"
		(at 121.991443 93.64982 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 114.371443 92.73542 90)
		(layer "F.SilkS")
	)
	(gr_text "D16"
		(at 137.220521 119.19682 90)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 119.451443 93.54822 90)
		(layer "F.SilkS")
	)
	(gr_text "D12"
		(at 122.042243 119.15142 90)
		(layer "F.SilkS")
	)
	(gr_text "D11"
		(at 119.502243 119.20222 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 164.592643 102.53442 90)
		(layer "F.SilkS")
	)
	(gr_text "POE_12V"
		(at 141.7309 102.383763 0)
		(layer "F.SilkS")
	)
	(gr_text "D13"
		(at 124.587643 119.14602 90)
		(layer "F.SilkS")
	)
	(zone
		(net 16)
		(net_name "POE_12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 135.9016 99.48642) (xy 137.3875 99.48642) (xy 138.6575 100.75642) (xy 138.6575 101.31522) (xy 138.9623 101.62002)
				(xy 145.9727 101.62002) (xy 147.1919 102.83922) (xy 147.1919 105.17602) (xy 146.8617 105.50622)
				(xy 136.9557 105.50622) (xy 135.3047 103.85522) (xy 135.3047 100.08332)
			)
		)
	)
	(zone
		(net 5)
		(net_name "VDD_5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 112.8003 88.31042) (xy 112.8003 89.83442) (xy 108.7617 93.87302) (xy 108.7617 97.35282) (xy 111.6319 97.35282)
				(xy 111.6319 94.60962) (xy 114.9593 91.28222) (xy 114.9593 88.31042)
			)
		)
	)
	(zone
		(net 50)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 105.6067 86.28382) (xy 105.6067 124.38382) (xy 191.1031 124.38382) (xy 191.1031 86.28382)
			)
		)
	)
	(zone
		(net 73)
		(net_name "3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 117.9311 88.36122) (xy 117.9311 90.79962) (xy 114.0703 94.66042) (xy 114.0703 98.11482) (xy 114.4767 98.52122)
				(xy 115.734 98.52122) (xy 116.03245 98.22277) (xy 116.03245 94.42547) (xy 119.8615 90.59642) (xy 119.8615 88.36122)
			)
		)
	)
	(zone
		(net 16)
		(net_name "POE_12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 131.8757 95.93042) (xy 131.8757 98.24182) (xy 132.1043 98.47042) (xy 133.0187 98.47042) (xy 133.3743 98.82602)
				(xy 133.3743 99.56262) (xy 134.9999 101.18822) (xy 134.9999 103.55042) (xy 134.4411 104.10922) (xy 133.2727 104.10922)
				(xy 131.02004 101.85656) (xy 131.02004 101.16282) (xy 130.82557 100.96835) (xy 130.0723 100.96835)
				(xy 129.97507 101.06559) (xy 129.97507 106.49682) (xy 130.81108 107.33284) (xy 130.81108 109.64642)
				(xy 132.37209 111.20743) (xy 133.4251 111.20743) (xy 133.59601 111.03653) (xy 133.59601 107.61442)
				(xy 133.74841 107.46202) (xy 135.1015 107.46202) (xy 138.09063 104.47289) (xy 138.09063 99.09735)
				(xy 136.2191 97.22582) (xy 136.2191 96.71782) (xy 135.2285 95.72722) (xy 132.0789 95.72722)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.2754 120.244954) (xy 189.309766 120.27932) (xy 189.309766 120.32792) (xy 189.2754 120.362286)
				(xy 189.2511 120.36712) (xy 186.7511 120.36712) (xy 186.7268 120.362286) (xy 186.692434 120.32792)
				(xy 186.692434 120.27932) (xy 186.7268 120.244954) (xy 186.7511 120.24012) (xy 189.2511 120.24012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.5646 89.203618) (xy 106.552474 89.240943) (xy 106.520724 89.264012) (xy 106.481479 89.264013)
				(xy 106.449728 89.240946) (xy 106.4376 89.203622) (xy 106.455247 88.934277) (xy 106.507901 88.669539)
				(xy 106.59466 88.41394) (xy 106.71404 88.171852) (xy 106.863998 87.947417) (xy 107.041968 87.744477)
				(xy 107.244905 87.566503) (xy 107.469336 87.41654) (xy 107.711422 87.297156) (xy 107.967019 87.210392)
				(xy 108.231756 87.157733) (xy 108.5011 87.14008) (xy 108.5011 87.14012) (xy 108.538425 87.152248)
				(xy 108.561492 87.183998) (xy 108.561492 87.223243) (xy 108.538424 87.254993) (xy 108.5011 87.26712)
				(xy 108.5011 87.26708) (xy 108.374173 87.26708) (xy 108.122491 87.300213) (xy 107.877288 87.365916)
				(xy 107.642758 87.463062) (xy 107.422915 87.589989) (xy 107.221521 87.744527) (xy 107.042021 87.92403)
				(xy 106.887488 88.125428) (xy 106.760564 88.345273) (xy 106.663423 88.579805) (xy 106.597726 88.825009)
				(xy 106.564597 89.076692) (xy 106.5646 89.203618)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 188.5254 122.744954) (xy 188.559766 122.77932) (xy 188.559766 122.82792) (xy 188.5254 122.862286)
				(xy 188.5011 122.86712) (xy 108.5011 122.86712) (xy 108.4768 122.862286) (xy 108.442434 122.82792)
				(xy 108.442434 122.77932) (xy 108.4768 122.744954) (xy 108.5011 122.74012) (xy 188.5011 122.74012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 188.5254 87.144954) (xy 188.559766 87.17932) (xy 188.559766 87.22792) (xy 188.5254 87.262286)
				(xy 188.5011 87.26712) (xy 108.5011 87.26712) (xy 108.4768 87.262286) (xy 108.442434 87.22792) (xy 108.442434 87.17932)
				(xy 108.4768 87.144954) (xy 108.5011 87.14012) (xy 188.5011 87.14012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.2754 89.644954) (xy 110.309766 89.67932) (xy 110.309766 89.72792) (xy 110.2754 89.762286)
				(xy 110.2511 89.76712) (xy 107.7511 89.76712) (xy 107.7268 89.762286) (xy 107.692434 89.72792) (xy 107.692434 89.67932)
				(xy 107.7268 89.644954) (xy 107.7511 89.64012) (xy 110.2511 89.64012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.4376 120.803622) (xy 190.449726 120.766297) (xy 190.481476 120.743228) (xy 190.520721 120.743227)
				(xy 190.552472 120.766294) (xy 190.5646 120.803618) (xy 190.546953 121.072964) (xy 190.494299 121.337703)
				(xy 190.40754 121.593303) (xy 190.288161 121.835392) (xy 190.138203 122.059828) (xy 189.960234 122.26277)
				(xy 189.757297 122.440746) (xy 189.532866 122.59071) (xy 189.29078 122.710097) (xy 189.035182 122.796863)
				(xy 188.770446 122.849525) (xy 188.5011 122.86718) (xy 188.5011 122.86712) (xy 188.463776 122.854993)
				(xy 188.440708 122.823243) (xy 188.440708 122.783998) (xy 188.463775 122.752248) (xy 188.5011 122.74012)
				(xy 188.5011 122.74018) (xy 188.628027 122.740179) (xy 188.879709 122.707043) (xy 189.124913 122.641338)
				(xy 189.359443 122.54419) (xy 189.579286 122.41726) (xy 189.78068 122.262721) (xy 189.960179 122.083216)
				(xy 190.114713 121.881817) (xy 190.241636 121.661971) (xy 190.338777 121.427438) (xy 190.404474 121.182232)
				(xy 190.437603 120.930549) (xy 190.4376 120.803622)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.442434 89.17933) (xy 190.4768 89.144964) (xy 190.5254 89.144964) (xy 190.559766 89.17933)
				(xy 190.5646 89.20363) (xy 190.5646 120.80362) (xy 190.559766 120.82792) (xy 190.5254 120.862286)
				(xy 190.4768 120.862286) (xy 190.442434 120.82792) (xy 190.4376 120.80362) (xy 190.4376 89.20363)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.5011 122.74012) (xy 108.538424 122.752247) (xy 108.561492 122.783997) (xy 108.561492 122.823242)
				(xy 108.538425 122.854992) (xy 108.5011 122.86712) (xy 108.231761 122.849468) (xy 107.96703 122.79681)
				(xy 107.711437 122.710047) (xy 107.469356 122.590665) (xy 107.244929 122.440706) (xy 107.041996 122.262735)
				(xy 106.864029 122.059798) (xy 106.714074 121.835368) (xy 106.594697 121.593285) (xy 106.50794 121.33769)
				(xy 106.455287 121.072958) (xy 106.43764 120.803618) (xy 106.4376 120.803618) (xy 106.449728 120.766294)
				(xy 106.481479 120.743227) (xy 106.520724 120.743228) (xy 106.552474 120.766297) (xy 106.5646 120.803622)
				(xy 106.56464 120.803622) (xy 106.564637 120.930546) (xy 106.597765 121.182223) (xy 106.663461 121.427423)
				(xy 106.7606 121.661949) (xy 106.887521 121.88179) (xy 107.042052 122.083183) (xy 107.221547 122.262683)
				(xy 107.422938 122.417217) (xy 107.642776 122.544143) (xy 107.877301 122.641287) (xy 108.122499 122.706987)
				(xy 108.374176 122.74012) (xy 108.5011 122.74012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.2754 120.244954) (xy 110.309766 120.27932) (xy 110.309766 120.32792) (xy 110.2754 120.362286)
				(xy 110.2511 120.36712) (xy 107.7511 120.36712) (xy 107.7268 120.362286) (xy 107.692434 120.32792)
				(xy 107.692434 120.27932) (xy 107.7268 120.244954) (xy 107.7511 120.24012) (xy 110.2511 120.24012)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.442434 89.17933) (xy 106.4768 89.144964) (xy 106.5254 89.144964) (xy 106.559766 89.17933)
				(xy 106.5646 89.20363) (xy 106.5646 120.80362) (xy 106.559766 120.82792) (xy 106.5254 120.862286)
				(xy 106.4768 120.862286) (xy 106.442434 120.82792) (xy 106.4376 120.80362) (xy 106.4376 89.20363)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 188.5011 87.26712) (xy 188.463775 87.254992) (xy 188.440708 87.223242) (xy 188.440708 87.183997)
				(xy 188.463776 87.152247) (xy 188.5011 87.14012) (xy 188.770438 87.157775) (xy 189.035167 87.210435)
				(xy 189.290757 87.297199) (xy 189.532836 87.416582) (xy 189.757261 87.566542) (xy 189.960191 87.744512)
				(xy 190.138156 87.947449) (xy 190.288109 88.171878) (xy 190.407485 88.41396) (xy 190.494241 88.669553)
				(xy 190.546893 88.934283) (xy 190.56454 89.203622) (xy 190.5646 89.203622) (xy 190.552472 89.240946)
				(xy 190.520721 89.264013) (xy 190.481476 89.264012) (xy 190.449726 89.240943) (xy 190.4376 89.203618)
				(xy 190.43754 89.203618) (xy 190.437543 89.076695) (xy 190.404415 88.82502) (xy 190.33872 88.579821)
				(xy 190.241582 88.345296) (xy 190.114663 88.125456) (xy 189.960134 87.924063) (xy 189.78064 87.744564)
				(xy 189.579253 87.590029) (xy 189.359416 87.463104) (xy 189.124894 87.365958) (xy 188.879698 87.300256)
				(xy 188.628023 87.267121) (xy 188.5011 87.26712)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.2754 89.644954) (xy 189.309766 89.67932) (xy 189.309766 89.72792) (xy 189.2754 89.762286)
				(xy 189.2511 89.76712) (xy 186.7511 89.76712) (xy 186.7268 89.762286) (xy 186.692434 89.72792) (xy 186.692434 89.67932)
				(xy 186.7268 89.644954) (xy 186.7511 89.64012) (xy 189.2511 89.64012)
			)
		)
	)
	(zone
		(net 50)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill
			(thermal_gap 0.254)
			(thermal_bridge_width 0.381)
		)
		(polygon
			(pts
				(xy 104.9463 85.11542) (xy 104.9463 125.29822) (xy 192.0683 125.29822) (xy 192.0683 85.11542)
			)
		)
	)
)
