(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XIAO-ESP32-C3-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.016 2.794 0)
		)
		(property "Value" "XIAO-ESP32-C3-DIP"
			(at 7.62 1.016 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 16.764 -29.464 0)
		)
		(property "Datasheet" ""
			(at 1.27 1.27 0)
		)
		(property "Description" ""
			(at 1.27 1.27 0)
		)
		(symbol "XIAO-ESP32-C3-DIP_1_0"
			(pin passive line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "GPIO2/A0/D0")
				(number "1")
			)
			(pin passive line
				(at -2.54 -6.35 0)
				(length 2.54)
				(name "GPIO3/A1/D1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "GPIO4/A2/D2")
				(number "3")
			)
			(pin passive line
				(at -2.54 -13.97 0)
				(length 2.54)
				(name "GPIO5/A3/D3")
				(number "4")
			)
			(pin passive line
				(at -2.54 -17.78 0)
				(length 2.54)
				(name "GPIO6/D4/SDA")
				(number "5")
			)
			(pin passive line
				(at -2.54 -21.59 0)
				(length 2.54)
				(name "GPIO7/D5/SCL")
				(number "6")
			)
			(pin passive line
				(at -2.54 -25.4 0)
				(length 2.54)
				(name "GPIO21/D6/TX")
				(number "7")
			)
			(pin passive line
				(at 35.56 -2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 35.56 -6.35 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 35.56 -10.16 180)
				(length 2.54)
				(name "VCC_3V3")
				(number "12")
			)
			(pin passive line
				(at 35.56 -13.97 180)
				(length 2.54)
				(name "GPIO10/D10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 35.56 -17.78 180)
				(length 2.54)
				(name "GPIO9/D9/MISO")
				(number "10")
			)
			(pin passive line
				(at 35.56 -21.59 180)
				(length 2.54)
				(name "GPIO8/D8/SCK")
				(number "9")
			)
			(pin passive line
				(at 35.56 -25.4 180)
				(length 2.54)
				(name "GPIO20/D7/RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-C3-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-C3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C3-SMD_0_1")
		(symbol "XIAO-ESP32-C3-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "GPIO2_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "GPIO3_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "GPIO4_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "GPIO5_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "GPIO6_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "GPIO7_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "GPIO21_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -10.16 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "24")
			)
			(pin passive line
				(at -6.35 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "25")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "26")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "32")
			)
			(pin passive line
				(at 1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "28")
			)
			(pin passive line
				(at 8.89 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "29")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "GPIO10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "GPIO9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "GPIO8_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "GPIO20_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-C6-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.16 0)
		)
		(property "Value" "XIAO ESP32C6"
			(at 0 0 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C6-DIP_0_1")
		(symbol "XIAO-ESP32-C6-DIP_1_1"
			(pin passive line
				(at -20.32 6.35 0)
				(length 2.54)
				(name "GPIO0_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "GPIO1_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -20.32 -1.27 0)
				(length 2.54)
				(name "GPIO2_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "GPIO21_D3")
				(number "4")
			)
			(pin passive line
				(at -20.32 -8.89 0)
				(length 2.54)
				(name "GPIO22_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "GPIO23_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -20.32 -16.51 0)
				(length 2.54)
				(name "GPIO16_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 17.78 6.35 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 17.78 -1.27 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO18_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 17.78 -8.89 180)
				(length 2.54)
				(name "GPIO20_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO19_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 17.78 -16.51 180)
				(length 2.54)
				(name "GPIO17_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-C6-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-C6-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C6-SMD_0_1")
		(symbol "XIAO-ESP32-C6-SMD_1_1"
			(pin passive line
				(at -21.59 10.16 0)
				(length 2.54)
				(name "GPIO0_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 6.35 0)
				(length 2.54)
				(name "GPIO1_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 2.54 0)
				(length 2.54)
				(name "GPIO2_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 -1.27 0)
				(length 2.54)
				(name "GPIO21_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -5.08 0)
				(length 2.54)
				(name "GPIO22_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -8.89 0)
				(length 2.54)
				(name "GPIO23_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -12.7 0)
				(length 2.54)
				(name "GPIO16_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -12.7 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "24")
			)
			(pin passive line
				(at -8.89 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "25")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "26")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "32")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "28")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "29")
			)
			(pin passive line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "BOOT")
				(number "30")
			)
			(pin passive line
				(at 13.97 22.86 270)
				(length 2.54)
				(name "3V3")
				(number "31")
			)
			(pin passive line
				(at 21.59 10.16 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 21.59 6.35 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 2.54 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 -1.27 180)
				(length 2.54)
				(name "GPIO18_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 -5.08 180)
				(length 2.54)
				(name "GPIO20_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 -8.89 180)
				(length 2.54)
				(name "GPIO19_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 21.59 -12.7 180)
				(length 2.54)
				(name "GPIO17_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-S3 Plus-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U2"
			(at -20.828 17.018 0)
		)
		(property "Value" "XIAO-HALF-HOLE-23P"
			(at -12.446 14.986 0)
		)
		(property "Footprint" "Module:MOUDLE23P-XIAO-HALF-HOLE"
			(at -1.016 -35.306 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "XIAO-HALF-HOLE-23P"
			(at -1.524 -33.02 0)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
		)
		(property "MPN" ""
			(at 0 0 0)
		)
		(property "SKU" "XIAO-HALF-HOLE-23P"
			(at 6.604 -9.652 0)
		)
		(property "Part Type" ""
			(at 0 0 0)
		)
		(property "Rating" ""
			(at 0 0 0)
		)
		(property "Status" ""
			(at 0 0 0)
		)
		(property "Temperature" ""
			(at 0 0 0)
		)
		(property "Priority" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Module:MOUDLE23P-XIAO-HALF-HOLE"
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3 Plus-SMD_0_1")
		(symbol "XIAO-ESP32-S3 Plus-SMD_1_0"
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "GPIO1_D0/A0")
				(number "1")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "GPIO2_D1/A1")
				(number "2")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "GPIO3_D2/A2")
				(number "3")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "GPIO4_D3/A3")
				(number "4")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "GPIO5_D4/A4/I2C_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "GPIO6_D5/A5/I2C_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "U0TXD_D6/TX")
				(number "7")
			)
			(pin passive line
				(at 36.83 11.43 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 36.83 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 36.83 3.81 180)
				(length 2.54)
				(name "VCC_3V3")
				(number "12")
			)
			(pin passive line
				(at 36.83 0 180)
				(length 2.54)
				(name "GPIO9_D10/A10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 36.83 -3.81 180)
				(length 2.54)
				(name "GPIO8_D9/A9/MISO")
				(number "10")
			)
			(pin passive line
				(at 36.83 -7.62 180)
				(length 2.54)
				(name "GPIO7_D8/A8/SCK")
				(number "9")
			)
			(pin passive line
				(at 36.83 -11.43 180)
				(length 2.54)
				(name "U0RXD_D7/RX")
				(number "8")
			)
		)
		(symbol "XIAO-ESP32-S3 Plus-SMD_1_1"
			(pin passive line
				(at -24.13 -16.51 0)
				(length 2.54)
				(name "GPIO38_DVP_VSYNC/I2S_SD")
				(number "15")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "GPIO39_CAM_SCL/I2S_SCK")
				(number "16")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 2.54)
				(name "GPIO40_CAM_SDA/I2S_WS")
				(number "17")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 2.54)
				(name "GPIO41_PDM_DATA/RX1")
				(number "18")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "GPIO42_PDM_CLK/TX1")
				(number "19")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 2.54)
				(name "GPIO10_XMCLK/ADC_BAT")
				(number "20")
			)
			(pin passive line
				(at 36.83 -16.51 180)
				(length 2.54)
				(name "GPIO11_DVP_Y8/SPI_MOSI1")
				(number "21")
			)
			(pin passive line
				(at 36.83 -19.05 180)
				(length 2.54)
				(name "GPIO12_DVP_Y7/SPI_MISO1")
				(number "22")
			)
			(pin passive line
				(at 36.83 -21.59 180)
				(length 2.54)
				(name "GPIO13_DVP_PCLK/SPI_SCK1")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-S3 Plus-SMD_33P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U2"
			(at -20.828 17.018 0)
		)
		(property "Value" "XIAO-HALF-HOLE-33P"
			(at -12.446 14.986 0)
		)
		(property "Footprint" "Seeed_Studio_XIAO_Series:XIAO-ESP32-S3-Plus-SMD"
			(at 9.652 6.604 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "XIAO-HALF-HOLE-33P"
			(at 7.366 2.286 0)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
		)
		(property "MPN" ""
			(at 0 0 0)
		)
		(property "SKU" "XIAO-HALF-HOLE-33P"
			(at 6.604 -9.652 0)
		)
		(property "Part Type" ""
			(at 0 0 0)
		)
		(property "Rating" ""
			(at 0 0 0)
		)
		(property "Status" ""
			(at 0 0 0)
		)
		(property "Temperature" ""
			(at 0 0 0)
		)
		(property "Priority" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Module:MOUDLE23P-XIAO-HALF-HOLE"
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3 Plus-SMD_33P_0_1")
		(symbol "XIAO-ESP32-S3 Plus-SMD_33P_1_0"
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "GPIO1_D0/A0")
				(number "1")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "GPIO2_D1/A1")
				(number "2")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "GPIO3_D2/A2")
				(number "3")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "GPIO4_D3/A3")
				(number "4")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "GPIO5_D4/A4/I2C_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "GPIO6_D5/A5/I2C_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "U0TXD_D6/TX")
				(number "7")
			)
			(pin passive line
				(at 36.83 11.43 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 36.83 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 36.83 3.81 180)
				(length 2.54)
				(name "VCC_3V3")
				(number "12")
			)
			(pin passive line
				(at 36.83 0 180)
				(length 2.54)
				(name "GPIO9_D10/A10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 36.83 -3.81 180)
				(length 2.54)
				(name "GPIO8_D9/A9/MISO")
				(number "10")
			)
			(pin passive line
				(at 36.83 -7.62 180)
				(length 2.54)
				(name "GPIO7_D8/A8/SCK")
				(number "9")
			)
			(pin passive line
				(at 36.83 -11.43 180)
				(length 2.54)
				(name "U0RXD_D7/RX")
				(number "8")
			)
		)
		(symbol "XIAO-ESP32-S3 Plus-SMD_33P_1_1"
			(pin passive line
				(at -24.13 -16.51 0)
				(length 2.54)
				(name "GPIO38_DVP_VSYNC/I2S_SD")
				(number "15")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "GPIO39_CAM_SCL/I2S_SCK")
				(number "16")
			)
			(pin passive line
				(at -24.13 -21.59 0)
				(length 2.54)
				(name "GPIO40_CAM_SDA/I2S_WS")
				(number "17")
			)
			(pin passive line
				(at -24.13 -24.13 0)
				(length 2.54)
				(name "GPIO41_PDM_DATA/RX1")
				(number "18")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "GPIO42_PDM_CLK/TX1")
				(number "19")
			)
			(pin passive line
				(at -24.13 -29.21 0)
				(length 2.54)
				(name "GPIO10_XMCLK/ADC_BAT")
				(number "20")
			)
			(pin passive line
				(at -24.13 -38.1 0)
				(length 2.54)
				(name "VBAT")
				(number "32")
			)
			(pin passive line
				(at -24.13 -40.64 0)
				(length 2.54)
				(name "GND2")
				(number "33")
			)
			(pin passive line
				(at -24.13 -45.72 0)
				(length 2.54)
				(name "PAD")
				(number "34")
			)
			(pin passive line
				(at 36.83 -16.51 180)
				(length 2.54)
				(name "GPIO11_DVP_Y8/SPI_MOSI1")
				(number "21")
			)
			(pin passive line
				(at 36.83 -19.05 180)
				(length 2.54)
				(name "GPIO12_DVP_Y7/SPI_MISO1")
				(number "22")
			)
			(pin passive line
				(at 36.83 -21.59 180)
				(length 2.54)
				(name "GPIO13_DVP_PCLK/SPI_SCK1")
				(number "23")
			)
			(pin passive line
				(at 36.83 -27.94 180)
				(length 2.54)
				(name "MTDI/IO41/PDM_DATA/RX1")
				(number "24")
			)
			(pin passive line
				(at 36.83 -30.48 180)
				(length 2.54)
				(name "MTDO/IO40/CAM_SDA/I2S_WS")
				(number "25")
			)
			(pin passive line
				(at 36.83 -33.02 180)
				(length 2.54)
				(name "EN")
				(number "26")
			)
			(pin passive line
				(at 36.83 -35.56 180)
				(length 2.54)
				(name "GND1")
				(number "27")
			)
			(pin passive line
				(at 36.83 -38.1 180)
				(length 2.54)
				(name "MTMS/IO42/PDM_CLK/TX1")
				(number "28")
			)
			(pin passive line
				(at 36.83 -40.64 180)
				(length 2.54)
				(name "MTCK/IO39/CAM_SCL/I2S_SCK")
				(number "29")
			)
			(pin passive line
				(at 36.83 -43.18 180)
				(length 2.54)
				(name "ESP_USB_D-")
				(number "30")
			)
			(pin passive line
				(at 36.83 -45.72 180)
				(length 2.54)
				(name "ESP_USB_D+")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-S3-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 0.508 0)
		)
		(property "Value" "XIAO-ESP32-S3-DIP"
			(at 9.652 -1.778 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 17.018 -31.75 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3-DIP_1_0"
			(pin passive line
				(at -2.54 -5.08 0)
				(length 2.54)
				(name "GPIO1/D0/A0")
				(number "1")
			)
			(pin passive line
				(at -2.54 -8.89 0)
				(length 2.54)
				(name "GPIO2/DA/A1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "GPIO3/D2/A2")
				(number "3")
			)
			(pin passive line
				(at -2.54 -16.51 0)
				(length 2.54)
				(name "GPIO4/D3/A3")
				(number "4")
			)
			(pin passive line
				(at -2.54 -20.32 0)
				(length 2.54)
				(name "GPIO5/D4/I2C_SDA")
				(number "5")
			)
			(pin passive line
				(at -2.54 -24.13 0)
				(length 2.54)
				(name "GPIO9/D5/I2C_SCL")
				(number "6")
			)
			(pin passive line
				(at -2.54 -27.94 0)
				(length 2.54)
				(name "U0TXD/D6/TX")
				(number "7")
			)
			(pin passive line
				(at 44.45 -5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 44.45 -8.89 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 44.45 -12.7 180)
				(length 2.54)
				(name "VCC_3V3")
				(number "12")
			)
			(pin passive line
				(at 44.45 -16.51 180)
				(length 2.54)
				(name "GPIO9/D10/A10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 44.45 -20.32 180)
				(length 2.54)
				(name "GPIO8/D9/A9/MISO")
				(number "10")
			)
			(pin passive line
				(at 44.45 -24.13 180)
				(length 2.54)
				(name "GPIO7/D8/A8/SCK")
				(number "9")
			)
			(pin passive line
				(at 44.45 -27.94 180)
				(length 2.54)
				(name "U0RXD/D7/RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-ESP32-S3-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-S3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3-SMD_0_1")
		(symbol "XIAO-ESP32-S3-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "GPIO1_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "GPIO2_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "GPIO3_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "GPIO4_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "GPIO5_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "GPIO6_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "GPIO43_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -12.7 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "24")
			)
			(pin passive line
				(at -8.89 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "25")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "26")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "32")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "28")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "29")
			)
			(pin passive line
				(at 7.62 -21.59 90)
				(length 2.54)
				(name "PAD")
				(number "34")
			)
			(pin passive line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "USB_DN")
				(number "30")
			)
			(pin passive line
				(at 13.97 22.86 270)
				(length 2.54)
				(name "USB_DP")
				(number "31")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "GPIO9_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "GPIO8_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "GPIO7_A8_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "GPIO44_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-MG24-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.508 0 0)
		)
		(property "Value" "XIAO-MG24-DIP"
			(at 7.366 -2.286 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 16.002 -33.782 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-MG24-DIP_1_0"
			(pin passive line
				(at -2.54 -6.35 0)
				(length 2.54)
				(name "PC00/A0/D0")
				(number "1")
			)
			(pin passive line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "PC01/A1/D1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -13.97 0)
				(length 2.54)
				(name "PC02/A2/D2")
				(number "3")
			)
			(pin passive line
				(at -2.54 -17.78 0)
				(length 2.54)
				(name "PC03/A3/D3")
				(number "4")
			)
			(pin passive line
				(at -2.54 -21.59 0)
				(length 2.54)
				(name "PC04/A4/D4/SDA")
				(number "5")
			)
			(pin passive line
				(at -2.54 -25.4 0)
				(length 2.54)
				(name "PC05/A5/D5/SCL")
				(number "6")
			)
			(pin passive line
				(at -2.54 -29.21 0)
				(length 2.54)
				(name "PC06/A6/D6/TX")
				(number "7")
			)
			(pin passive line
				(at 43.18 -6.35 180)
				(length 2.54)
				(name "VIN")
				(number "14")
			)
			(pin passive line
				(at 43.18 -10.16 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 43.18 -13.97 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 43.18 -17.78 180)
				(length 2.54)
				(name "PA05/A10/D10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 43.18 -21.59 180)
				(length 2.54)
				(name "PA04/A9/D9/MISO")
				(number "10")
			)
			(pin passive line
				(at 43.18 -25.4 180)
				(length 2.54)
				(name "PA03/A8/D8/SCLK")
				(number "9")
			)
			(pin passive line
				(at 43.18 -29.21 180)
				(length 2.54)
				(name "PC07/A7/D7/RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-MG24-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 27.432 0)
		)
		(property "Value" "XIAO-MG24-SMD"
			(at -21.59 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-MG24-SMD_0_1")
		(symbol "XIAO-MG24-SMD_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "PC00_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "PC01_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "PC02_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "PC03_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "PC04_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "PC05_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "PC06_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "PC07_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "PA03_A8_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "PA04_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "PA05_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
		)
		(symbol "XIAO-MG24-SMD_1_1"
			(pin passive line
				(at -24.13 -30.48 0)
				(length 2.54)
				(name "BAT")
				(number "31")
			)
			(pin passive line
				(at -24.13 -34.29 0)
				(length 2.54)
				(name "GND_2")
				(number "32")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWCLK")
				(number "30")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_1")
				(number "29")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "3V3_1")
				(number "28")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "SAMD11_SWCLK")
				(number "27")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "SAMD11_SWDIO")
				(number "26")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "SAMD11_RST")
				(number "25")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "MG24_RST")
				(number "24")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "PD02_A18_D18")
				(number "22")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "PA00_A17_D17_SCK1")
				(number "21")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "PB01_A16_D16_MISO1")
				(number "20")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "PB00_A15_D15_MOSI1")
				(number "19")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "PB02_A14_D14_SDA1")
				(number "18")
			)
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "PB02_A13_D13_SCL1")
				(number "17")
			)
			(pin passive line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PA08_A12_D12_SAMD11_RX")
				(number "16")
			)
			(pin passive line
				(at 25.4 -34.29 180)
				(length 2.54)
				(name "PA08_A11_D11_SAMD11_TX")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RA4M1-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0.762 0.254 0)
		)
		(property "Value" "XIAO-RA4M1-DIP"
			(at 5.588 -1.524 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 16.51 -32.004 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RA4M1-DIP_1_0"
			(pin passive line
				(at -2.54 -5.08 0)
				(length 2.54)
				(name "P500/P014/AN09/DAC")
				(number "1")
			)
			(pin passive line
				(at -2.54 -8.89 0)
				(length 2.54)
				(name "P000/ADC00/AMP0+")
				(number "2")
			)
			(pin passive line
				(at -2.54 -12.7 0)
				(length 2.54)
				(name "P001/ADC01/AMP0-")
				(number "3")
			)
			(pin passive line
				(at -2.54 -16.51 0)
				(length 2.54)
				(name "P002/ADC02/AMP0O")
				(number "4")
			)
			(pin passive line
				(at -2.54 -20.32 0)
				(length 2.54)
				(name "P206/SDA1")
				(number "5")
			)
			(pin passive line
				(at -2.54 -24.13 0)
				(length 2.54)
				(name "P100/ADC22/SCL1")
				(number "6")
			)
			(pin passive line
				(at -2.54 -27.94 0)
				(length 2.54)
				(name "P302/TXD2")
				(number "7")
			)
			(pin passive line
				(at 38.1 -5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 38.1 -8.89 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 38.1 -12.7 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 38.1 -16.51 180)
				(length 2.54)
				(name "P109/MOSI9")
				(number "11")
			)
			(pin passive line
				(at 38.1 -20.32 180)
				(length 2.54)
				(name "P110/MISO9")
				(number "10")
			)
			(pin passive line
				(at 38.1 -24.13 180)
				(length 2.54)
				(name "P111/SCK9")
				(number "9")
			)
			(pin passive line
				(at 38.1 -27.94 180)
				(length 2.54)
				(name "P301/RXD2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RA4M1-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.844 27.432 0)
		)
		(property "Value" "XIAO-RA4M1-SMD"
			(at -21.844 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-RA4M1-SMD_0_1")
		(symbol "XIAO-RA4M1-SMD_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "P014_AN09_DAC")
				(number "1")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "P000_ADC00_AMP0+")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "P001_ADC01_AMP0-")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "P002_ADC02_AMP00")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "P206_SDA1")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "P100_ADC22_SCL1")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "P302_TXD2")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "P301_RXD2")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "P111_SCK9")
				(number "9")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "P110_MISO9")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "P109_MOSI9")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
		)
		(symbol "XIAO-RA4M1-SMD_1_1"
			(pin passive line
				(at -2.54 -31.75 90)
				(length 2.54)
				(name "BAT")
				(number "29")
			)
			(pin passive line
				(at 2.54 -31.75 90)
				(length 2.54)
				(name "GND_2")
				(number "30")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWDCLK")
				(number "28")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_1")
				(number "27")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "3V3_1")
				(number "26")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "BOOT")
				(number "25")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RST")
				(number "24")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "P103_SS0")
				(number "22")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "P102_SCK0")
				(number "21")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "P104_MISO0")
				(number "20")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "P101_ADC21_MOSI0")
				(number "19")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "P012")
				(number "18")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "P013")
				(number "17")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "P409_TX9")
				(number "16")
			)
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "P408_RX9")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RP2040-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "XIAO-RP2040-DIP"
			(at 5.334 -1.778 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 14.478 -32.258 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RP2040-DIP_1_0"
			(pin passive line
				(at -3.81 -5.08 0)
				(length 2.54)
				(name "GPIO26/ADC0/A0")
				(number "1")
			)
			(pin passive line
				(at -3.81 -8.89 0)
				(length 2.54)
				(name "GPIO27/ADC1/A1")
				(number "2")
			)
			(pin passive line
				(at -3.81 -12.7 0)
				(length 2.54)
				(name "GPIO28/ADC2/A2")
				(number "3")
			)
			(pin passive line
				(at -3.81 -16.51 0)
				(length 2.54)
				(name "GPIO29/ADC3/A3")
				(number "4")
			)
			(pin passive line
				(at -3.81 -20.32 0)
				(length 2.54)
				(name "GPIO6/SDA")
				(number "5")
			)
			(pin passive line
				(at -3.81 -24.13 0)
				(length 2.54)
				(name "GPIO7/SCL")
				(number "6")
			)
			(pin passive line
				(at -3.81 -27.94 0)
				(length 2.54)
				(name "GPIO0/TX")
				(number "7")
			)
			(pin passive line
				(at 31.75 -5.08 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 31.75 -8.89 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 31.75 -12.7 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 31.75 -16.51 180)
				(length 2.54)
				(name "GPIO3/MOSI")
				(number "11")
			)
			(pin passive line
				(at 31.75 -20.32 180)
				(length 2.54)
				(name "GPIO4/MISO")
				(number "10")
			)
			(pin passive line
				(at 31.75 -24.13 180)
				(length 2.54)
				(name "GPIO2/SCK")
				(number "9")
			)
			(pin passive line
				(at 31.75 -27.94 180)
				(length 2.54)
				(name "GPIO1/RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RP2040-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-RP2040-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RP2040-SMD_0_1")
		(symbol "XIAO-RP2040-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "GPIO26_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "GPIO27_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "GPIO28_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "GPIO29_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "GPIO6_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "GPIO7_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "GPIO0_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -6.35 22.86 270)
				(length 2.54)
				(name "SWDIO")
				(number "24")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "SWDCLK")
				(number "25")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "32")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RST")
				(number "26")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "GPIO3_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "GPIO4_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "GPIO2_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "GPIO1_D7_CSn_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RP2350-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.588 2.032 0)
		)
		(property "Value" "XIAO-RP2350-DIP"
			(at 0 0 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 11.684 -30.734 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RP2350-DIP_1_0"
			(pin passive line
				(at -8.89 -3.81 0)
				(length 2.54)
				(name "GPIO26/D0/ADC0")
				(number "1")
			)
			(pin passive line
				(at -8.89 -7.62 0)
				(length 2.54)
				(name "GPIO27/D1/ADC1")
				(number "2")
			)
			(pin passive line
				(at -8.89 -11.43 0)
				(length 2.54)
				(name "GPIO28/D2/ADC2")
				(number "3")
			)
			(pin passive line
				(at -8.89 -15.24 0)
				(length 2.54)
				(name "GPIO5/D3/SPI_CS")
				(number "4")
			)
			(pin passive line
				(at -8.89 -19.05 0)
				(length 2.54)
				(name "GPIO6/D4/SDA1")
				(number "5")
			)
			(pin passive line
				(at -8.89 -22.86 0)
				(length 2.54)
				(name "GPIO7/D5/SCL1")
				(number "6")
			)
			(pin passive line
				(at -8.89 -26.67 0)
				(length 2.54)
				(name "GPIO0/D6/TX0")
				(number "7")
			)
			(pin passive line
				(at 39.37 -3.81 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 39.37 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 39.37 -11.43 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 39.37 -15.24 180)
				(length 2.54)
				(name "GPIO3/D10/SPI0_MOSI")
				(number "11")
			)
			(pin passive line
				(at 39.37 -19.05 180)
				(length 2.54)
				(name "GPIO4/D9/SPI_MISO")
				(number "10")
			)
			(pin passive line
				(at 39.37 -22.86 180)
				(length 2.54)
				(name "GPIO2/D8/SPI0_SCK")
				(number "9")
			)
			(pin passive line
				(at 39.37 -26.67 180)
				(length 2.54)
				(name "GPIO1/D7/RX0")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-RP2350-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 27.432 0)
		)
		(property "Value" "XIAO-RP2350-SMD"
			(at -21.59 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-RP2350-SMD_0_1")
		(symbol "XIAO-RP2350-SMD_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "GPIO26/D0/ADC0")
				(number "1")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "GPIO27/D1/ADC1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "GPIO28/D2/ADC2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "GPIO5/D3/SPI0_CS")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "GPIO6/D4/SDA1")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "GPIO7/D5/SCL1")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "GPIO0/D6/TXO")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "GPIO1/D7/RX0")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "GPIO2/D8/SPI0_SCK")
				(number "9")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "GPIO4/D9/SPI0_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "GPIO3/D10/SPI0_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
		)
		(symbol "XIAO-RP2350-SMD_1_1"
			(pin passive line
				(at -2.54 -31.75 90)
				(length 2.54)
				(name "BAT")
				(number "29")
			)
			(pin passive line
				(at 2.54 -31.75 90)
				(length 2.54)
				(name "GND_2")
				(number "30")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWDCLK")
				(number "28")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_1")
				(number "27")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "3V3_1")
				(number "26")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "BOOT")
				(number "25")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RST")
				(number "24")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO9/D18/SPI1_CS")
				(number "22")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO10/D17/SPI1_SCK")
				(number "21")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO12/D16/SPI1_MISO")
				(number "20")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO11/D15/SPI1_MOSI")
				(number "19")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO16/D14/SDA0")
				(number "18")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "GPIO17/D13/SCL0")
				(number "17")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIO20/D12/TX1")
				(number "16")
			)
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "GPIO21/D11/RX1")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-SAMD21-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 22.86 0)
		)
		(property "Value" "XIAO-SAMD21-DIP"
			(at -10.16 21.082 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-SAMD21-DIP_0_1")
		(symbol "XIAO-SAMD21-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-SAMD21-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-SAMD21-SMD"
			(at -9.906 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-SAMD21-SMD_0_1")
		(symbol "XIAO-SAMD21-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "PA31_SWDIO")
				(number "24")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "VIN")
				(number "32")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "PA30_SWCLK")
				(number "25")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RESET")
				(number "26")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-nRF52840-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.048 1.778 0)
		)
		(property "Value" "XIAO-nRF52840-DIP"
			(at 3.048 -0.254 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 12.7 -30.734 0)
		)
		(property "Datasheet" ""
			(at -3.81 2.54 0)
		)
		(property "Description" ""
			(at -3.81 2.54 0)
		)
		(symbol "XIAO-nRF52840-DIP_1_0"
			(pin passive line
				(at -6.35 -3.81 0)
				(length 2.54)
				(name "P0.02_AIN0_LOW_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -6.35 -7.62 0)
				(length 2.54)
				(name "P0.03_AIN1_LOW_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -6.35 -11.43 0)
				(length 2.54)
				(name "P0.28_AIN4_LOW_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -6.35 -15.24 0)
				(length 2.54)
				(name "P0.29_AIN5_LOW_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -6.35 -19.05 0)
				(length 2.54)
				(name "P0.04_AIN2_A4_D4")
				(number "5")
			)
			(pin passive line
				(at -6.35 -22.86 0)
				(length 2.54)
				(name "P0.05_AIN3_A5_D5")
				(number "6")
			)
			(pin passive line
				(at -6.35 -26.67 0)
				(length 2.54)
				(name "P1.11_TX_D6")
				(number "7")
			)
			(pin passive line
				(at 41.91 -3.81 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 41.91 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 41.91 -11.43 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 41.91 -15.24 180)
				(length 2.54)
				(name "P1.15_MOSI_D10")
				(number "11")
			)
			(pin passive line
				(at 41.91 -19.05 180)
				(length 2.54)
				(name "P1.14_MISO_D9")
				(number "10")
			)
			(pin passive line
				(at 41.91 -22.86 180)
				(length 2.54)
				(name "P1.13_SCK_D8")
				(number "9")
			)
			(pin passive line
				(at 41.91 -26.67 180)
				(length 2.54)
				(name "P1.12_RX_D7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-nRF52840-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-nRF52840-SMD"
			(at -8.636 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-nRF52840-SMD_0_1")
		(symbol "XIAO-nRF52840-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "P0.02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "P0.03_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "P0.28_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "P0.29_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "P0.04_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "P0.05_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "P1.11_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -7.62 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "32")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "PA31_SWDIO")
				(number "24")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "PA30_SWCLK")
				(number "25")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RESET")
				(number "26")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "NFC1")
				(number "34")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 7.62 -21.59 90)
				(length 2.54)
				(name "NFC2")
				(number "35")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "P1.15_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "P1.14_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P1.13_D8_SCK")
				(number "9")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "P1.12_D7_RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO-nRF52840_Plus_SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 2.54 0)
		)
		(property "Value" ""
			(at 0 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-nRF52840_Plus_SMD_0_1")
		(symbol "XIAO-nRF52840_Plus_SMD_1_0"
			(pin passive line
				(at -2.54 -2.54 0)
				(length 2.54)
				(name "P0.02_AIN0_LOW_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -2.54 -6.35 0)
				(length 2.54)
				(name "P0.03_AIN1_LOW_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 0)
				(length 2.54)
				(name "P0.28_AIN4_LOW_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -2.54 -13.97 0)
				(length 2.54)
				(name "P0.29_AIN5_LOW_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -2.54 -17.78 0)
				(length 2.54)
				(name "P0.04_AIN2_A4_D4")
				(number "5")
			)
			(pin passive line
				(at -2.54 -21.59 0)
				(length 2.54)
				(name "P0.05_AIN3_A5_D5")
				(number "6")
			)
			(pin passive line
				(at -2.54 -25.4 0)
				(length 2.54)
				(name "P1.11_TX_D6")
				(number "7")
			)
			(pin passive line
				(at 45.72 -2.54 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at 45.72 -6.35 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 45.72 -10.16 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 45.72 -13.97 180)
				(length 2.54)
				(name "P1.15_MOSI_D10")
				(number "11")
			)
			(pin passive line
				(at 45.72 -17.78 180)
				(length 2.54)
				(name "P1.14_MISO_D9")
				(number "10")
			)
			(pin passive line
				(at 45.72 -21.59 180)
				(length 2.54)
				(name "P1.13_SCK_D8")
				(number "9")
			)
			(pin passive line
				(at 45.72 -25.4 180)
				(length 2.54)
				(name "P1.12_RX_D7")
				(number "8")
			)
		)
		(symbol "XIAO-nRF52840_Plus_SMD_1_1"
			(pin passive line
				(at -2.54 -30.48 0)
				(length 2.54)
				(name "P0.15_I2S_SD")
				(number "15")
			)
			(pin passive line
				(at -2.54 -33.02 0)
				(length 2.54)
				(name "P0.19_I2S_SCK")
				(number "16")
			)
			(pin passive line
				(at -2.54 -35.56 0)
				(length 2.54)
				(name "P1.01_I2S_WS")
				(number "17")
			)
			(pin passive line
				(at -2.54 -38.1 0)
				(length 2.54)
				(name "P0.09/NFC1/RX1")
				(number "18")
			)
			(pin passive line
				(at -2.54 -40.64 0)
				(length 2.54)
				(name "P0.10/NFC2/TX1")
				(number "19")
			)
			(pin passive line
				(at -2.54 -43.18 0)
				(length 2.54)
				(name "P0.31_AIN7_BAT")
				(number "20")
			)
			(pin passive line
				(at -2.54 -46.99 0)
				(length 2.54)
				(name "VBAT")
				(number "32")
			)
			(pin passive line
				(at -2.54 -49.53 0)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 45.72 -30.48 180)
				(length 2.54)
				(name "P1.03_SCK1")
				(number "21")
			)
			(pin passive line
				(at 45.72 -33.02 180)
				(length 2.54)
				(name "P1.05_MISO1")
				(number "22")
			)
			(pin passive line
				(at 45.72 -35.56 180)
				(length 2.54)
				(name "P1.07_MOSI1")
				(number "23")
			)
			(pin passive line
				(at 45.72 -41.91 180)
				(length 2.54)
				(name "SWDIO")
				(number "24")
			)
			(pin passive line
				(at 45.72 -44.45 180)
				(length 2.54)
				(name "SWDCLK")
				(number "25")
			)
			(pin passive line
				(at 45.72 -46.99 180)
				(length 2.54)
				(name "REST")
				(number "26")
			)
			(pin passive line
				(at 45.72 -49.53 180)
				(length 2.54)
				(name "GND")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XIAO_ESP32-C6-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.574 17.018 0)
		)
		(property "Value" "XIAO-ESP32-C6"
			(at -15.24 14.986 0)
		)
		(property "Footprint" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at -4.572 -18.542 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
		)
		(property "MPN" ""
			(at 0 0 0)
		)
		(property "SKU" "XIAO-DIP"
			(at -5.842 -2.286 0)
		)
		(property "Part Type" ""
			(at 0 0 0)
		)
		(property "Rating" ""
			(at 0 0 0)
		)
		(property "Status" ""
			(at 0 0 0)
		)
		(property "Temperature" ""
			(at 0 0 0)
		)
		(property "Priority" ""
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Module:MOUDLE14P-XIAO-DIP-SMD"
			(at 0 0 0)
		)
		(symbol "XIAO_ESP32-C6-DIP_1_0"
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "GPIO0/A0/D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "GPIO1/A1/D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "GPIO2/A2/D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "GPIO21/D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "GPIO22/D4/SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "GPIO23/D5/SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "GPIO16/D6/TX")
				(number "7")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "VBUS")
				(number "14")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO18/D10/MOSI")
				(number "11")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO20/D9/MISO")
				(number "10")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO19/D8/SCK")
				(number "9")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO17/D7/RX")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
)
