(kicad_symbol_lib
	(version 20231120)
	(generator "kicad_symbol_editor")
	(generator_version "8.0")
	(symbol "XIAO-ESP32-C3-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-C3-DIP"
			(at -9.144 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C3-DIP_0_1")
		(symbol "XIAO-ESP32-C3-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-C3-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-C3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C3-SMD_0_1")
		(symbol "XIAO-ESP32-C3-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -10.16 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "17")
			)
			(pin passive line
				(at -6.35 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "18")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at 1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "21")
			)
			(pin passive line
				(at 8.89 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "22")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-C6-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-C6-DIP"
			(at -9.144 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C6-DIP_0_1")
		(symbol "XIAO-ESP32-C6-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-C6-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-S3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-C6-SMD_0_1")
		(symbol "XIAO-ESP32-C6-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -12.7 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "17")
			)
			(pin passive line
				(at -8.89 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "21")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "22")
			)
			(pin passive line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "BOOT")
				(number "23")
			)
			(pin passive line
				(at 13.97 22.86 270)
				(length 2.54)
				(name "3V3_1")
				(number "24")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-S3-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-S3-DIP"
			(at -9.144 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3-DIP_0_1")
		(symbol "XIAO-ESP32-S3-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-S3-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-S3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3-SMD_0_1")
		(symbol "XIAO-ESP32-S3-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -12.7 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "17")
			)
			(pin passive line
				(at -8.89 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "21")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "22")
			)
			(pin passive line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "USB_DN")
				(number "23")
			)
			(pin passive line
				(at 13.97 22.86 270)
				(length 2.54)
				(name "USB_DP")
				(number "24")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-ESP32-S3-SMD_PAD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-ESP32-S3-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-ESP32-S3-SMD_PAD_0_1")
		(symbol "XIAO-ESP32-S3-SMD_PAD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -12.7 22.86 270)
				(length 2.54)
				(name "MTDI")
				(number "17")
			)
			(pin passive line
				(at -8.89 22.86 270)
				(length 2.54)
				(name "MTDO")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "CHIP_EN")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "MTMS")
				(number "21")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "MTCK")
				(number "22")
			)
			(pin passive line
				(at 10.16 22.86 270)
				(length 2.54)
				(name "USB_DN")
				(number "23")
			)
			(pin passive line
				(at 13.97 22.86 270)
				(length 2.54)
				(name "USB_DP")
				(number "24")
			)
			(pin passive line
				(at 7.62 -21.59 90)
				(length 2.54)
				(name "PAD")
				(number "25")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-R4-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.844 27.432 0)
		)
		(property "Value" "XIAO-R4-DIP"
			(at -21.59 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-R4-DIP_0_1")
		(symbol "XIAO-R4-DIP_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
		(symbol "XIAO-R4-DIP_1_1"
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "GPIO21/D11/RX1")
				(number "15")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIO20/D12/TX1")
				(number "16")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "GPIO17/D13/SCL0")
				(number "17")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO16/D14/SDA0")
				(number "18")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO11/D15/SPI1_MOSI")
				(number "19")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO12/D16/SPI1_MISO")
				(number "20")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO10/D17/SPI1_SCK")
				(number "21")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO9/D18/SPI1_CS")
				(number "22")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "BAT")
				(number "23")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_2")
				(number "24")
			)
		)
	)
	(symbol "XIAO-R4-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.844 27.432 0)
		)
		(property "Value" "XIAO-R4-SMD"
			(at -21.844 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-R4-SMD_0_1")
		(symbol "XIAO-R4-SMD_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
		(symbol "XIAO-R4-SMD_1_1"
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "GPIO21/D11/RX1")
				(number "15")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIO20/D12/TX1")
				(number "16")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "GPIO17/D13/SCL0")
				(number "17")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO16/D14/SDA0")
				(number "18")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO11/D15/SPI1_MOSI")
				(number "19")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO12/D16/SPI1_MISO")
				(number "20")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO10/D17/SPI1_SCK")
				(number "21")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO9/D18/SPI1_CS")
				(number "22")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RST")
				(number "24")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "BOOT")
				(number "25")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "3V3_1")
				(number "26")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_1")
				(number "27")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWDCLK")
				(number "28")
			)
			(pin passive line
				(at -2.54 -31.75 90)
				(length 2.54)
				(name "BAT")
				(number "29")
			)
			(pin passive line
				(at 2.54 -31.75 90)
				(length 2.54)
				(name "GND_2")
				(number "30")
			)
		)
	)
	(symbol "XIAO-RP2040-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-RP2040-DIP"
			(at -10.16 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RP2040-DIP_0_1")
		(symbol "XIAO-RP2040-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-RP2040-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-RP2040-SMD"
			(at -8.382 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-RP2040-SMD_0_1")
		(symbol "XIAO-RP2040-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 21.59 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 21.59 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 21.59 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 21.59 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 21.59 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -6.35 22.86 270)
				(length 2.54)
				(name "SWDIO")
				(number "17")
			)
			(pin passive line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "SWDCLK")
				(number "18")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RST")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 21.59 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 21.59 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-RP2350-DIP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.844 27.432 0)
		)
		(property "Value" "XIAO-RP2350-DIP"
			(at -21.844 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-RP2350-DIP_0_1")
		(symbol "XIAO-RP2350-DIP_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
		(symbol "XIAO-RP2350-DIP_1_1"
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "GPIO21/D11/RX1")
				(number "15")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIO20/D12/TX1")
				(number "16")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "GPIO17/D13/SCL0")
				(number "17")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO16/D14/SDA0")
				(number "18")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO11/D15/SPI1_MOSI")
				(number "19")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO12/D16/SPI1_MISO")
				(number "20")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO10/D17/SPI1_SCK")
				(number "21")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO9/D18/SPI1_CS")
				(number "22")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "BAT")
				(number "23")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_2")
				(number "24")
			)
		)
	)
	(symbol "XIAO-RP2350-SMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 27.432 0)
		)
		(property "Value" "XIAO-RP2350-SMD"
			(at -21.59 25.654 0)
		)
		(property "Footprint" ""
			(at 0 11.43 0)
		)
		(property "Datasheet" ""
			(at 0 11.43 0)
		)
		(property "Description" ""
			(at 0 11.43 0)
		)
		(symbol "XIAO-RP2350-SMD_0_1")
		(symbol "XIAO-RP2350-SMD_1_0"
			(pin passive line
				(at -24.13 22.86 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at -24.13 -11.43 0)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at -24.13 -15.24 0)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at -24.13 -19.05 0)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at -24.13 -22.86 0)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at -24.13 -26.67 0)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -24.13 19.05 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -24.13 15.24 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -24.13 11.43 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -24.13 7.62 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -24.13 3.81 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -24.13 0 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at -24.13 -3.81 0)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at -24.13 -7.62 0)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
		(symbol "XIAO-RP2350-SMD_1_1"
			(pin passive line
				(at 25.4 -26.67 180)
				(length 2.54)
				(name "GPIO21/D11/RX1")
				(number "15")
			)
			(pin passive line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIO20/D12/TX1")
				(number "16")
			)
			(pin passive line
				(at 25.4 -19.05 180)
				(length 2.54)
				(name "GPIO17/D13/SCL0")
				(number "17")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIO16/D14/SDA0")
				(number "18")
			)
			(pin passive line
				(at 25.4 -11.43 180)
				(length 2.54)
				(name "GPIO11/D15/SPI1_MOSI")
				(number "19")
			)
			(pin passive line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIO12/D16/SPI1_MISO")
				(number "20")
			)
			(pin passive line
				(at 25.4 -3.81 180)
				(length 2.54)
				(name "GPIO10/D17/SPI1_SCK")
				(number "21")
			)
			(pin passive line
				(at 25.4 0 180)
				(length 2.54)
				(name "GPIO9/D18/SPI1_CS")
				(number "22")
			)
			(pin passive line
				(at 25.4 3.81 180)
				(length 2.54)
				(name "SWDIO")
				(number "23")
			)
			(pin passive line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RST")
				(number "24")
			)
			(pin passive line
				(at 25.4 11.43 180)
				(length 2.54)
				(name "BOOT")
				(number "25")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "3V3_1")
				(number "26")
			)
			(pin passive line
				(at 25.4 19.05 180)
				(length 2.54)
				(name "GND_1")
				(number "27")
			)
			(pin passive line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SWDCLK")
				(number "28")
			)
			(pin passive line
				(at -2.54 -31.75 90)
				(length 2.54)
				(name "BAT")
				(number "29")
			)
			(pin passive line
				(at 2.54 -31.75 90)
				(length 2.54)
				(name "GND_2")
				(number "30")
			)
		)
	)
	(symbol "XIAO-SAMD21-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 22.86 0)
		)
		(property "Value" "XIAO-SAMD21-DIP"
			(at -10.16 21.082 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-SAMD21-DIP_0_1")
		(symbol "XIAO-SAMD21-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-SAMD21-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-SAMD21-SMD"
			(at -9.906 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-SAMD21-SMD_0_1")
		(symbol "XIAO-SAMD21-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "VIN")
				(number "15")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "PA31_SWDIO")
				(number "17")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "PA30_SWCLK")
				(number "18")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RESET")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-nRF52840-DIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-nRF52840-DIP"
			(at -9.144 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-nRF52840-DIP_0_1")
		(symbol "XIAO-nRF52840-DIP_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
	(symbol "XIAO-nRF52840-SMD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 23.114 0)
		)
		(property "Value" "XIAO-nRF52840-SMD"
			(at -8.636 21.336 0)
		)
		(property "Footprint" ""
			(at -8.89 5.08 0)
		)
		(property "Datasheet" ""
			(at -8.89 5.08 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "XIAO-nRF52840-SMD_0_1")
		(symbol "XIAO-nRF52840-SMD_1_1"
			(pin passive line
				(at -21.59 11.43 0)
				(length 2.54)
				(name "PA02_A0_D0")
				(number "1")
			)
			(pin passive line
				(at 20.32 -3.81 180)
				(length 2.54)
				(name "PA5_A9_D9_MISO")
				(number "10")
			)
			(pin passive line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6_A10_D10_MOSI")
				(number "11")
			)
			(pin passive line
				(at 20.32 3.81 180)
				(length 2.54)
				(name "3V3")
				(number "12")
			)
			(pin passive line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 20.32 11.43 180)
				(length 2.54)
				(name "5V")
				(number "14")
			)
			(pin passive line
				(at -7.62 -21.59 90)
				(length 2.54)
				(name "BAT")
				(number "15")
			)
			(pin passive line
				(at -2.54 -21.59 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 2.54 -21.59 90)
				(length 2.54)
				(name "NFC1")
				(number "17")
			)
			(pin passive line
				(at 7.62 -21.59 90)
				(length 2.54)
				(name "NFC2")
				(number "18")
			)
			(pin passive line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "PA31_SWDIO")
				(number "19")
			)
			(pin passive line
				(at -21.59 7.62 0)
				(length 2.54)
				(name "PA4_A1_D1")
				(number "2")
			)
			(pin passive line
				(at -1.27 22.86 270)
				(length 2.54)
				(name "PA30_SWCLK")
				(number "20")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "RESET")
				(number "21")
			)
			(pin passive line
				(at 6.35 22.86 270)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at -21.59 3.81 0)
				(length 2.54)
				(name "PA10_A2_D2")
				(number "3")
			)
			(pin passive line
				(at -21.59 0 0)
				(length 2.54)
				(name "PA11_A3_D3")
				(number "4")
			)
			(pin passive line
				(at -21.59 -3.81 0)
				(length 2.54)
				(name "PA8_A4_D4_SDA")
				(number "5")
			)
			(pin passive line
				(at -21.59 -7.62 0)
				(length 2.54)
				(name "PA9_A5_D5_SCL")
				(number "6")
			)
			(pin passive line
				(at -21.59 -11.43 0)
				(length 2.54)
				(name "PB08_A6_D6_TX")
				(number "7")
			)
			(pin passive line
				(at 20.32 -11.43 180)
				(length 2.54)
				(name "PB09_A7_D7_RX")
				(number "8")
			)
			(pin passive line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PA7_A8_D8_SCK")
				(number "9")
			)
		)
	)
)